Classes | Enumerations
Structures
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Management
Collaboration diagram for Structures:

## Classes
struct | ble_gap_adv_param_t
| Advertising parameters for legacy advertising. More...
struct | ble_gap_adv_prim_cfg_t
| Configuration for advertising on primary channel. More...
struct | ble_gap_adv_second_cfg_t
| Configuration for advertising on secondary channel. More...
struct | ble_gap_adv_period_cfg_t
| Configuration for periodic advertising. More...
struct | ble_gap_ext_adv_param_t
| Advertising parameters for extended advertising and periodic advertising. More...
struct | ble_gap_adv_time_param_t
| Advertising timing parameter. More...
struct | ble_gap_sec_key_t
| Security key. More...
struct | ble_gap_scan_param_t
| Parameters for legacy scanning. More...
struct | ble_gap_scan_wd_op_param_t
| Scan Window operation parameters. More...
struct | ble_gap_ext_scan_param_t
| Parameters for extended scanning. More...
struct | ble_gap_period_adv_addr_cfg_t
| Periodic advertising information. More...
struct | ble_gap_per_sync_param_t
| Periodic advertising synchronization parameters. More...
struct | ble_gap_init_param_t
| Legacy initiating parameters. More...
struct | ble_gap_ext_conn_param_t
| Connection parameters. More...
struct | ble_gap_ext_init_param_t
| Extended initiating parameters. More...
struct | ble_gap_lepsm_register_t
| LE Protocol/Service Multiplexer information. More...
struct | ble_gap_bond_dev_list_t
| Bonded device list. More...
struct | ble_gap_white_list_t
| White list. More...
struct | ble_gap_period_adv_list_t
| Periodic advertising list. More...
struct | ble_gap_ral_dev_info_t
| RPA list item info. More...
struct | ble_gap_ral_dev_list_t
| RPA list info. More...
struct | ble_gap_evt_adv_stop_t
| Advertising Stop info. More...
struct | ble_gap_evt_scan_req_t
| Scan request info. More...
struct | ble_gap_evt_scan_stop_t
| Scan Stop info struct. More...
struct | ble_gap_evt_adv_report_t
| Advertising report event for BLE_GAPM_EVT_ADV_REPORT. More...
struct | ble_gap_evt_sync_established_t
| Sync established event for BLE_GAPM_EVT_SYNC_ESTABLISH. More...
struct | ble_gap_evt_rslv_addr_read_t
| Read resolvable address event for BLE_GAPM_EVT_READ_RSLV_ADDR. More...
struct | ble_gap_evt_rslv_addr_report_t
| Resolvable address report event for BLE_GAPM_EVT_RSLV_ADDR_REPORT. More...
struct | ble_gapm_evt_t
| BLE GAPM event structure. More...

## Enumerations
enum | ble_gap_rslv_addr_read_op_id_t { BLE_GAP_OPCODE_LOCAL_RSLV_ADDR_READ, BLE_GAP_OPCODE_PEER_RSLV_ADDR_READ }
| Operation code used to read resolvable address. More...

## Detailed Description

## Enumeration Type Documentation

## ◆ ble_gap_rslv_addr_read_op_id_t

enum ble_gap_rslv_addr_read_op_id_t

Operation code used to read resolvable address.

Enumerator
BLE_GAP_OPCODE_LOCAL_RSLV_ADDR_READ | Local resolvable address operation.
BLE_GAP_OPCODE_PEER_RSLV_ADDR_READ | Peer resolvable address operation.

Definition at line 784 of file ble_gapm.h.