Here is a list of all file members with links to the files they belong to:

### - l -

- LCP_RX : ble_lcp.h
- LCP_TX : ble_lcp.h
- lfrc32k_calibration() : platform_sdk.h
- LL_ADC_CLK_1 : gr55xx_ll_adc.h
- LL_ADC_CLK_16 : gr55xx_ll_adc.h
- LL_ADC_CLK_1P6 : gr55xx_ll_adc.h
- LL_ADC_CLK_2 : gr55xx_ll_adc.h
- LL_ADC_CLK_4 : gr55xx_ll_adc.h
- LL_ADC_CLK_8 : gr55xx_ll_adc.h
- LL_ADC_DEFAULT_CONFIG : gr55xx_ll_adc.h
- ll_adc_deinit() : gr55xx_ll_adc.h
- ll_adc_disable() : gr55xx_ll_adc.h
- ll_adc_disable_clock() : gr55xx_ll_adc.h
- ll_adc_disable_mas_rst() : gr55xx_ll_adc.h
- ll_adc_disable_ofs_cal() : gr55xx_ll_adc.h
- ll_adc_disable_temp() : gr55xx_ll_adc.h
- ll_adc_disable_vbat() : gr55xx_ll_adc.h
- ll_adc_enable() : gr55xx_ll_adc.h
- ll_adc_enable_clock() : gr55xx_ll_adc.h
- ll_adc_enable_mas_rst() : gr55xx_ll_adc.h
- ll_adc_enable_ofs_cal() : gr55xx_ll_adc.h
- ll_adc_enable_temp() : gr55xx_ll_adc.h
- ll_adc_enable_vbat() : gr55xx_ll_adc.h
- ll_adc_get_channeln() : gr55xx_ll_adc.h
- ll_adc_get_channelp() : gr55xx_ll_adc.h
- ll_adc_get_clock() : gr55xx_ll_adc.h
- ll_adc_get_dynamic_rang() : gr55xx_ll_adc.h
- ll_adc_get_fifo_count() : gr55xx_ll_adc.h
- ll_adc_get_input_mode() : gr55xx_ll_adc.h
- ll_adc_get_ref() : gr55xx_ll_adc.h
- ll_adc_get_ref_current() : gr55xx_ll_adc.h
- ll_adc_get_ref_value() : gr55xx_ll_adc.h
- ll_adc_get_thresh() : gr55xx_ll_adc.h
- ll_adc_init() : gr55xx_ll_adc.h
- ll_adc_init_t : gr55xx_ll_adc.h
- LL_ADC_INPUT_DIFFERENTIAL : gr55xx_ll_adc.h
- LL_ADC_INPUT_SINGLE : gr55xx_ll_adc.h
- LL_ADC_INPUT_SRC_BAT : gr55xx_ll_adc.h
- LL_ADC_INPUT_SRC_IO0 : gr55xx_ll_adc.h
- LL_ADC_INPUT_SRC_IO1 : gr55xx_ll_adc.h
- LL_ADC_INPUT_SRC_IO2 : gr55xx_ll_adc.h
- LL_ADC_INPUT_SRC_IO3 : gr55xx_ll_adc.h
- LL_ADC_INPUT_SRC_IO4 : gr55xx_ll_adc.h
- LL_ADC_INPUT_SRC_REF : gr55xx_ll_adc.h
- LL_ADC_INPUT_SRC_TMP : gr55xx_ll_adc.h
- ll_adc_is_enabled() : gr55xx_ll_adc.h
- ll_adc_is_enabled_clock() : gr55xx_ll_adc.h
- ll_adc_is_enabled_mas_rst() : gr55xx_ll_adc.h
- ll_adc_is_enabled_ofs_cal() : gr55xx_ll_adc.h
- ll_adc_is_enabled_temp() : gr55xx_ll_adc.h
- ll_adc_is_enabled_vbat() : gr55xx_ll_adc.h
- ll_adc_is_fifo_notempty() : gr55xx_ll_adc.h
- ll_adc_read_fifo() : gr55xx_ll_adc.h
- LL_ADC_ReadReg : gr55xx_ll_adc.h
- LL_ADC_REF_SRC_BUF_INT : gr55xx_ll_adc.h
- LL_ADC_REF_SRC_IO0 : gr55xx_ll_adc.h
- LL_ADC_REF_SRC_IO1 : gr55xx_ll_adc.h
- LL_ADC_REF_SRC_IO2 : gr55xx_ll_adc.h
- LL_ADC_REF_SRC_IO3 : gr55xx_ll_adc.h
- LL_ADC_REF_VALUE_0P8 : gr55xx_ll_adc.h
- LL_ADC_REF_VALUE_1P2 : gr55xx_ll_adc.h
- LL_ADC_REF_VALUE_1P6 : gr55xx_ll_adc.h
- ll_adc_set_channeln() : gr55xx_ll_adc.h
- ll_adc_set_channelp() : gr55xx_ll_adc.h
- ll_adc_set_clock() : gr55xx_ll_adc.h
- ll_adc_set_dynamic_rang() : gr55xx_ll_adc.h
- ll_adc_set_input_mode() : gr55xx_ll_adc.h
- ll_adc_set_ref() : gr55xx_ll_adc.h
- ll_adc_set_ref_current() : gr55xx_ll_adc.h
- ll_adc_set_ref_value() : gr55xx_ll_adc.h
- ll_adc_set_thresh() : gr55xx_ll_adc.h
- ll_adc_struct_init() : gr55xx_ll_adc.h
- LL_ADC_WriteReg : gr55xx_ll_adc.h
- ll_aes_clear_flag_it_done() : gr55xx_ll_aes.h
- ll_aes_deinit() : gr55xx_ll_aes.h
- ll_aes_disable() : gr55xx_ll_aes.h
- ll_aes_disable_dma_start() : gr55xx_ll_aes.h
- ll_aes_disable_encryption() : gr55xx_ll_aes.h
- ll_aes_disable_full_mask() : gr55xx_ll_aes.h
- ll_aes_disable_it_done() : gr55xx_ll_aes.h
- ll_aes_disable_little_endian() : gr55xx_ll_aes.h
- ll_aes_disable_start() : gr55xx_ll_aes.h
- LL_AES_DMA_TRANSIZE_MAX : gr55xx_ll_aes.h
- LL_AES_DMA_TRANSIZE_MIN : gr55xx_ll_aes.h
- ll_aes_enable() : gr55xx_ll_aes.h
- ll_aes_enable_dma_start() : gr55xx_ll_aes.h
- ll_aes_enable_encryption() : gr55xx_ll_aes.h
- ll_aes_enable_full_mask() : gr55xx_ll_aes.h
- ll_aes_enable_it_done() : gr55xx_ll_aes.h
- ll_aes_enable_little_endian() : gr55xx_ll_aes.h
- ll_aes_enable_read_key() : gr55xx_ll_aes.h
- ll_aes_enable_start() : gr55xx_ll_aes.h
- LL_AES_FLAG_DATAREADY : gr55xx_ll_aes.h
- LL_AES_FLAG_DMA_DONE : gr55xx_ll_aes.h
- LL_AES_FLAG_DMA_ERR : gr55xx_ll_aes.h
- LL_AES_FLAG_KEY_VALID : gr55xx_ll_aes.h
- ll_aes_get_data_127_96() : gr55xx_ll_aes.h
- ll_aes_get_data_31_0() : gr55xx_ll_aes.h
- ll_aes_get_data_63_32() : gr55xx_ll_aes.h
- ll_aes_get_data_95_64() : gr55xx_ll_aes.h
- ll_aes_get_dma_read_address() : gr55xx_ll_aes.h
- ll_aes_get_dma_transfer_block() : gr55xx_ll_aes.h
- ll_aes_get_dma_write_address() : gr55xx_ll_aes.h
- ll_aes_get_key_address() : gr55xx_ll_aes.h
- ll_aes_get_key_size() : gr55xx_ll_aes.h
- ll_aes_get_key_type() : gr55xx_ll_aes.h
- ll_aes_get_operation_mode() : gr55xx_ll_aes.h
- ll_aes_get_seed_Imask() : gr55xx_ll_aes.h
- ll_aes_get_seed_in() : gr55xx_ll_aes.h
- ll_aes_get_seed_Osbox() : gr55xx_ll_aes.h
- ll_aes_get_seed_out() : gr55xx_ll_aes.h
- ll_aes_init() : gr55xx_ll_aes.h
- ll_aes_init_t : gr55xx_ll_aes.h
- ll_aes_is_action_flag_dma_done() : gr55xx_ll_aes.h
- ll_aes_is_action_flag_dma_error() : gr55xx_ll_aes.h
- ll_aes_is_action_flag_it_done() : gr55xx_ll_aes.h
- ll_aes_is_action_flag_key_valid() : gr55xx_ll_aes.h
- ll_aes_is_action_flag_ready() : gr55xx_ll_aes.h
- ll_aes_is_enabled() : gr55xx_ll_aes.h
- ll_aes_is_enabled_dma_start() : gr55xx_ll_aes.h
- ll_aes_is_enabled_encryption() : gr55xx_ll_aes.h
- ll_aes_is_enabled_full_mask() : gr55xx_ll_aes.h
- ll_aes_is_enabled_it_done() : gr55xx_ll_aes.h
- ll_aes_is_enabled_little_endian() : gr55xx_ll_aes.h
- ll_aes_is_enabled_start() : gr55xx_ll_aes.h
- LL_AES_KEY_SIZE_128 : gr55xx_ll_aes.h
- LL_AES_KEY_SIZE_192 : gr55xx_ll_aes.h
- LL_AES_KEY_SIZE_256 : gr55xx_ll_aes.h
- LL_AES_KEYTYPE_AHB : gr55xx_ll_aes.h
- LL_AES_KEYTYPE_KRAM : gr55xx_ll_aes.h
- LL_AES_KEYTYPE_MCU : gr55xx_ll_aes.h
- LL_AES_OPERATION_MODE_CBC : gr55xx_ll_aes.h
- LL_AES_OPERATION_MODE_ECB : gr55xx_ll_aes.h
- LL_AES_ReadReg : gr55xx_ll_aes.h
- ll_aes_set_data_127_96() : gr55xx_ll_aes.h
- ll_aes_set_data_31_0() : gr55xx_ll_aes.h
- ll_aes_set_data_63_32() : gr55xx_ll_aes.h
- ll_aes_set_data_95_64() : gr55xx_ll_aes.h
- ll_aes_set_dma_read_address() : gr55xx_ll_aes.h
- ll_aes_set_dma_transfer_block() : gr55xx_ll_aes.h
- ll_aes_set_dma_write_address() : gr55xx_ll_aes.h
- ll_aes_set_first_block() : gr55xx_ll_aes.h
- ll_aes_set_key_127_96() : gr55xx_ll_aes.h
- ll_aes_set_key_159_128() : gr55xx_ll_aes.h
- ll_aes_set_key_191_160() : gr55xx_ll_aes.h
- ll_aes_set_key_223_192() : gr55xx_ll_aes.h
- ll_aes_set_key_255_224() : gr55xx_ll_aes.h
- ll_aes_set_key_31_0() : gr55xx_ll_aes.h
- ll_aes_set_key_63_32() : gr55xx_ll_aes.h
- ll_aes_set_key_95_64() : gr55xx_ll_aes.h
- ll_aes_set_key_address() : gr55xx_ll_aes.h
- ll_aes_set_key_port_mask() : gr55xx_ll_aes.h
- ll_aes_set_key_size() : gr55xx_ll_aes.h
- ll_aes_set_key_type() : gr55xx_ll_aes.h
- ll_aes_set_load_seed() : gr55xx_ll_aes.h
- ll_aes_set_operation_mode() : gr55xx_ll_aes.h
- ll_aes_set_seed_Imask() : gr55xx_ll_aes.h
- ll_aes_set_seed_in() : gr55xx_ll_aes.h
- ll_aes_set_seed_Osbox() : gr55xx_ll_aes.h
- ll_aes_set_seed_out() : gr55xx_ll_aes.h
- ll_aes_set_vector_127_96() : gr55xx_ll_aes.h
- ll_aes_set_vector_31_0() : gr55xx_ll_aes.h
- ll_aes_set_vector_63_32() : gr55xx_ll_aes.h
- ll_aes_set_vector_95_64() : gr55xx_ll_aes.h
- ll_aes_struct_init() : gr55xx_ll_aes.h
- LL_AES_WriteReg : gr55xx_ll_aes.h
- ll_aon_gpio_clear_flag_it() : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_DEFAULT_CONFIG : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_deinit() : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_disable_it() : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_disable_xo_2mhz_output() : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_enable_falling_trigger() : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_enable_high_trigger() : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_enable_it() : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_enable_low_trigger() : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_enable_rising_trigger() : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_enable_xo_2mhz_output() : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_get_mux_pin_0_7() : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_get_pin_mode() : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_get_pin_pull() : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_init() : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_init_t : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_is_active_flag_it() : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_is_enabled_falling_trigger() : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_is_enabled_high_trigger() : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_is_enabled_it() : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_is_enabled_low_trigger() : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_is_enabled_rising_trigger() : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_is_enabled_xo_2mhz_output() : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_is_input_pin_set() : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_is_output_pin_set() : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_MODE_INPUT : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_MODE_MUX : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_MODE_OUTPUT : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_MUX_0 : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_MUX_1 : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_MUX_2 : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_MUX_3 : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_MUX_4 : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_MUX_5 : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_MUX_6 : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_MUX_7 : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_MUX_8 : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_PIN_0 : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_PIN_1 : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_PIN_2 : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_PIN_3 : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_PIN_4 : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_PIN_5 : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_PIN_6 : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_PIN_7 : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_PIN_ALL : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_PULL_DOWN : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_PULL_NO : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_PULL_UP : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_RE_N : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_RE_N_Msk : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_RE_N_Pos : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_read_flag_it() : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_read_input_port() : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_read_output_port() : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_ReadReg : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_reset_output_pin() : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_RTYP : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_RTYP_Msk : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_RTYP_Pos : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_set_mux_pin_0_7() : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_set_output_pin() : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_set_pin_mode() : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_set_pin_pull() : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_struct_init() : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_toggle_pin() : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_TRIGGER_FALLING : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_TRIGGER_HIGH : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_TRIGGER_LOW : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_TRIGGER_NONE : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_TRIGGER_RISING : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_write_output_port() : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_WriteReg : gr55xx_ll_aon_gpio.h
- ll_aon_wdt_clear_flag_reboot() : gr55xx_ll_aon_wdt.h
- ll_aon_wdt_disable() : gr55xx_ll_aon_wdt.h
- ll_aon_wdt_enable() : gr55xx_ll_aon_wdt.h
- ll_aon_wdt_get_alarm_counter() : gr55xx_ll_aon_wdt.h
- ll_aon_wdt_get_counter() : gr55xx_ll_aon_wdt.h
- ll_aon_wdt_is_active_flag_reboot() : gr55xx_ll_aon_wdt.h
- ll_aon_wdt_is_active_flag_running() : gr55xx_ll_aon_wdt.h
- ll_aon_wdt_is_enabled() : gr55xx_ll_aon_wdt.h
- ll_aon_wdt_reload_counter() : gr55xx_ll_aon_wdt.h
- ll_aon_wdt_set_alarm_counter() : gr55xx_ll_aon_wdt.h
- ll_aon_wdt_set_reload_counter() : gr55xx_ll_aon_wdt.h
- LL_BOD2_DISABLE : gr55xx_ll_bod.h
- ll_bod2_disable() : gr55xx_ll_bod.h
- ll_bod2_enable() : gr55xx_ll_bod.h
- LL_BOD2_ENABLE : gr55xx_ll_bod.h
- LL_BOD2_LEVEL_0 : gr55xx_ll_bod.h
- LL_BOD2_LEVEL_1 : gr55xx_ll_bod.h
- LL_BOD2_LEVEL_2 : gr55xx_ll_bod.h
- LL_BOD2_LEVEL_3 : gr55xx_ll_bod.h
- LL_BOD2_LEVEL_4 : gr55xx_ll_bod.h
- LL_BOD2_LEVEL_5 : gr55xx_ll_bod.h
- LL_BOD2_LEVEL_6 : gr55xx_ll_bod.h
- LL_BOD2_LEVEL_7 : gr55xx_ll_bod.h
- ll_bod2_lvl_ctrl_lv_set() : gr55xx_ll_bod.h
- ll_bod_clear_flag_fedge() : gr55xx_ll_bod.h
- ll_bod_deinit() : gr55xx_ll_bod.h
- ll_bod_disable() : gr55xx_ll_bod.h
- LL_BOD_DISABLE : gr55xx_ll_bod.h
- ll_bod_disable_fedge() : gr55xx_ll_bod.h
- ll_bod_enable() : gr55xx_ll_bod.h
- LL_BOD_ENABLE : gr55xx_ll_bod.h
- ll_bod_enable_fedge() : gr55xx_ll_bod.h
- ll_bod_init() : gr55xx_ll_bod.h
- ll_bod_init_t : gr55xx_ll_bod.h
- ll_bod_is_active_flag_fedge() : gr55xx_ll_bod.h
- LL_BOD_STATIC_DISABLE : gr55xx_ll_bod.h
- LL_BOD_STATIC_ENABLE : gr55xx_ll_bod.h
- ll_bod_static_lv_disable() : gr55xx_ll_bod.h
- ll_bod_static_lv_enable() : gr55xx_ll_bod.h
- ll_bod_struct_init() : gr55xx_ll_bod.h
- ll_calendar_clear_flag_alarm() : gr55xx_ll_calendar.h
- ll_calendar_clear_flag_wrap() : gr55xx_ll_calendar.h
- ll_calendar_disable() : gr55xx_ll_calendar.h
- LL_CALENDAR_DIV_128 : gr55xx_ll_calendar.h
- LL_CALENDAR_DIV_256 : gr55xx_ll_calendar.h
- LL_CALENDAR_DIV_32 : gr55xx_ll_calendar.h
- LL_CALENDAR_DIV_64 : gr55xx_ll_calendar.h
- LL_CALENDAR_DIV_NONE : gr55xx_ll_calendar.h
- ll_calendar_enable() : gr55xx_ll_calendar.h
- ll_calendar_get_alarm() : gr55xx_ll_calendar.h
- ll_calendar_get_counter() : gr55xx_ll_calendar.h
- ll_calendar_get_wrapcnt() : gr55xx_ll_calendar.h
- ll_calendar_is_active_flag_alarm() : gr55xx_ll_calendar.h
- ll_calendar_is_active_flag_wrap() : gr55xx_ll_calendar.h
- ll_calendar_is_enabled() : gr55xx_ll_calendar.h
- ll_calendar_it_disable_alarm() : gr55xx_ll_calendar.h
- ll_calendar_it_disable_wrap() : gr55xx_ll_calendar.h
- ll_calendar_it_enable_alarm() : gr55xx_ll_calendar.h
- ll_calendar_it_enable_wrap() : gr55xx_ll_calendar.h
- ll_calendar_it_is_enabled_alarm() : gr55xx_ll_calendar.h
- ll_calendar_it_is_enabled_wrap() : gr55xx_ll_calendar.h
- LL_CALENDAR_NO_CLOCK : gr55xx_ll_calendar.h
- ll_calendar_reload_alarm() : gr55xx_ll_calendar.h
- ll_calendar_reload_counter() : gr55xx_ll_calendar.h
- ll_calendar_set_clock_div() : gr55xx_ll_calendar.h
- LL_CGC_DEFAULT_CONFIG : gr55xx_ll_cgc.h
- ll_cgc_deinit() : gr55xx_ll_cgc.h
- ll_cgc_disable_force_off_aon_mcusub_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_force_off_apb_sub_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_force_off_ble_brg_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_force_off_dma_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_force_off_gpio_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_force_off_htb_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_force_off_i2c0_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_force_off_i2c1_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_force_off_i2s_m_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_force_off_i2s_s_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_force_off_pwm_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_force_off_qspi0_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_force_off_qspi1_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_force_off_rom_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_force_off_secu_div4_pclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_force_off_secu_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_force_off_serial_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_force_off_sim_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_force_off_snsadc_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_force_off_spim_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_force_off_spis_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_force_off_sram_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_force_off_uart0_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_force_off_uart1_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_force_off_xqspi_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_wfi_off_aon_mcusub_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_wfi_off_apb_sub_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_wfi_off_ble_brg_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_wfi_off_dma_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_wfi_off_gpio_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_wfi_off_htb_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_wfi_off_i2s_s_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_wfi_off_pwm_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_wfi_off_rom_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_wfi_off_secu_div4_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_wfi_off_secu_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_wfi_off_serial_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_wfi_off_sim_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_wfi_off_snsadc_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_wfi_off_sram_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_wfi_off_xqspi_div4_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_wfi_off_xqspi_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_force_off_aon_mcusub_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_force_off_apb_sub_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_force_off_ble_brg_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_force_off_dma_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_force_off_gpio_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_force_off_htb_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_force_off_i2c0_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_force_off_i2c1_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_force_off_i2s_m_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_force_off_i2s_s_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_force_off_pwm_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_force_off_qspi0_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_force_off_qspi1_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_force_off_rom_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_force_off_secu_div4_pclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_force_off_secu_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_force_off_serial_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_force_off_sim_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_force_off_snsadc_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_force_off_spim_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_force_off_spis_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_force_off_sram_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_force_off_uart0_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_force_off_uart1_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_force_off_xqspi_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_wfi_off_aon_mcusub_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_wfi_off_apb_sub_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_wfi_off_ble_brg_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_wfi_off_dma_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_wfi_off_gpio_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_wfi_off_htb_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_wfi_off_i2s_s_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_wfi_off_pwm_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_wfi_off_rom_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_wfi_off_secu_div4_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_wfi_off_secu_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_wfi_off_serial_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_wfi_off_sim_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_wfi_off_snsadc_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_wfi_off_sram_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_wfi_off_xqspi_div4_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_wfi_off_xqspi_hclk() : gr55xx_ll_cgc.h
- LL_CGC_FRC_ALL_HCLK0 : gr55xx_ll_cgc.h
- LL_CGC_FRC_ALL_HCLK1 : gr55xx_ll_cgc.h
- LL_CGC_FRC_ALL_HCLK2 : gr55xx_ll_cgc.h
- LL_CGC_FRC_AON_MCUSUB_HCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_APB_SUB_HCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_BLE_BRG_HCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_DMA_HCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_GPIO_HCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_HTB_HCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_I2C0_HCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_I2C1_HCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_I2S_HCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_I2S_S_HCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_PWM_HCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_QSPI0_HCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_QSPI1_HCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_ROM_HCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_SECU_DIV4_PCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_SECU_HCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_SERIAL_HCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_SERIALS_HCLK2 : gr55xx_ll_cgc.h
- LL_CGC_FRC_SIM_HCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_SNSADC_HCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_SPIM_HCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_SPIS_HCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_SRAM_HCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_UART0_HCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_UART1_HCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_XF_XQSPI_HCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_XQSPI_DIV4_PCLK : gr55xx_ll_cgc.h
- ll_cgc_get_force_off_hclk_0() : gr55xx_ll_cgc.h
- ll_cgc_get_force_off_hclk_1() : gr55xx_ll_cgc.h
- ll_cgc_get_force_off_hclk_2() : gr55xx_ll_cgc.h
- ll_cgc_get_wfi_off_hclk_0() : gr55xx_ll_cgc.h
- ll_cgc_get_wfi_off_hclk_1() : gr55xx_ll_cgc.h
- ll_cgc_get_wfi_off_hclk_2() : gr55xx_ll_cgc.h
- ll_cgc_init() : gr55xx_ll_cgc.h
- ll_cgc_init_t : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_force_off_aon_mcusub_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_force_off_apb_sub_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_force_off_ble_brg_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_force_off_dma_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_force_off_gpio_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_force_off_htb_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_force_off_i2c0_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_force_off_i2c1_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_force_off_i2s_m_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_force_off_i2s_s_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_force_off_pwm_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_force_off_qspi0_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_force_off_qspi1_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_force_off_rom_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_force_off_secu_div4_pclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_force_off_secu_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_force_off_serial_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_force_off_sim_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_force_off_snsadc_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_force_off_spim_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_force_off_spis_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_force_off_sram_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_force_off_uart0_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_force_off_uart1_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_force_off_xqspi_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_wfi_off_aon_mcusub_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_wfi_off_apb_sub_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_wfi_off_ble_brg_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_wfi_off_dma_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_wfi_off_gpio_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_wfi_off_htb_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_wfi_off_i2s_s_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_wfi_off_pwm_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_wfi_off_rom_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_wfi_off_secu_div4_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_wfi_off_secu_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_wfi_off_serial_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_wfi_off_sim_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_wfi_off_snsadc_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_wfi_off_sram_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_wfi_off_xqspi_div4_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_wfi_off_xqspi_hclk() : gr55xx_ll_cgc.h
- LL_CGC_ReadReg : gr55xx_ll_cgc.h
- ll_cgc_set_force_off_hclk_0() : gr55xx_ll_cgc.h
- ll_cgc_set_force_off_hclk_1() : gr55xx_ll_cgc.h
- ll_cgc_set_force_off_hclk_2() : gr55xx_ll_cgc.h
- ll_cgc_set_wfi_off_hclk_0() : gr55xx_ll_cgc.h
- ll_cgc_set_wfi_off_hclk_1() : gr55xx_ll_cgc.h
- ll_cgc_set_wfi_off_hclk_2() : gr55xx_ll_cgc.h
- ll_cgc_struct_init() : gr55xx_ll_cgc.h
- LL_CGC_WFI_ALL_HCLK0 : gr55xx_ll_cgc.h
- LL_CGC_WFI_ALL_HCLK1 : gr55xx_ll_cgc.h
- LL_CGC_WFI_ALL_HCLK2 : gr55xx_ll_cgc.h
- LL_CGC_WFI_AON_MCUSUB_HCLK : gr55xx_ll_cgc.h
- LL_CGC_WFI_APB_SUB_HCLK : gr55xx_ll_cgc.h
- LL_CGC_WFI_BLE_BRG_HCLK : gr55xx_ll_cgc.h
- LL_CGC_WFI_DMA_HCLK : gr55xx_ll_cgc.h
- LL_CGC_WFI_GPIO_HCLK : gr55xx_ll_cgc.h
- LL_CGC_WFI_HTB_HCLK : gr55xx_ll_cgc.h
- LL_CGC_WFI_I2S_S_HCLK : gr55xx_ll_cgc.h
- LL_CGC_WFI_PWM_HCLK : gr55xx_ll_cgc.h
- LL_CGC_WFI_ROM_HCLK : gr55xx_ll_cgc.h
- LL_CGC_WFI_SECU_DIV4_PCLK : gr55xx_ll_cgc.h
- LL_CGC_WFI_SECU_HCLK : gr55xx_ll_cgc.h
- LL_CGC_WFI_SERIAL_HCLK : gr55xx_ll_cgc.h
- LL_CGC_WFI_SIM_HCLK : gr55xx_ll_cgc.h
- LL_CGC_WFI_SNSADC_HCLK : gr55xx_ll_cgc.h
- LL_CGC_WFI_SRAM_HCLK : gr55xx_ll_cgc.h
- LL_CGC_WFI_XF_XQSPI_HCLK : gr55xx_ll_cgc.h
- LL_CGC_WFI_XQSPI_DIV4_PCLK : gr55xx_ll_cgc.h
- LL_CGC_WriteReg : gr55xx_ll_cgc.h
- ll_comp_clear_flag_it() : gr55xx_ll_comp.h
- LL_COMP_DEFAULT_CONFIG : gr55xx_ll_comp.h
- ll_comp_deinit() : gr55xx_ll_comp.h
- ll_comp_disable() : gr55xx_ll_comp.h
- ll_comp_enable() : gr55xx_ll_comp.h
- ll_comp_init() : gr55xx_ll_comp.h
- ll_comp_init_t : gr55xx_ll_comp.h
- LL_COMP_INPUT_SRC_IO0 : gr55xx_ll_comp.h
- LL_COMP_INPUT_SRC_IO1 : gr55xx_ll_comp.h
- LL_COMP_INPUT_SRC_IO2 : gr55xx_ll_comp.h
- LL_COMP_INPUT_SRC_IO3 : gr55xx_ll_comp.h
- LL_COMP_INPUT_SRC_IO4 : gr55xx_ll_comp.h
- ll_comp_is_active_flag_it() : gr55xx_ll_comp.h
- LL_COMP_ReadReg : gr55xx_ll_comp.h
- LL_COMP_REF_SRC_IO0 : gr55xx_ll_comp.h
- LL_COMP_REF_SRC_IO1 : gr55xx_ll_comp.h
- LL_COMP_REF_SRC_IO2 : gr55xx_ll_comp.h
- LL_COMP_REF_SRC_IO3 : gr55xx_ll_comp.h
- LL_COMP_REF_SRC_IO4 : gr55xx_ll_comp.h
- LL_COMP_REF_SRC_VBAT : gr55xx_ll_comp.h
- LL_COMP_REF_SRC_VREF : gr55xx_ll_comp.h
- ll_comp_set_input_src() : gr55xx_ll_comp.h
- ll_comp_set_ref_src() : gr55xx_ll_comp.h
- ll_comp_set_vbatt_lvl() : gr55xx_ll_comp.h
- ll_comp_set_vref_lvl() : gr55xx_ll_comp.h
- ll_comp_struct_init() : gr55xx_ll_comp.h
- LL_COMP_WriteReg : gr55xx_ll_comp.h
- LL_DMA_CHANNEL_0 : gr55xx_ll_dma.h
- LL_DMA_CHANNEL_1 : gr55xx_ll_dma.h
- LL_DMA_CHANNEL_2 : gr55xx_ll_dma.h
- LL_DMA_CHANNEL_3 : gr55xx_ll_dma.h
- LL_DMA_CHANNEL_4 : gr55xx_ll_dma.h
- LL_DMA_CHANNEL_5 : gr55xx_ll_dma.h
- LL_DMA_CHANNEL_6 : gr55xx_ll_dma.h
- LL_DMA_CHANNEL_7 : gr55xx_ll_dma.h
- LL_DMA_CHANNEL_ALL : gr55xx_ll_dma.h
- ll_dma_clear_flag_blk() : gr55xx_ll_dma.h
- ll_dma_clear_flag_blk0() : gr55xx_ll_dma.h
- ll_dma_clear_flag_blk1() : gr55xx_ll_dma.h
- ll_dma_clear_flag_blk2() : gr55xx_ll_dma.h
- ll_dma_clear_flag_blk3() : gr55xx_ll_dma.h
- ll_dma_clear_flag_blk4() : gr55xx_ll_dma.h
- ll_dma_clear_flag_blk5() : gr55xx_ll_dma.h
- ll_dma_clear_flag_blk6() : gr55xx_ll_dma.h
- ll_dma_clear_flag_blk7() : gr55xx_ll_dma.h
- ll_dma_clear_flag_dstt() : gr55xx_ll_dma.h
- ll_dma_clear_flag_dstt0() : gr55xx_ll_dma.h
- ll_dma_clear_flag_dstt1() : gr55xx_ll_dma.h
- ll_dma_clear_flag_dstt2() : gr55xx_ll_dma.h
- ll_dma_clear_flag_dstt3() : gr55xx_ll_dma.h
- ll_dma_clear_flag_dstt4() : gr55xx_ll_dma.h
- ll_dma_clear_flag_dstt5() : gr55xx_ll_dma.h
- ll_dma_clear_flag_dstt6() : gr55xx_ll_dma.h
- ll_dma_clear_flag_dstt7() : gr55xx_ll_dma.h
- ll_dma_clear_flag_err() : gr55xx_ll_dma.h
- ll_dma_clear_flag_err0() : gr55xx_ll_dma.h
- ll_dma_clear_flag_err1() : gr55xx_ll_dma.h
- ll_dma_clear_flag_err2() : gr55xx_ll_dma.h
- ll_dma_clear_flag_err3() : gr55xx_ll_dma.h
- ll_dma_clear_flag_err4() : gr55xx_ll_dma.h
- ll_dma_clear_flag_err5() : gr55xx_ll_dma.h
- ll_dma_clear_flag_err6() : gr55xx_ll_dma.h
- ll_dma_clear_flag_err7() : gr55xx_ll_dma.h
- ll_dma_clear_flag_srct() : gr55xx_ll_dma.h
- ll_dma_clear_flag_srct0() : gr55xx_ll_dma.h
- ll_dma_clear_flag_srct1() : gr55xx_ll_dma.h
- ll_dma_clear_flag_srct2() : gr55xx_ll_dma.h
- ll_dma_clear_flag_srct3() : gr55xx_ll_dma.h
- ll_dma_clear_flag_srct4() : gr55xx_ll_dma.h
- ll_dma_clear_flag_srct5() : gr55xx_ll_dma.h
- ll_dma_clear_flag_srct6() : gr55xx_ll_dma.h
- ll_dma_clear_flag_srct7() : gr55xx_ll_dma.h
- ll_dma_clear_flag_tfr() : gr55xx_ll_dma.h
- ll_dma_clear_flag_tfr0() : gr55xx_ll_dma.h
- ll_dma_clear_flag_tfr1() : gr55xx_ll_dma.h
- ll_dma_clear_flag_tfr2() : gr55xx_ll_dma.h
- ll_dma_clear_flag_tfr3() : gr55xx_ll_dma.h
- ll_dma_clear_flag_tfr4() : gr55xx_ll_dma.h
- ll_dma_clear_flag_tfr5() : gr55xx_ll_dma.h
- ll_dma_clear_flag_tfr6() : gr55xx_ll_dma.h
- ll_dma_clear_flag_tfr7() : gr55xx_ll_dma.h
- ll_dma_config_address() : gr55xx_ll_dma.h
- ll_dma_config_transfer() : gr55xx_ll_dma.h
- LL_DMA_DDATAALIGN_BYTE : gr55xx_ll_dma.h
- LL_DMA_DDATAALIGN_HALFWORD : gr55xx_ll_dma.h
- LL_DMA_DDATAALIGN_WORD : gr55xx_ll_dma.h
- ll_dma_deinit() : gr55xx_ll_dma.h
- LL_DMA_DHANDSHAKING_HW : gr55xx_ll_dma.h
- LL_DMA_DHANDSHAKING_SW : gr55xx_ll_dma.h
- LL_DMA_DIRECTION_MEMORY_TO_MEMORY : gr55xx_ll_dma.h
- LL_DMA_DIRECTION_MEMORY_TO_PERIPH : gr55xx_ll_dma.h
- LL_DMA_DIRECTION_PERIPH_TO_MEMORY : gr55xx_ll_dma.h
- LL_DMA_DIRECTION_PERIPH_TO_PERIPH : gr55xx_ll_dma.h
- ll_dma_disable() : gr55xx_ll_dma.h
- ll_dma_disable_channel() : gr55xx_ll_dma.h
- ll_dma_disable_it() : gr55xx_ll_dma.h
- ll_dma_disable_it_blk() : gr55xx_ll_dma.h
- ll_dma_disable_it_dstt() : gr55xx_ll_dma.h
- ll_dma_disable_it_err() : gr55xx_ll_dma.h
- ll_dma_disable_it_srct() : gr55xx_ll_dma.h
- ll_dma_disable_it_tfr() : gr55xx_ll_dma.h
- LL_DMA_DST_BURST_LENGTH_1 : gr55xx_ll_dma.h
- LL_DMA_DST_BURST_LENGTH_16 : gr55xx_ll_dma.h
- LL_DMA_DST_BURST_LENGTH_32 : gr55xx_ll_dma.h
- LL_DMA_DST_BURST_LENGTH_4 : gr55xx_ll_dma.h
- LL_DMA_DST_BURST_LENGTH_64 : gr55xx_ll_dma.h
- LL_DMA_DST_BURST_LENGTH_8 : gr55xx_ll_dma.h
- LL_DMA_DST_DECREMENT : gr55xx_ll_dma.h
- LL_DMA_DST_INCREMENT : gr55xx_ll_dma.h
- LL_DMA_DST_NO_CHANGE : gr55xx_ll_dma.h
- ll_dma_enable() : gr55xx_ll_dma.h
- ll_dma_enable_channel() : gr55xx_ll_dma.h
- ll_dma_enable_it() : gr55xx_ll_dma.h
- ll_dma_enable_it_blk() : gr55xx_ll_dma.h
- ll_dma_enable_it_dstt() : gr55xx_ll_dma.h
- ll_dma_enable_it_err() : gr55xx_ll_dma.h
- ll_dma_enable_it_srct() : gr55xx_ll_dma.h
- ll_dma_enable_it_tfr() : gr55xx_ll_dma.h
- ll_dma_get_block_size() : gr55xx_ll_dma.h
- ll_dma_get_channel_priority_level() : gr55xx_ll_dma.h
- ll_dma_get_data_transfer_direction() : gr55xx_ll_dma.h
- ll_dma_get_destination_address() : gr55xx_ll_dma.h
- ll_dma_get_destination_burst_length() : gr55xx_ll_dma.h
- ll_dma_get_destination_increment_mode() : gr55xx_ll_dma.h
- ll_dma_get_destination_peripheral() : gr55xx_ll_dma.h
- ll_dma_get_destination_width() : gr55xx_ll_dma.h
- ll_dma_get_m2m_dst_address() : gr55xx_ll_dma.h
- ll_dma_get_m2m_src_address() : gr55xx_ll_dma.h
- ll_dma_get_mode() : gr55xx_ll_dma.h
- ll_dma_get_source_address() : gr55xx_ll_dma.h
- ll_dma_get_source_burst_length() : gr55xx_ll_dma.h
- ll_dma_get_source_increment_mode() : gr55xx_ll_dma.h
- ll_dma_get_source_peripheral() : gr55xx_ll_dma.h
- ll_dma_get_source_width() : gr55xx_ll_dma.h
- ll_dma_init() : gr55xx_ll_dma.h
- ll_dma_init_t : gr55xx_ll_dma.h
- ll_dma_is_active_flag_blk() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_blk0() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_blk1() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_blk2() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_blk3() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_blk4() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_blk5() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_blk6() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_blk7() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_dstt() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_dstt0() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_dstt1() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_dstt2() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_dstt3() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_dstt4() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_dstt5() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_dstt6() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_dstt7() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_err() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_err0() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_err1() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_err2() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_err3() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_err4() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_err5() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_err6() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_err7() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_gblk() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_gdstt() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_gerr() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_gsrct() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_gtfr() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_rblk() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_rdstt() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_rerr() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_rsrct() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_rtfr() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_srct() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_srct0() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_srct1() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_srct2() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_srct3() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_srct4() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_srct5() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_srct6() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_srct7() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_tfr() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_tfr0() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_tfr1() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_tfr2() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_tfr3() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_tfr4() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_tfr5() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_tfr6() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_tfr7() : gr55xx_ll_dma.h
- ll_dma_is_empty_fifo() : gr55xx_ll_dma.h
- ll_dma_is_enable() : gr55xx_ll_dma.h
- ll_dma_is_enable_it_blk() : gr55xx_ll_dma.h
- ll_dma_is_enable_it_dstt() : gr55xx_ll_dma.h
- ll_dma_is_enable_it_err() : gr55xx_ll_dma.h
- ll_dma_is_enable_it_srct() : gr55xx_ll_dma.h
- ll_dma_is_enable_it_tfr() : gr55xx_ll_dma.h
- ll_dma_is_enabled_channel() : gr55xx_ll_dma.h
- ll_dma_is_suspended() : gr55xx_ll_dma.h
- LL_DMA_MODE_MULTI_BLOCK_ALL_RELOAD : gr55xx_ll_dma.h
- LL_DMA_MODE_MULTI_BLOCK_DST_RELOAD : gr55xx_ll_dma.h
- LL_DMA_MODE_MULTI_BLOCK_SRC_RELOAD : gr55xx_ll_dma.h
- LL_DMA_MODE_SINGLE_BLOCK : gr55xx_ll_dma.h
- LL_DMA_PERIPH_I2C0_RX : gr55xx_ll_dma.h
- LL_DMA_PERIPH_I2C0_TX : gr55xx_ll_dma.h
- LL_DMA_PERIPH_I2C1_RX : gr55xx_ll_dma.h
- LL_DMA_PERIPH_I2C1_TX : gr55xx_ll_dma.h
- LL_DMA_PERIPH_I2S_M_RX : gr55xx_ll_dma.h
- LL_DMA_PERIPH_I2S_M_TX : gr55xx_ll_dma.h
- LL_DMA_PERIPH_I2S_S_RX : gr55xx_ll_dma.h
- LL_DMA_PERIPH_I2S_S_TX : gr55xx_ll_dma.h
- LL_DMA_PERIPH_MEM : gr55xx_ll_dma.h
- LL_DMA_PERIPH_QSPI0_RX : gr55xx_ll_dma.h
- LL_DMA_PERIPH_QSPI0_TX : gr55xx_ll_dma.h
- LL_DMA_PERIPH_QSPI1_RX : gr55xx_ll_dma.h
- LL_DMA_PERIPH_QSPI1_TX : gr55xx_ll_dma.h
- LL_DMA_PERIPH_SNSADC : gr55xx_ll_dma.h
- LL_DMA_PERIPH_SPIM_RX : gr55xx_ll_dma.h
- LL_DMA_PERIPH_SPIM_TX : gr55xx_ll_dma.h
- LL_DMA_PERIPH_SPIS_RX : gr55xx_ll_dma.h
- LL_DMA_PERIPH_SPIS_TX : gr55xx_ll_dma.h
- LL_DMA_PERIPH_UART0_RX : gr55xx_ll_dma.h
- LL_DMA_PERIPH_UART0_TX : gr55xx_ll_dma.h
- LL_DMA_PRIORITY_0 : gr55xx_ll_dma.h
- LL_DMA_PRIORITY_1 : gr55xx_ll_dma.h
- LL_DMA_PRIORITY_2 : gr55xx_ll_dma.h
- LL_DMA_PRIORITY_3 : gr55xx_ll_dma.h
- LL_DMA_PRIORITY_4 : gr55xx_ll_dma.h
- LL_DMA_PRIORITY_5 : gr55xx_ll_dma.h
- LL_DMA_PRIORITY_6 : gr55xx_ll_dma.h
- LL_DMA_PRIORITY_7 : gr55xx_ll_dma.h
- LL_DMA_ReadReg : gr55xx_ll_dma.h
- ll_dma_req_dst_burst_transaction() : gr55xx_ll_dma.h
- ll_dma_req_dst_last_burst_transaction() : gr55xx_ll_dma.h
- ll_dma_req_dst_last_single_transaction() : gr55xx_ll_dma.h
- ll_dma_req_dst_single_transaction() : gr55xx_ll_dma.h
- ll_dma_req_src_burst_transaction() : gr55xx_ll_dma.h
- ll_dma_req_src_last_burst_transaction() : gr55xx_ll_dma.h
- ll_dma_req_src_last_single_transaction() : gr55xx_ll_dma.h
- ll_dma_req_src_single_transaction() : gr55xx_ll_dma.h
- ll_dma_resume_channel() : gr55xx_ll_dma.h
- LL_DMA_SDATAALIGN_BYTE : gr55xx_ll_dma.h
- LL_DMA_SDATAALIGN_HALFWORD : gr55xx_ll_dma.h
- LL_DMA_SDATAALIGN_WORD : gr55xx_ll_dma.h
- ll_dma_select_handshaking() : gr55xx_ll_dma.h
- ll_dma_set_block_size() : gr55xx_ll_dma.h
- ll_dma_set_channel_priority_level() : gr55xx_ll_dma.h
- ll_dma_set_data_transfer_direction() : gr55xx_ll_dma.h
- ll_dma_set_destination_address() : gr55xx_ll_dma.h
- ll_dma_set_destination_burst_length() : gr55xx_ll_dma.h
- ll_dma_set_destination_increment_mode() : gr55xx_ll_dma.h
- ll_dma_set_destination_peripheral() : gr55xx_ll_dma.h
- ll_dma_set_destination_width() : gr55xx_ll_dma.h
- ll_dma_set_m2m_dst_address() : gr55xx_ll_dma.h
- ll_dma_set_m2m_src_address() : gr55xx_ll_dma.h
- ll_dma_set_mode() : gr55xx_ll_dma.h
- ll_dma_set_source_address() : gr55xx_ll_dma.h
- ll_dma_set_source_burst_length() : gr55xx_ll_dma.h
- ll_dma_set_source_increment_mode() : gr55xx_ll_dma.h
- ll_dma_set_source_peripheral() : gr55xx_ll_dma.h
- ll_dma_set_source_width() : gr55xx_ll_dma.h
- LL_DMA_SHANDSHAKING_HW : gr55xx_ll_dma.h
- LL_DMA_SHANDSHAKING_SW : gr55xx_ll_dma.h
- LL_DMA_SRC_BURST_LENGTH_1 : gr55xx_ll_dma.h
- LL_DMA_SRC_BURST_LENGTH_16 : gr55xx_ll_dma.h
- LL_DMA_SRC_BURST_LENGTH_32 : gr55xx_ll_dma.h
- LL_DMA_SRC_BURST_LENGTH_4 : gr55xx_ll_dma.h
- LL_DMA_SRC_BURST_LENGTH_64 : gr55xx_ll_dma.h
- LL_DMA_SRC_BURST_LENGTH_8 : gr55xx_ll_dma.h
- LL_DMA_SRC_DECREMENT : gr55xx_ll_dma.h
- LL_DMA_SRC_INCREMENT : gr55xx_ll_dma.h
- LL_DMA_SRC_NO_CHANGE : gr55xx_ll_dma.h
- ll_dma_struct_init() : gr55xx_ll_dma.h
- ll_dma_suspend_channel() : gr55xx_ll_dma.h
- LL_DMA_WriteReg : gr55xx_ll_dma.h
- ll_dual_timer_clear_flag_it() : gr55xx_ll_dual_tim.h
- LL_DUAL_TIMER_COUNTERSIZE_16 : gr55xx_ll_dual_tim.h
- LL_DUAL_TIMER_COUNTERSIZE_32 : gr55xx_ll_dual_tim.h
- ll_dual_timer_deinit() : gr55xx_ll_dual_tim.h
- ll_dual_timer_disable_counter() : gr55xx_ll_dual_tim.h
- ll_dual_timer_disable_it() : gr55xx_ll_dual_tim.h
- ll_dual_timer_disable_oneshot() : gr55xx_ll_dual_tim.h
- ll_dual_timer_enable_counter() : gr55xx_ll_dual_tim.h
- ll_dual_timer_enable_it() : gr55xx_ll_dual_tim.h
- ll_dual_timer_enable_oneshot() : gr55xx_ll_dual_tim.h
- LL_DUAL_TIMER_FREERUNNING_MODE : gr55xx_ll_dual_tim.h
- ll_dual_timer_get_auto_reload() : gr55xx_ll_dual_tim.h
- ll_dual_timer_get_background_reload() : gr55xx_ll_dual_tim.h
- ll_dual_timer_get_counter() : gr55xx_ll_dual_tim.h
- ll_dual_timer_get_counter_mode() : gr55xx_ll_dual_tim.h
- ll_dual_timer_get_counter_size() : gr55xx_ll_dual_tim.h
- ll_dual_timer_get_prescaler() : gr55xx_ll_dual_tim.h
- ll_dual_timer_get_raw_it_flag() : gr55xx_ll_dual_tim.h
- ll_dual_timer_init() : gr55xx_ll_dual_tim.h
- ll_dual_timer_init_t : gr55xx_ll_dual_tim.h
- ll_dual_timer_is_active_flag_it() : gr55xx_ll_dual_tim.h
- ll_dual_timer_is_enabled_counter() : gr55xx_ll_dual_tim.h
- ll_dual_timer_is_enabled_it() : gr55xx_ll_dual_tim.h
- ll_dual_timer_is_enabled_oneshot() : gr55xx_ll_dual_tim.h
- LL_DUAL_TIMER_PERIODIC_MODE : gr55xx_ll_dual_tim.h
- LL_DUAL_TIMER_PRESCALER_DIV0 : gr55xx_ll_dual_tim.h
- LL_DUAL_TIMER_PRESCALER_DIV16 : gr55xx_ll_dual_tim.h
- LL_DUAL_TIMER_PRESCALER_DIV256 : gr55xx_ll_dual_tim.h
- LL_DUAL_TIMER_ReadReg : gr55xx_ll_dual_tim.h
- ll_dual_timer_set_auto_reload() : gr55xx_ll_dual_tim.h
- ll_dual_timer_set_background_reload() : gr55xx_ll_dual_tim.h
- ll_dual_timer_set_counter_mode() : gr55xx_ll_dual_tim.h
- ll_dual_timer_set_counter_size() : gr55xx_ll_dual_tim.h
- ll_dual_timer_set_prescaler() : gr55xx_ll_dual_tim.h
- ll_dual_timer_struct_init() : gr55xx_ll_dual_tim.h
- LL_DUAL_TIMER_WriteReg : gr55xx_ll_dual_tim.h
- LL_ECC_CURVE_DEFAULT_CONFIG : gr55xx_ll_pkc.h
- ll_ecc_curve_init_t : gr55xx_ll_pkc.h
- LL_ECC_CURVE_SECP256K1_CONFIG : gr55xx_ll_pkc.h
- LL_ECC_CURVE_SECP256R1_CONFIG : gr55xx_ll_pkc.h
- ll_ecc_point_t : gr55xx_ll_pkc.h
- LL_EFUSE_CRC_CHECK : gr55xx_ll_efuse.h
- LL_EFUSE_CRC_CHECK_DONE : gr55xx_ll_efuse.h
- LL_EFUSE_CRC_CHECK_SUCCESS : gr55xx_ll_efuse.h
- ll_efuse_disable_controller_power() : gr55xx_ll_efuse.h
- ll_efuse_disable_main_backup() : gr55xx_ll_efuse.h
- ll_efuse_disable_pgenb() : gr55xx_ll_efuse.h
- ll_efuse_disable_power() : gr55xx_ll_efuse.h
- ll_efuse_enable_controller_power_begin() : gr55xx_ll_efuse.h
- ll_efuse_enable_controller_power_stop() : gr55xx_ll_efuse.h
- ll_efuse_enable_main_backup() : gr55xx_ll_efuse.h
- ll_efuse_enable_pgenb() : gr55xx_ll_efuse.h
- ll_efuse_enable_power() : gr55xx_ll_efuse.h
- ll_efuse_get_crc_check_addr() : gr55xx_ll_efuse.h
- ll_efuse_get_crc_check_len() : gr55xx_ll_efuse.h
- ll_efuse_get_crc_check_result() : gr55xx_ll_efuse.h
- ll_efuse_get_interval() : gr55xx_ll_efuse.h
- ll_efuse_get_key_mask() : gr55xx_ll_efuse.h
- ll_efuse_get_test_mode() : gr55xx_ll_efuse.h
- ll_efuse_get_tpro() : gr55xx_ll_efuse.h
- ll_efuse_get_trim_addr() : gr55xx_ll_efuse.h
- ll_efuse_get_trim_length() : gr55xx_ll_efuse.h
- ll_efuse_get_trim_value() : gr55xx_ll_efuse.h
- LL_EFUSE_INIT_CHECK : gr55xx_ll_efuse.h
- LL_EFUSE_INIT_CHECK_DONE : gr55xx_ll_efuse.h
- LL_EFUSE_INIT_CHECK_SUCCESS : gr55xx_ll_efuse.h
- ll_efuse_is_active_flag() : gr55xx_ll_efuse.h
- ll_efuse_is_controller_power_flag() : gr55xx_ll_efuse.h
- ll_efuse_is_enabled_main_backup() : gr55xx_ll_efuse.h
- ll_efuse_is_enabled_pgenb() : gr55xx_ll_efuse.h
- LL_EFUSE_PWR_CTL_DIS_DONE : gr55xx_ll_efuse.h
- LL_EFUSE_PWR_CTL_EN_DONE : gr55xx_ll_efuse.h
- LL_EFUSE_READ_TRIM : gr55xx_ll_efuse.h
- LL_EFUSE_READ_TRIM_DONE : gr55xx_ll_efuse.h
- LL_EFUSE_ReadReg : gr55xx_ll_efuse.h
- ll_efuse_set_controller_power_timing() : gr55xx_ll_efuse.h
- ll_efuse_set_crc_check_addr() : gr55xx_ll_efuse.h
- ll_efuse_set_crc_check_len() : gr55xx_ll_efuse.h
- ll_efuse_set_interval() : gr55xx_ll_efuse.h
- ll_efuse_set_key_mask() : gr55xx_ll_efuse.h
- ll_efuse_set_operation() : gr55xx_ll_efuse.h
- ll_efuse_set_tpro() : gr55xx_ll_efuse.h
- ll_efuse_set_trim_addr() : gr55xx_ll_efuse.h
- ll_efuse_set_trim_length() : gr55xx_ll_efuse.h
- LL_EFUSE_TEST_DONE : gr55xx_ll_efuse.h
- LL_EFUSE_TEST_READ : gr55xx_ll_efuse.h
- LL_EFUSE_WRITE_DONE : gr55xx_ll_efuse.h
- LL_EFUSE_WRITE_KEYRAM : gr55xx_ll_efuse.h
- LL_EFUSE_WRITE_KEYRAM_BUSY : gr55xx_ll_efuse.h
- LL_EFUSE_WriteReg : gr55xx_ll_efuse.h
- ll_gpio_clear_flag_it() : gr55xx_ll_gpio.h
- LL_GPIO_DEFAULT_CONFIG : gr55xx_ll_gpio.h
- ll_gpio_deinit() : gr55xx_ll_gpio.h
- ll_gpio_disable_it() : gr55xx_ll_gpio.h
- ll_gpio_enable_falling_trigger() : gr55xx_ll_gpio.h
- ll_gpio_enable_high_trigger() : gr55xx_ll_gpio.h
- ll_gpio_enable_it() : gr55xx_ll_gpio.h
- ll_gpio_enable_low_trigger() : gr55xx_ll_gpio.h
- ll_gpio_enable_rising_trigger() : gr55xx_ll_gpio.h
- ll_gpio_get_mux_pin_0_7() : gr55xx_ll_gpio.h
- ll_gpio_get_mux_pin_8_15() : gr55xx_ll_gpio.h
- ll_gpio_get_pin_mode() : gr55xx_ll_gpio.h
- ll_gpio_get_pin_pull() : gr55xx_ll_gpio.h
- LL_GPIO_GET_REG_MUX_CTRL_0_7 : gr55xx_ll_gpio.h
- LL_GPIO_GET_REG_MUX_CTRL_8_15 : gr55xx_ll_gpio.h
- LL_GPIO_GET_RESISTOR_POS : gr55xx_ll_gpio.h
- ll_gpio_init() : gr55xx_ll_gpio.h
- ll_gpio_init_t : gr55xx_ll_gpio.h
- ll_gpio_is_active_flag_it() : gr55xx_ll_gpio.h
- ll_gpio_is_enabled_falling_trigger() : gr55xx_ll_gpio.h
- ll_gpio_is_enabled_high_trigger() : gr55xx_ll_gpio.h
- ll_gpio_is_enabled_it() : gr55xx_ll_gpio.h
- ll_gpio_is_enabled_low_trigger() : gr55xx_ll_gpio.h
- ll_gpio_is_enabled_rising_trigger() : gr55xx_ll_gpio.h
- ll_gpio_is_input_pin_set() : gr55xx_ll_gpio.h
- ll_gpio_is_output_pin_set() : gr55xx_ll_gpio.h
- LL_GPIO_MODE_INPUT : gr55xx_ll_gpio.h
- LL_GPIO_MODE_MUX : gr55xx_ll_gpio.h
- LL_GPIO_MODE_OUTPUT : gr55xx_ll_gpio.h
- LL_GPIO_MUX_0 : gr55xx_ll_gpio.h
- LL_GPIO_MUX_1 : gr55xx_ll_gpio.h
- LL_GPIO_MUX_2 : gr55xx_ll_gpio.h
- LL_GPIO_MUX_3 : gr55xx_ll_gpio.h
- LL_GPIO_MUX_4 : gr55xx_ll_gpio.h
- LL_GPIO_MUX_5 : gr55xx_ll_gpio.h
- LL_GPIO_MUX_6 : gr55xx_ll_gpio.h
- LL_GPIO_MUX_7 : gr55xx_ll_gpio.h
- LL_GPIO_MUX_8 : gr55xx_ll_gpio.h
- LL_GPIO_PIN_0 : gr55xx_ll_gpio.h
- LL_GPIO_PIN_1 : gr55xx_ll_gpio.h
- LL_GPIO_PIN_10 : gr55xx_ll_gpio.h
- LL_GPIO_PIN_11 : gr55xx_ll_gpio.h
- LL_GPIO_PIN_12 : gr55xx_ll_gpio.h
- LL_GPIO_PIN_13 : gr55xx_ll_gpio.h
- LL_GPIO_PIN_14 : gr55xx_ll_gpio.h
- LL_GPIO_PIN_15 : gr55xx_ll_gpio.h
- LL_GPIO_PIN_2 : gr55xx_ll_gpio.h
- LL_GPIO_PIN_3 : gr55xx_ll_gpio.h
- LL_GPIO_PIN_4 : gr55xx_ll_gpio.h
- LL_GPIO_PIN_5 : gr55xx_ll_gpio.h
- LL_GPIO_PIN_6 : gr55xx_ll_gpio.h
- LL_GPIO_PIN_7 : gr55xx_ll_gpio.h
- LL_GPIO_PIN_8 : gr55xx_ll_gpio.h
- LL_GPIO_PIN_9 : gr55xx_ll_gpio.h
- LL_GPIO_PIN_ALL : gr55xx_ll_gpio.h
- LL_GPIO_PULL_DOWN : gr55xx_ll_gpio.h
- LL_GPIO_PULL_NO : gr55xx_ll_gpio.h
- LL_GPIO_PULL_UP : gr55xx_ll_gpio.h
- LL_GPIO_RE_N : gr55xx_ll_gpio.h
- LL_GPIO_RE_N_Msk : gr55xx_ll_gpio.h
- LL_GPIO_RE_N_Pos : gr55xx_ll_gpio.h
- ll_gpio_read_flag_it() : gr55xx_ll_gpio.h
- ll_gpio_read_input_port() : gr55xx_ll_gpio.h
- ll_gpio_read_output_port() : gr55xx_ll_gpio.h
- LL_GPIO_ReadReg : gr55xx_ll_gpio.h
- ll_gpio_reset_output_pin() : gr55xx_ll_gpio.h
- LL_GPIO_RTYP : gr55xx_ll_gpio.h
- LL_GPIO_RTYP_Msk : gr55xx_ll_gpio.h
- LL_GPIO_RTYP_Pos : gr55xx_ll_gpio.h
- ll_gpio_set_mux_pin_0_7() : gr55xx_ll_gpio.h
- ll_gpio_set_mux_pin_8_15() : gr55xx_ll_gpio.h
- ll_gpio_set_output_pin() : gr55xx_ll_gpio.h
- ll_gpio_set_pin_mode() : gr55xx_ll_gpio.h
- ll_gpio_set_pin_pull() : gr55xx_ll_gpio.h
- ll_gpio_struct_init() : gr55xx_ll_gpio.h
- ll_gpio_toggle_pin() : gr55xx_ll_gpio.h
- LL_GPIO_TRIGGER_FALLING : gr55xx_ll_gpio.h
- LL_GPIO_TRIGGER_HIGH : gr55xx_ll_gpio.h
- LL_GPIO_TRIGGER_LOW : gr55xx_ll_gpio.h
- LL_GPIO_TRIGGER_NONE : gr55xx_ll_gpio.h
- LL_GPIO_TRIGGER_RISING : gr55xx_ll_gpio.h
- ll_gpio_write_output_port() : gr55xx_ll_gpio.h
- LL_GPIO_WriteReg : gr55xx_ll_gpio.h
- LL_HMAC_CALCULATETYPE_HMAC : gr55xx_ll_hmac.h
- LL_HMAC_CALCULATETYPE_SHA : gr55xx_ll_hmac.h
- ll_hmac_clear_flag_it_done() : gr55xx_ll_hmac.h
- ll_hmac_deinit() : gr55xx_ll_hmac.h
- ll_hmac_disable() : gr55xx_ll_hmac.h
- ll_hmac_disable_dma_start() : gr55xx_ll_hmac.h
- ll_hmac_disable_it_done() : gr55xx_ll_hmac.h
- ll_hmac_disable_little_endian() : gr55xx_ll_hmac.h
- ll_hmac_disable_private() : gr55xx_ll_hmac.h
- ll_hmac_disable_sha() : gr55xx_ll_hmac.h
- ll_hmac_disable_user_hash() : gr55xx_ll_hmac.h
- LL_HMAC_DMA_TRANSIZE_MAX : gr55xx_ll_hmac.h
- LL_HMAC_DMA_TRANSIZE_MIN : gr55xx_ll_hmac.h
- ll_hmac_enable() : gr55xx_ll_hmac.h
- ll_hmac_enable_dma_start() : gr55xx_ll_hmac.h
- ll_hmac_enable_it_done() : gr55xx_ll_hmac.h
- ll_hmac_enable_last_transfer() : gr55xx_ll_hmac.h
- ll_hmac_enable_little_endian() : gr55xx_ll_hmac.h
- ll_hmac_enable_private() : gr55xx_ll_hmac.h
- ll_hmac_enable_read_key() : gr55xx_ll_hmac.h
- ll_hmac_enable_sha() : gr55xx_ll_hmac.h
- ll_hmac_enable_user_hash() : gr55xx_ll_hmac.h
- LL_HMAC_FLAG_DATAREADY_HMAC : gr55xx_ll_hmac.h
- LL_HMAC_FLAG_DATAREADY_SHA : gr55xx_ll_hmac.h
- LL_HMAC_FLAG_DMA_DONE : gr55xx_ll_hmac.h
- LL_HMAC_FLAG_DMA_ERR : gr55xx_ll_hmac.h
- LL_HMAC_FLAG_DMA_MESSAGEDONE : gr55xx_ll_hmac.h
- LL_HMAC_FLAG_KEY_VALID : gr55xx_ll_hmac.h
- ll_hmac_get_data() : gr55xx_ll_hmac.h
- ll_hmac_get_dma_read_address() : gr55xx_ll_hmac.h
- ll_hmac_get_dma_transfer_block() : gr55xx_ll_hmac.h
- ll_hmac_get_dma_write_address() : gr55xx_ll_hmac.h
- ll_hmac_get_key_address() : gr55xx_ll_hmac.h
- ll_hmac_get_key_type() : gr55xx_ll_hmac.h
- LL_HMAC_HASH_STANDARD : gr55xx_ll_hmac.h
- LL_HMAC_HASH_USER : gr55xx_ll_hmac.h
- ll_hmac_init() : gr55xx_ll_hmac.h
- ll_hmac_init_t : gr55xx_ll_hmac.h
- ll_hmac_is_action_flag_dma_done() : gr55xx_ll_hmac.h
- ll_hmac_is_action_flag_dma_error() : gr55xx_ll_hmac.h
- ll_hmac_is_action_flag_dma_message_done() : gr55xx_ll_hmac.h
- ll_hmac_is_action_flag_hmac_ready() : gr55xx_ll_hmac.h
- ll_hmac_is_action_flag_it_done() : gr55xx_ll_hmac.h
- ll_hmac_is_action_flag_key_valid() : gr55xx_ll_hmac.h
- ll_hmac_is_action_flag_sha_ready() : gr55xx_ll_hmac.h
- ll_hmac_is_enabled() : gr55xx_ll_hmac.h
- ll_hmac_is_enabled_dma_start() : gr55xx_ll_hmac.h
- ll_hmac_is_enabled_it_done() : gr55xx_ll_hmac.h
- ll_hmac_is_enabled_little_endian() : gr55xx_ll_hmac.h
- ll_hmac_is_enabled_private() : gr55xx_ll_hmac.h
- ll_hmac_is_enabled_sha() : gr55xx_ll_hmac.h
- ll_hmac_is_enabled_user_hash() : gr55xx_ll_hmac.h
- LL_HMAC_KEYTYPE_AHB : gr55xx_ll_hmac.h
- LL_HMAC_KEYTYPE_KRAM : gr55xx_ll_hmac.h
- LL_HMAC_KEYTYPE_MCU : gr55xx_ll_hmac.h
- LL_HMAC_ReadReg : gr55xx_ll_hmac.h
- ll_hmac_set_data() : gr55xx_ll_hmac.h
- ll_hmac_set_dma_read_address() : gr55xx_ll_hmac.h
- ll_hmac_set_dma_transfer_block() : gr55xx_ll_hmac.h
- ll_hmac_set_dma_write_address() : gr55xx_ll_hmac.h
- ll_hmac_set_key0() : gr55xx_ll_hmac.h
- ll_hmac_set_key1() : gr55xx_ll_hmac.h
- ll_hmac_set_key2() : gr55xx_ll_hmac.h
- ll_hmac_set_key3() : gr55xx_ll_hmac.h
- ll_hmac_set_key4() : gr55xx_ll_hmac.h
- ll_hmac_set_key5() : gr55xx_ll_hmac.h
- ll_hmac_set_key6() : gr55xx_ll_hmac.h
- ll_hmac_set_key7() : gr55xx_ll_hmac.h
- ll_hmac_set_key_address() : gr55xx_ll_hmac.h
- ll_hmac_set_key_port_mask() : gr55xx_ll_hmac.h
- ll_hmac_set_key_type() : gr55xx_ll_hmac.h
- ll_hmac_set_user_hash_127_96() : gr55xx_ll_hmac.h
- ll_hmac_set_user_hash_159_128() : gr55xx_ll_hmac.h
- ll_hmac_set_user_hash_191_160() : gr55xx_ll_hmac.h
- ll_hmac_set_user_hash_223_192() : gr55xx_ll_hmac.h
- ll_hmac_set_user_hash_255_224() : gr55xx_ll_hmac.h
- ll_hmac_set_user_hash_31_0() : gr55xx_ll_hmac.h
- ll_hmac_set_user_hash_63_32() : gr55xx_ll_hmac.h
- ll_hmac_set_user_hash_95_64() : gr55xx_ll_hmac.h
- ll_hmac_struct_init() : gr55xx_ll_hmac.h
- LL_HMAC_WriteReg : gr55xx_ll_hmac.h
- LL_I2C_ABRT_10ADDR1_NOACK : gr55xx_ll_i2c.h
- LL_I2C_ABRT_10ADDR2_NOACK : gr55xx_ll_i2c.h
- LL_I2C_ABRT_10B_RD_NORSTRT : gr55xx_ll_i2c.h
- LL_I2C_ABRT_7B_ADDR_NOACK : gr55xx_ll_i2c.h
- LL_I2C_ABRT_ARB_LOST : gr55xx_ll_i2c.h
- LL_I2C_ABRT_GCALL_NOACK : gr55xx_ll_i2c.h
- LL_I2C_ABRT_GCALL_READ : gr55xx_ll_i2c.h
- LL_I2C_ABRT_HS_ACKDET : gr55xx_ll_i2c.h
- LL_I2C_ABRT_HS_NORSTRT : gr55xx_ll_i2c.h
- LL_I2C_ABRT_MST_DIS : gr55xx_ll_i2c.h
- LL_I2C_ABRT_SBYTE_ACKDET : gr55xx_ll_i2c.h
- LL_I2C_ABRT_SBYTE_NORSTRT : gr55xx_ll_i2c.h
- LL_I2C_ABRT_SLV_ARBLOST : gr55xx_ll_i2c.h
- LL_I2C_ABRT_SLVFLUSH_TXFIFO : gr55xx_ll_i2c.h
- LL_I2C_ABRT_SLVRD_INTX : gr55xx_ll_i2c.h
- LL_I2C_ABRT_TX_FLUSH_CNT : gr55xx_ll_i2c.h
- LL_I2C_ABRT_TXDATA_NOACK : gr55xx_ll_i2c.h
- LL_I2C_ABRT_USER_ABRT : gr55xx_ll_i2c.h
- LL_I2C_ADDRESSING_MODE_10BIT : gr55xx_ll_i2c.h
- LL_I2C_ADDRESSING_MODE_7BIT : gr55xx_ll_i2c.h
- ll_i2c_clear_flag_activity() : gr55xx_ll_i2c.h
- ll_i2c_clear_flag_gen_call() : gr55xx_ll_i2c.h
- ll_i2c_clear_flag_intr() : gr55xx_ll_i2c.h
- ll_i2c_clear_flag_read_req() : gr55xx_ll_i2c.h
- ll_i2c_clear_flag_rx_done() : gr55xx_ll_i2c.h
- ll_i2c_clear_flag_rx_over() : gr55xx_ll_i2c.h
- ll_i2c_clear_flag_rx_under() : gr55xx_ll_i2c.h
- ll_i2c_clear_flag_start_det() : gr55xx_ll_i2c.h
- ll_i2c_clear_flag_stop_det() : gr55xx_ll_i2c.h
- ll_i2c_clear_flag_tx_abort() : gr55xx_ll_i2c.h
- ll_i2c_clear_flag_tx_over() : gr55xx_ll_i2c.h
- LL_I2C_CMD_MST_GEN_RESTART : gr55xx_ll_i2c.h
- LL_I2C_CMD_MST_GEN_STOP : gr55xx_ll_i2c.h
- LL_I2C_CMD_MST_READ : gr55xx_ll_i2c.h
- LL_I2C_CMD_MST_WRITE : gr55xx_ll_i2c.h
- LL_I2C_CMD_SLV_NONE : gr55xx_ll_i2c.h
- LL_I2C_DEFAULT_CONFIG : gr55xx_ll_i2c.h
- ll_i2c_deinit() : gr55xx_ll_i2c.h
- LL_I2C_DIRECTION_ERROR : gr55xx_ll_i2c.h
- LL_I2C_DIRECTION_NONE : gr55xx_ll_i2c.h
- LL_I2C_DIRECTION_READ : gr55xx_ll_i2c.h
- LL_I2C_DIRECTION_WRITE : gr55xx_ll_i2c.h
- ll_i2c_disable() : gr55xx_ll_i2c.h
- ll_i2c_disable_dma_req_rx() : gr55xx_ll_i2c.h
- ll_i2c_disable_dma_req_tx() : gr55xx_ll_i2c.h
- ll_i2c_disable_general_call() : gr55xx_ll_i2c.h
- ll_i2c_disable_it() : gr55xx_ll_i2c.h
- ll_i2c_disable_it_activity() : gr55xx_ll_i2c.h
- ll_i2c_disable_it_gen_call() : gr55xx_ll_i2c.h
- ll_i2c_disable_it_master_om_hold() : gr55xx_ll_i2c.h
- ll_i2c_disable_it_read_req() : gr55xx_ll_i2c.h
- ll_i2c_disable_it_restart_det() : gr55xx_ll_i2c.h
- ll_i2c_disable_it_rx_done() : gr55xx_ll_i2c.h
- ll_i2c_disable_it_rx_over() : gr55xx_ll_i2c.h
- ll_i2c_disable_it_rx_under() : gr55xx_ll_i2c.h
- ll_i2c_disable_it_start_det() : gr55xx_ll_i2c.h
- ll_i2c_disable_it_stop_det() : gr55xx_ll_i2c.h
- ll_i2c_disable_it_tx_abort() : gr55xx_ll_i2c.h
- ll_i2c_disable_it_tx_empty() : gr55xx_ll_i2c.h
- ll_i2c_disable_it_tx_over() : gr55xx_ll_i2c.h
- ll_i2c_disable_master_mode() : gr55xx_ll_i2c.h
- ll_i2c_disable_master_restart() : gr55xx_ll_i2c.h
- ll_i2c_disable_stop_det_if_addressed() : gr55xx_ll_i2c.h
- ll_i2c_disbale_it_rx_full() : gr55xx_ll_i2c.h
- ll_i2c_dma_get_register_address() : gr55xx_ll_i2c.h
- ll_i2c_enable() : gr55xx_ll_i2c.h
- ll_i2c_enable_dma_req_rx() : gr55xx_ll_i2c.h
- ll_i2c_enable_dma_req_tx() : gr55xx_ll_i2c.h
- ll_i2c_enable_general_call() : gr55xx_ll_i2c.h
- ll_i2c_enable_it() : gr55xx_ll_i2c.h
- ll_i2c_enable_it_activity() : gr55xx_ll_i2c.h
- ll_i2c_enable_it_gen_call() : gr55xx_ll_i2c.h
- ll_i2c_enable_it_master_on_hold() : gr55xx_ll_i2c.h
- ll_i2c_enable_it_read_req() : gr55xx_ll_i2c.h
- ll_i2c_enable_it_restart_det() : gr55xx_ll_i2c.h
- ll_i2c_enable_it_rx_abort() : gr55xx_ll_i2c.h
- ll_i2c_enable_it_rx_done() : gr55xx_ll_i2c.h
- ll_i2c_enable_it_rx_full() : gr55xx_ll_i2c.h
- ll_i2c_enable_it_rx_over() : gr55xx_ll_i2c.h
- ll_i2c_enable_it_rx_under() : gr55xx_ll_i2c.h
- ll_i2c_enable_it_start_det() : gr55xx_ll_i2c.h
- ll_i2c_enable_it_stop_det() : gr55xx_ll_i2c.h
- ll_i2c_enable_it_tx_empty() : gr55xx_ll_i2c.h
- ll_i2c_enable_it_tx_over() : gr55xx_ll_i2c.h
- ll_i2c_enable_master_mode() : gr55xx_ll_i2c.h
- ll_i2c_enable_master_restart() : gr55xx_ll_i2c.h
- ll_i2c_enable_stop_det_if_addressed() : gr55xx_ll_i2c.h
- ll_i2c_enable_transfer_abort() : gr55xx_ll_i2c.h
- ll_i2c_get_abort_source() : gr55xx_ll_i2c.h
- ll_i2c_get_clock_high_period_fs() : gr55xx_ll_i2c.h
- ll_i2c_get_clock_high_period_hs() : gr55xx_ll_i2c.h
- ll_i2c_get_clock_high_period_ss() : gr55xx_ll_i2c.h
- ll_i2c_get_clock_low_period_fs() : gr55xx_ll_i2c.h
- ll_i2c_get_clock_low_period_hs() : gr55xx_ll_i2c.h
- ll_i2c_get_clock_low_period_ss() : gr55xx_ll_i2c.h
- ll_i2c_get_data_rx_hold_time() : gr55xx_ll_i2c.h
- ll_i2c_get_data_setup_time() : gr55xx_ll_i2c.h
- ll_i2c_get_data_tx_hold_time() : gr55xx_ll_i2c.h
- ll_i2c_get_dma_rx_data_level() : gr55xx_ll_i2c.h
- ll_i2c_get_dma_tx_data_level() : gr55xx_ll_i2c.h
- ll_i2c_get_high_speed_master_code() : gr55xx_ll_i2c.h
- ll_i2c_get_it_flag() : gr55xx_ll_i2c.h
- ll_i2c_get_master_addressing_mode() : gr55xx_ll_i2c.h
- ll_i2c_get_raw_it_flag() : gr55xx_ll_i2c.h
- ll_i2c_get_rx_fifo_level() : gr55xx_ll_i2c.h
- ll_i2c_get_rx_fifo_threshold() : gr55xx_ll_i2c.h
- ll_i2c_get_slave_address() : gr55xx_ll_i2c.h
- ll_i2c_get_speed_mode() : gr55xx_ll_i2c.h
- ll_i2c_get_spike_len_fs() : gr55xx_ll_i2c.h
- ll_i2c_get_spike_len_hs() : gr55xx_ll_i2c.h
- ll_i2c_get_transfer_direction() : gr55xx_ll_i2c.h
- ll_i2c_get_tx_fifo_level() : gr55xx_ll_i2c.h
- ll_i2c_get_tx_fifo_threshold() : gr55xx_ll_i2c.h
- ll_i2c_get_tx_flush_count() : gr55xx_ll_i2c.h
- ll_i2c_handle_transfer() : gr55xx_ll_i2c.h
- ll_i2c_init() : gr55xx_ll_i2c.h
- ll_i2c_init_t : gr55xx_ll_i2c.h
- LL_I2C_INTR_MASK_ACTIVITY : gr55xx_ll_i2c.h
- LL_I2C_INTR_MASK_ALL : gr55xx_ll_i2c.h
- LL_I2C_INTR_MASK_GEN_CALL : gr55xx_ll_i2c.h
- LL_I2C_INTR_MASK_MST_ON_HOLD : gr55xx_ll_i2c.h
- LL_I2C_INTR_MASK_RD_REQ : gr55xx_ll_i2c.h
- LL_I2C_INTR_MASK_RESTART_DET : gr55xx_ll_i2c.h
- LL_I2C_INTR_MASK_RX_DONE : gr55xx_ll_i2c.h
- LL_I2C_INTR_MASK_RX_FULL : gr55xx_ll_i2c.h
- LL_I2C_INTR_MASK_RX_OVER : gr55xx_ll_i2c.h
- LL_I2C_INTR_MASK_RX_UNDER : gr55xx_ll_i2c.h
- LL_I2C_INTR_MASK_START_DET : gr55xx_ll_i2c.h
- LL_I2C_INTR_MASK_STOP_DET : gr55xx_ll_i2c.h
- LL_I2C_INTR_MASK_TX_ABRT : gr55xx_ll_i2c.h
- LL_I2C_INTR_MASK_TX_EMPTY : gr55xx_ll_i2c.h
- LL_I2C_INTR_MASK_TX_OVER : gr55xx_ll_i2c.h
- LL_I2C_INTR_STAT_ACTIVITY : gr55xx_ll_i2c.h
- LL_I2C_INTR_STAT_GEN_CALL : gr55xx_ll_i2c.h
- LL_I2C_INTR_STAT_MST_ON_HOLD : gr55xx_ll_i2c.h
- LL_I2C_INTR_STAT_RD_REQ : gr55xx_ll_i2c.h
- LL_I2C_INTR_STAT_RESTART_DET : gr55xx_ll_i2c.h
- LL_I2C_INTR_STAT_RX_DONE : gr55xx_ll_i2c.h
- LL_I2C_INTR_STAT_RX_FULL : gr55xx_ll_i2c.h
- LL_I2C_INTR_STAT_RX_OVER : gr55xx_ll_i2c.h
- LL_I2C_INTR_STAT_RX_UNDER : gr55xx_ll_i2c.h
- LL_I2C_INTR_STAT_START_DET : gr55xx_ll_i2c.h
- LL_I2C_INTR_STAT_STOP_DET : gr55xx_ll_i2c.h
- LL_I2C_INTR_STAT_TX_ABRT : gr55xx_ll_i2c.h
- LL_I2C_INTR_STAT_TX_EMPTY : gr55xx_ll_i2c.h
- LL_I2C_INTR_STAT_TX_OVER : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_activity() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_gen_call() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_master_on_hold() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_raw_activity() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_raw_gen_call() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_raw_master_on_hold() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_raw_read_req() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_raw_restart_det() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_raw_rx_done() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_raw_rx_full() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_raw_rx_over() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_raw_rx_under() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_raw_start_det() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_raw_stop_det() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_raw_tx_abort() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_raw_tx_empty() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_raw_tx_over() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_read_req() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_restart_det() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_rx_done() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_rx_full() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_rx_over() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_rx_under() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_slave_dis_whl_busy() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_slave_rx_data_lost() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_start_det() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_status_activity() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_status_master_activity() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_status_rff() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_status_rfne() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_status_slave_activity() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_status_tfe() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_status_tfnf() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_stop_det() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_tx_abort() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_tx_empty() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_tx_over() : gr55xx_ll_i2c.h
- ll_i2c_is_enable_it_rx_done() : gr55xx_ll_i2c.h
- ll_i2c_is_enabled() : gr55xx_ll_i2c.h
- ll_i2c_is_enabled_dma_req_rx() : gr55xx_ll_i2c.h
- ll_i2c_is_enabled_dma_req_tx() : gr55xx_ll_i2c.h
- ll_i2c_is_enabled_general_call() : gr55xx_ll_i2c.h
- ll_i2c_is_enabled_it() : gr55xx_ll_i2c.h
- ll_i2c_is_enabled_it_activity() : gr55xx_ll_i2c.h
- ll_i2c_is_enabled_it_gen_call() : gr55xx_ll_i2c.h
- ll_i2c_is_enabled_it_master_on_hold() : gr55xx_ll_i2c.h
- ll_i2c_is_enabled_it_read_req() : gr55xx_ll_i2c.h
- ll_i2c_is_enabled_it_restart_det() : gr55xx_ll_i2c.h
- ll_i2c_is_enabled_it_rx_over() : gr55xx_ll_i2c.h
- ll_i2c_is_enabled_it_rx_under() : gr55xx_ll_i2c.h
- ll_i2c_is_enabled_it_start_det() : gr55xx_ll_i2c.h
- ll_i2c_is_enabled_it_stop_det() : gr55xx_ll_i2c.h
- ll_i2c_is_enabled_it_tx_abort() : gr55xx_ll_i2c.h
- ll_i2c_is_enabled_it_tx_empty() : gr55xx_ll_i2c.h
- ll_i2c_is_enabled_it_tx_over() : gr55xx_ll_i2c.h
- ll_i2c_is_enabled_master_mode() : gr55xx_ll_i2c.h
- ll_i2c_is_enabled_master_restart() : gr55xx_ll_i2c.h
- ll_i2c_is_enabled_stop_det_if_addressed() : gr55xx_ll_i2c.h
- ll_i2c_is_enabled_transfer_abort() : gr55xx_ll_i2c.h
- ll_i2c_ls_enabled_it_rx_full() : gr55xx_ll_i2c.h
- LL_I2C_OWNADDRESS_10BIT : gr55xx_ll_i2c.h
- LL_I2C_OWNADDRESS_7BIT : gr55xx_ll_i2c.h
- LL_I2C_ReadReg : gr55xx_ll_i2c.h
- ll_i2c_receive_data8() : gr55xx_ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_1 : gr55xx_ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_2 : gr55xx_ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_3 : gr55xx_ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_4 : gr55xx_ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_5 : gr55xx_ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_6 : gr55xx_ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_7 : gr55xx_ll_i2c.h
- LL_I2C_RX_FIFO_TH_FULL : gr55xx_ll_i2c.h
- ll_i2c_set_clock_high_period_fs() : gr55xx_ll_i2c.h
- ll_i2c_set_clock_high_period_hs() : gr55xx_ll_i2c.h
- ll_i2c_set_clock_high_period_ss() : gr55xx_ll_i2c.h
- ll_i2c_set_clock_low_period_fs() : gr55xx_ll_i2c.h
- ll_i2c_set_clock_low_period_hs() : gr55xx_ll_i2c.h
- ll_i2c_set_clock_low_period_ss() : gr55xx_ll_i2c.h
- ll_i2c_set_data_rx_hold_time() : gr55xx_ll_i2c.h
- ll_i2c_set_data_setup_time() : gr55xx_ll_i2c.h
- ll_i2c_set_data_tx_hold_time() : gr55xx_ll_i2c.h
- ll_i2c_set_dma_rx_data_level() : gr55xx_ll_i2c.h
- ll_i2c_set_dma_tx_data_level() : gr55xx_ll_i2c.h
- ll_i2c_set_high_speed_master_code() : gr55xx_ll_i2c.h
- ll_i2c_set_master_addressing_mode() : gr55xx_ll_i2c.h
- ll_i2c_set_own_address() : gr55xx_ll_i2c.h
- ll_i2c_set_rx_fifo_threshold() : gr55xx_ll_i2c.h
- ll_i2c_set_slave_address() : gr55xx_ll_i2c.h
- ll_i2c_set_speed_mode() : gr55xx_ll_i2c.h
- ll_i2c_set_spike_len_fs() : gr55xx_ll_i2c.h
- ll_i2c_set_spike_len_hs() : gr55xx_ll_i2c.h
- ll_i2c_set_tx_fifo_threshold() : gr55xx_ll_i2c.h
- LL_I2C_SPEED_1000K : gr55xx_ll_i2c.h
- LL_I2C_SPEED_100K : gr55xx_ll_i2c.h
- LL_I2C_SPEED_2000K : gr55xx_ll_i2c.h
- LL_I2C_SPEED_400K : gr55xx_ll_i2c.h
- LL_I2C_SPEED_MODE_FAST : gr55xx_ll_i2c.h
- LL_I2C_SPEED_MODE_HIGH : gr55xx_ll_i2c.h
- LL_I2C_SPEED_MODE_STANDARD : gr55xx_ll_i2c.h
- ll_i2c_struct_init() : gr55xx_ll_i2c.h
- ll_i2c_transmit_data8() : gr55xx_ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_1 : gr55xx_ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_2 : gr55xx_ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_3 : gr55xx_ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_4 : gr55xx_ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_5 : gr55xx_ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_6 : gr55xx_ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_7 : gr55xx_ll_i2c.h
- LL_I2C_TX_FIFO_TH_EMPTY : gr55xx_ll_i2c.h
- LL_I2C_WriteReg : gr55xx_ll_i2c.h
- LL_I2S_APB_WIDTH_16BIT : gr55xx_ll_i2s.h
- LL_I2S_APB_WIDTH_32BIT : gr55xx_ll_i2s.h
- LL_I2S_APB_WIDTH_8BIT : gr55xx_ll_i2s.h
- LL_I2S_CHANNEL_NUM_1 : gr55xx_ll_i2s.h
- LL_I2S_CHANNEL_NUM_2 : gr55xx_ll_i2s.h
- LL_I2S_CHANNEL_NUM_3 : gr55xx_ll_i2s.h
- LL_I2S_CHANNEL_NUM_4 : gr55xx_ll_i2s.h
- ll_i2s_clear_it_rxovr() : gr55xx_ll_i2s.h
- ll_i2s_clear_it_txovr() : gr55xx_ll_i2s.h
- LL_I2S_CLOCK_SRC_32M : gr55xx_ll_i2s.h
- LL_I2S_CLOCK_SRC_96M : gr55xx_ll_i2s.h
- ll_i2s_clr_rxfifo_all() : gr55xx_ll_i2s.h
- ll_i2s_clr_rxfifo_channel() : gr55xx_ll_i2s.h
- ll_i2s_clr_txfifo_all() : gr55xx_ll_i2s.h
- ll_i2s_clr_txfifo_channel() : gr55xx_ll_i2s.h
- LL_I2S_DATASIZE_12BIT : gr55xx_ll_i2s.h
- LL_I2S_DATASIZE_16BIT : gr55xx_ll_i2s.h
- LL_I2S_DATASIZE_20BIT : gr55xx_ll_i2s.h
- LL_I2S_DATASIZE_24BIT : gr55xx_ll_i2s.h
- LL_I2S_DATASIZE_32BIT : gr55xx_ll_i2s.h
- LL_I2S_DATASIZE_IGNORE : gr55xx_ll_i2s.h
- LL_I2S_DEFAULT_CONFIG : gr55xx_ll_i2s.h
- ll_i2s_deinit() : gr55xx_ll_i2s.h
- ll_i2s_disable() : gr55xx_ll_i2s.h
- ll_i2s_disable_clock() : gr55xx_ll_i2s.h
- ll_i2s_disable_clock_div() : gr55xx_ll_i2s.h
- ll_i2s_disable_dma() : gr55xx_ll_i2s.h
- ll_i2s_disable_it() : gr55xx_ll_i2s.h
- ll_i2s_disable_rx() : gr55xx_ll_i2s.h
- ll_i2s_disable_rxblock() : gr55xx_ll_i2s.h
- ll_i2s_disable_tx() : gr55xx_ll_i2s.h
- ll_i2s_disable_txblock() : gr55xx_ll_i2s.h
- ll_i2s_enable() : gr55xx_ll_i2s.h
- ll_i2s_enable_clock() : gr55xx_ll_i2s.h
- ll_i2s_enable_clock_div() : gr55xx_ll_i2s.h
- ll_i2s_enable_dma() : gr55xx_ll_i2s.h
- ll_i2s_enable_it() : gr55xx_ll_i2s.h
- ll_i2s_enable_rx() : gr55xx_ll_i2s.h
- ll_i2s_enable_rxblock() : gr55xx_ll_i2s.h
- ll_i2s_enable_tx() : gr55xx_ll_i2s.h
- ll_i2s_enable_txblock() : gr55xx_ll_i2s.h
- LL_I2S_FIFO_DEPTH_16 : gr55xx_ll_i2s.h
- LL_I2S_FIFO_DEPTH_2 : gr55xx_ll_i2s.h
- LL_I2S_FIFO_DEPTH_4 : gr55xx_ll_i2s.h
- LL_I2S_FIFO_DEPTH_8 : gr55xx_ll_i2s.h
- LL_I2S_FULL_DUPLEX : gr55xx_ll_i2s.h
- ll_i2s_get_apb_width() : gr55xx_ll_i2s.h
- ll_i2s_get_clock_div() : gr55xx_ll_i2s.h
- ll_i2s_get_clock_src() : gr55xx_ll_i2s.h
- ll_i2s_get_fifo_depth() : gr55xx_ll_i2s.h
- ll_i2s_get_it_flag() : gr55xx_ll_i2s.h
- ll_i2s_get_master_mode() : gr55xx_ll_i2s.h
- ll_i2s_get_rx_block() : gr55xx_ll_i2s.h
- ll_i2s_get_rx_channels() : gr55xx_ll_i2s.h
- ll_i2s_get_rx_fifo_threshold() : gr55xx_ll_i2s.h
- ll_i2s_get_rx_resolution() : gr55xx_ll_i2s.h
- ll_i2s_get_rxsize() : gr55xx_ll_i2s.h
- ll_i2s_get_sclkg() : gr55xx_ll_i2s.h
- ll_i2s_get_tx_block() : gr55xx_ll_i2s.h
- ll_i2s_get_tx_channels() : gr55xx_ll_i2s.h
- ll_i2s_get_tx_fifo_threshold() : gr55xx_ll_i2s.h
- ll_i2s_get_tx_resolution() : gr55xx_ll_i2s.h
- ll_i2s_get_txsize() : gr55xx_ll_i2s.h
- ll_i2s_get_type() : gr55xx_ll_i2s.h
- ll_i2s_get_version() : gr55xx_ll_i2s.h
- ll_i2s_get_wss() : gr55xx_ll_i2s.h
- ll_i2s_init() : gr55xx_ll_i2s.h
- ll_i2s_init_t : gr55xx_ll_i2s.h
- LL_I2S_INT_RXDA : gr55xx_ll_i2s.h
- LL_I2S_INT_RXFO : gr55xx_ll_i2s.h
- LL_I2S_INT_TXFE : gr55xx_ll_i2s.h
- LL_I2S_INT_TXFO : gr55xx_ll_i2s.h
- ll_i2s_is_active_it_flag() : gr55xx_ll_i2s.h
- ll_i2s_is_enabled() : gr55xx_ll_i2s.h
- ll_i2s_is_enabled_clock() : gr55xx_ll_i2s.h
- ll_i2s_is_enabled_clock_div() : gr55xx_ll_i2s.h
- ll_i2s_is_enabled_dma() : gr55xx_ll_i2s.h
- ll_i2s_is_enabled_it() : gr55xx_ll_i2s.h
- ll_i2s_is_enabled_rx() : gr55xx_ll_i2s.h
- ll_i2s_is_enabled_rxblock() : gr55xx_ll_i2s.h
- ll_i2s_is_enabled_tx() : gr55xx_ll_i2s.h
- ll_i2s_is_enabled_txblock() : gr55xx_ll_i2s.h
- LL_I2S_ReadReg : gr55xx_ll_i2s.h
- ll_i2s_receive_ldata() : gr55xx_ll_i2s.h
- ll_i2s_receive_rdata() : gr55xx_ll_i2s.h
- LL_I2S_RESOLUTION_12BIT : gr55xx_ll_i2s.h
- LL_I2S_RESOLUTION_16BIT : gr55xx_ll_i2s.h
- LL_I2S_RESOLUTION_20BIT : gr55xx_ll_i2s.h
- LL_I2S_RESOLUTION_24BIT : gr55xx_ll_i2s.h
- LL_I2S_RESOLUTION_32BIT : gr55xx_ll_i2s.h
- ll_i2s_rst_rxdma() : gr55xx_ll_i2s.h
- ll_i2s_rst_txdma() : gr55xx_ll_i2s.h
- LL_I2S_SCLKG_CYCLES_12 : gr55xx_ll_i2s.h
- LL_I2S_SCLKG_CYCLES_16 : gr55xx_ll_i2s.h
- LL_I2S_SCLKG_CYCLES_20 : gr55xx_ll_i2s.h
- LL_I2S_SCLKG_CYCLES_24 : gr55xx_ll_i2s.h
- LL_I2S_SCLKG_NONE : gr55xx_ll_i2s.h
- ll_i2s_set_clock_div() : gr55xx_ll_i2s.h
- ll_i2s_set_clock_src() : gr55xx_ll_i2s.h
- ll_i2s_set_rx_fifo_threshold() : gr55xx_ll_i2s.h
- ll_i2s_set_rxsize() : gr55xx_ll_i2s.h
- ll_i2s_set_sclkg() : gr55xx_ll_i2s.h
- ll_i2s_set_tx_fifo_threshold() : gr55xx_ll_i2s.h
- ll_i2s_set_txsize() : gr55xx_ll_i2s.h
- ll_i2s_set_wss() : gr55xx_ll_i2s.h
- LL_I2S_SIMPLEX_RX : gr55xx_ll_i2s.h
- LL_I2S_SIMPLEX_TX : gr55xx_ll_i2s.h
- LL_I2S_STATUS_RXDA : gr55xx_ll_i2s.h
- LL_I2S_STATUS_RXFO : gr55xx_ll_i2s.h
- LL_I2S_STATUS_TXFE : gr55xx_ll_i2s.h
- LL_I2S_STATUS_TXFO : gr55xx_ll_i2s.h
- ll_i2s_struct_init() : gr55xx_ll_i2s.h
- LL_I2S_THRESHOLD_10FIFO : gr55xx_ll_i2s.h
- LL_I2S_THRESHOLD_11FIFO : gr55xx_ll_i2s.h
- LL_I2S_THRESHOLD_12FIFO : gr55xx_ll_i2s.h
- LL_I2S_THRESHOLD_13FIFO : gr55xx_ll_i2s.h
- LL_I2S_THRESHOLD_14FIFO : gr55xx_ll_i2s.h
- LL_I2S_THRESHOLD_15FIFO : gr55xx_ll_i2s.h
- LL_I2S_THRESHOLD_16FIFO : gr55xx_ll_i2s.h
- LL_I2S_THRESHOLD_1FIFO : gr55xx_ll_i2s.h
- LL_I2S_THRESHOLD_2FIFO : gr55xx_ll_i2s.h
- LL_I2S_THRESHOLD_3FIFO : gr55xx_ll_i2s.h
- LL_I2S_THRESHOLD_4FIFO : gr55xx_ll_i2s.h
- LL_I2S_THRESHOLD_5FIFO : gr55xx_ll_i2s.h
- LL_I2S_THRESHOLD_6FIFO : gr55xx_ll_i2s.h
- LL_I2S_THRESHOLD_7FIFO : gr55xx_ll_i2s.h
- LL_I2S_THRESHOLD_8FIFO : gr55xx_ll_i2s.h
- LL_I2S_THRESHOLD_9FIFO : gr55xx_ll_i2s.h
- ll_i2s_transmit_ldata() : gr55xx_ll_i2s.h
- ll_i2s_transmit_rdata() : gr55xx_ll_i2s.h
- LL_I2S_WriteReg : gr55xx_ll_i2s.h
- LL_I2S_WS_CYCLES_16 : gr55xx_ll_i2s.h
- LL_I2S_WS_CYCLES_24 : gr55xx_ll_i2s.h
- LL_I2S_WS_CYCLES_32 : gr55xx_ll_i2s.h
- LL_ISO7816_ACTION_NONE : gr55xx_ll_iso7816.h
- LL_ISO7816_ACTION_OFF : gr55xx_ll_iso7816.h
- LL_ISO7816_ACTION_ON : gr55xx_ll_iso7816.h
- LL_ISO7816_ACTION_RX : gr55xx_ll_iso7816.h
- LL_ISO7816_ACTION_STOPCLK : gr55xx_ll_iso7816.h
- LL_ISO7816_ACTION_TX : gr55xx_ll_iso7816.h
- LL_ISO7816_ACTION_TXRX : gr55xx_ll_iso7816.h
- LL_ISO7816_ACTION_WARMRST : gr55xx_ll_iso7816.h
- LL_ISO7816_CARD_ABSENT : gr55xx_ll_iso7816.h
- LL_ISO7816_CARD_PRESENT : gr55xx_ll_iso7816.h
- ll_iso7816_check_card_presence() : gr55xx_ll_iso7816.h
- ll_iso7816_clear_flag_all_intr() : gr55xx_ll_iso7816.h
- ll_iso7816_clear_flag_dma_err() : gr55xx_ll_iso7816.h
- ll_iso7816_clear_flag_done() : gr55xx_ll_iso7816.h
- ll_iso7816_clear_flag_presence() : gr55xx_ll_iso7816.h
- ll_iso7816_clear_flag_retry_err() : gr55xx_ll_iso7816.h
- ll_iso7816_clear_flag_rx_err() : gr55xx_ll_iso7816.h
- ll_iso7816_clear_flag_state_err() : gr55xx_ll_iso7816.h
- ll_iso7816_clear_flag_test() : gr55xx_ll_iso7816.h
- ll_iso7816_clear_rx_retry_max() : gr55xx_ll_iso7816.h
- ll_iso7816_clear_tx_retry_max() : gr55xx_ll_iso7816.h
- LL_ISO7816_CLKSTOP_HIGH : gr55xx_ll_iso7816.h
- LL_ISO7816_CLKSTOP_LOW : gr55xx_ll_iso7816.h
- LL_ISO7816_CODING_DEFAULT : gr55xx_ll_iso7816.h
- LL_ISO7816_CODING_INVERSE : gr55xx_ll_iso7816.h
- ll_iso7816_deinit() : gr55xx_ll_iso7816.h
- ll_iso7816_disable_coding_detection() : gr55xx_ll_iso7816.h
- ll_iso7816_enable_coding_detection() : gr55xx_ll_iso7816.h
- ll_iso7816_get_base_addr() : gr55xx_ll_iso7816.h
- ll_iso7816_get_buffer_addr() : gr55xx_ll_iso7816.h
- ll_iso7816_get_clkdiv() : gr55xx_ll_iso7816.h
- ll_iso7816_get_clkstop_level() : gr55xx_ll_iso7816.h
- ll_iso7816_get_coding_convention() : gr55xx_ll_iso7816.h
- ll_iso7816_get_current_addr() : gr55xx_ll_iso7816.h
- ll_iso7816_get_current_addr_frac() : gr55xx_ll_iso7816.h
- ll_iso7816_get_etudiv() : gr55xx_ll_iso7816.h
- ll_iso7816_get_guardtime() : gr55xx_ll_iso7816.h
- ll_iso7816_get_io_states() : gr55xx_ll_iso7816.h
- ll_iso7816_get_it_flag() : gr55xx_ll_iso7816.h
- ll_iso7816_get_power_states() : gr55xx_ll_iso7816.h
- ll_iso7816_get_retry_limit() : gr55xx_ll_iso7816.h
- ll_iso7816_get_rx_end_addr() : gr55xx_ll_iso7816.h
- ll_iso7816_get_rx_end_addr_frac() : gr55xx_ll_iso7816.h
- ll_iso7816_get_rx_endbyte_addr() : gr55xx_ll_iso7816.h
- ll_iso7816_get_rx_retry_max() : gr55xx_ll_iso7816.h
- ll_iso7816_get_start_addr() : gr55xx_ll_iso7816.h
- ll_iso7816_get_tx_end_addr() : gr55xx_ll_iso7816.h
- ll_iso7816_get_tx_end_addr_frac() : gr55xx_ll_iso7816.h
- ll_iso7816_get_tx_endbyte_addr() : gr55xx_ll_iso7816.h
- ll_iso7816_get_tx_retry_max() : gr55xx_ll_iso7816.h
- ll_iso7816_get_waittime() : gr55xx_ll_iso7816.h
- ll_iso7816_init() : gr55xx_ll_iso7816.h
- ll_iso7816_init_t : gr55xx_ll_iso7816.h
- LL_ISO7816_INTR_DMA_ERR : gr55xx_ll_iso7816.h
- LL_ISO7816_INTR_DONE : gr55xx_ll_iso7816.h
- LL_ISO7816_INTR_MASK_ALL : gr55xx_ll_iso7816.h
- LL_ISO7816_INTR_PRESENCE : gr55xx_ll_iso7816.h
- LL_ISO7816_INTR_RETRY_ERR : gr55xx_ll_iso7816.h
- LL_ISO7816_INTR_RX_ERR : gr55xx_ll_iso7816.h
- LL_ISO7816_INTR_STATE_ERR : gr55xx_ll_iso7816.h
- LL_ISO7816_INTR_TEST : gr55xx_ll_iso7816.h
- LL_ISO7816_IO_STATE_IDLE : gr55xx_ll_iso7816.h
- LL_ISO7816_IO_STATE_OFF : gr55xx_ll_iso7816.h
- LL_ISO7816_IO_STATE_RX : gr55xx_ll_iso7816.h
- LL_ISO7816_IO_STATE_RX_WAIT : gr55xx_ll_iso7816.h
- LL_ISO7816_IO_STATE_TX : gr55xx_ll_iso7816.h
- LL_ISO7816_IO_STATE_TX_GUARD : gr55xx_ll_iso7816.h
- ll_iso7816_is_active_flag_dma_err() : gr55xx_ll_iso7816.h
- ll_iso7816_is_active_flag_done() : gr55xx_ll_iso7816.h
- ll_iso7816_is_active_flag_presence() : gr55xx_ll_iso7816.h
- ll_iso7816_is_active_flag_retry_err() : gr55xx_ll_iso7816.h
- ll_iso7816_is_active_flag_rx_err() : gr55xx_ll_iso7816.h
- ll_iso7816_is_active_flag_state_err() : gr55xx_ll_iso7816.h
- ll_iso7816_is_active_flag_test() : gr55xx_ll_iso7816.h
- ll_iso7816_is_busy() : gr55xx_ll_iso7816.h
- LL_ISO7816_PWR_STATE_IDLE : gr55xx_ll_iso7816.h
- LL_ISO7816_PWR_STATE_OFF : gr55xx_ll_iso7816.h
- LL_ISO7816_PWR_STATE_PWRDN_RST : gr55xx_ll_iso7816.h
- LL_ISO7816_PWR_STATE_PWRDN_VCC : gr55xx_ll_iso7816.h
- LL_ISO7816_PWR_STATE_PWRUP_RST : gr55xx_ll_iso7816.h
- LL_ISO7816_PWR_STATE_PWRUP_VCC : gr55xx_ll_iso7816.h
- LL_ISO7816_PWR_STATE_RX : gr55xx_ll_iso7816.h
- LL_ISO7816_PWR_STATE_RX_TS0 : gr55xx_ll_iso7816.h
- LL_ISO7816_PWR_STATE_RX_TS1 : gr55xx_ll_iso7816.h
- LL_ISO7816_PWR_STATE_STOP : gr55xx_ll_iso7816.h
- LL_ISO7816_PWR_STATE_STOP_POST : gr55xx_ll_iso7816.h
- LL_ISO7816_PWR_STATE_STOP_PRE : gr55xx_ll_iso7816.h
- LL_ISO7816_PWR_STATE_TX : gr55xx_ll_iso7816.h
- LL_ISO7816_PWR_STATE_TX_RX : gr55xx_ll_iso7816.h
- LL_ISO7816_ReadReg : gr55xx_ll_iso7816.h
- ll_iso7816_set_action() : gr55xx_ll_iso7816.h
- ll_iso7816_set_base_addr() : gr55xx_ll_iso7816.h
- ll_iso7816_set_buffer_addr() : gr55xx_ll_iso7816.h
- ll_iso7816_set_clkdiv() : gr55xx_ll_iso7816.h
- ll_iso7816_set_clkstop_level() : gr55xx_ll_iso7816.h
- ll_iso7816_set_coding_convention() : gr55xx_ll_iso7816.h
- ll_iso7816_set_etudiv() : gr55xx_ll_iso7816.h
- ll_iso7816_set_guardtime() : gr55xx_ll_iso7816.h
- ll_iso7816_set_retry_limit() : gr55xx_ll_iso7816.h
- ll_iso7816_set_rx_end_addr() : gr55xx_ll_iso7816.h
- ll_iso7816_set_rx_end_addr_frac() : gr55xx_ll_iso7816.h
- ll_iso7816_set_rx_endbyte_addr() : gr55xx_ll_iso7816.h
- ll_iso7816_set_start_addr() : gr55xx_ll_iso7816.h
- ll_iso7816_set_tx_end_addr() : gr55xx_ll_iso7816.h
- ll_iso7816_set_tx_end_addr_frac() : gr55xx_ll_iso7816.h
- ll_iso7816_set_tx_endbyte_addr() : gr55xx_ll_iso7816.h
- ll_iso7816_set_waittime() : gr55xx_ll_iso7816.h
- LL_ISO7816_WriteReg : gr55xx_ll_iso7816.h
- LL_MSIO_DEFAULT_CONFIG : gr55xx_ll_msio.h
- ll_msio_deinit() : gr55xx_ll_msio.h
- LL_MSIO_DIRECTION_INOUT : gr55xx_ll_msio.h
- LL_MSIO_DIRECTION_INPUT : gr55xx_ll_msio.h
- LL_MSIO_DIRECTION_NONE : gr55xx_ll_msio.h
- LL_MSIO_DIRECTION_OUTPUT : gr55xx_ll_msio.h
- ll_msio_get_pin_direction() : gr55xx_ll_msio.h
- ll_msio_get_pin_mode() : gr55xx_ll_msio.h
- ll_msio_get_pin_mux() : gr55xx_ll_msio.h
- ll_msio_get_pin_pull() : gr55xx_ll_msio.h
- ll_msio_init() : gr55xx_ll_msio.h
- ll_msio_init_t : gr55xx_ll_msio.h
- ll_msio_is_input_pin_set() : gr55xx_ll_msio.h
- ll_msio_is_output_pin_set() : gr55xx_ll_msio.h
- LL_MSIO_MODE_ANALOG : gr55xx_ll_msio.h
- LL_MSIO_MODE_DIGITAL : gr55xx_ll_msio.h
- LL_MSIO_MUX_0 : gr55xx_ll_msio.h
- LL_MSIO_MUX_1 : gr55xx_ll_msio.h
- LL_MSIO_MUX_2 : gr55xx_ll_msio.h
- LL_MSIO_MUX_3 : gr55xx_ll_msio.h
- LL_MSIO_MUX_4 : gr55xx_ll_msio.h
- LL_MSIO_MUX_5 : gr55xx_ll_msio.h
- LL_MSIO_MUX_6 : gr55xx_ll_msio.h
- LL_MSIO_MUX_7 : gr55xx_ll_msio.h
- LL_MSIO_PIN_0 : gr55xx_ll_msio.h
- LL_MSIO_PIN_1 : gr55xx_ll_msio.h
- LL_MSIO_PIN_2 : gr55xx_ll_msio.h
- LL_MSIO_PIN_3 : gr55xx_ll_msio.h
- LL_MSIO_PIN_4 : gr55xx_ll_msio.h
- LL_MSIO_PIN_ALL : gr55xx_ll_msio.h
- LL_MSIO_PULL_DOWN : gr55xx_ll_msio.h
- LL_MSIO_PULL_NO : gr55xx_ll_msio.h
- LL_MSIO_PULL_UP : gr55xx_ll_msio.h
- ll_msio_read_input_port() : gr55xx_ll_msio.h
- ll_msio_read_output_port() : gr55xx_ll_msio.h
- LL_MSIO_ReadReg : gr55xx_ll_msio.h
- ll_msio_reset_output_pin() : gr55xx_ll_msio.h
- ll_msio_set_output_pin() : gr55xx_ll_msio.h
- ll_msio_set_pin_direction() : gr55xx_ll_msio.h
- ll_msio_set_pin_mode() : gr55xx_ll_msio.h
- ll_msio_set_pin_mux() : gr55xx_ll_msio.h
- ll_msio_set_pin_pull() : gr55xx_ll_msio.h
- ll_msio_struct_init() : gr55xx_ll_msio.h
- ll_msio_toggle_pin() : gr55xx_ll_msio.h
- ll_msio_write_output_port() : gr55xx_ll_msio.h
- LL_MSIO_WriteReg : gr55xx_ll_msio.h
- LL_PKC_BIGMULTI_BITS_LENGTH_MAX : gr55xx_ll_pkc.h
- LL_PKC_BITS_LENGTH_MAX : gr55xx_ll_pkc.h
- LL_PKC_BITS_LENGTH_MIN : gr55xx_ll_pkc.h
- ll_pkc_clear_flag_it_big_add_overflow() : gr55xx_ll_pkc.h
- ll_pkc_clear_flag_it_done() : gr55xx_ll_pkc.h
- ll_pkc_clear_flag_it_err() : gr55xx_ll_pkc.h
- ll_pkc_deinit() : gr55xx_ll_pkc.h
- ll_pkc_disable() : gr55xx_ll_pkc.h
- ll_pkc_disable_dummy_multi() : gr55xx_ll_pkc.h
- ll_pkc_disable_hardware_start() : gr55xx_ll_pkc.h
- ll_pkc_disable_it_big_add_overflow() : gr55xx_ll_pkc.h
- ll_pkc_disable_it_done() : gr55xx_ll_pkc.h
- ll_pkc_disable_it_err() : gr55xx_ll_pkc.h
- ll_pkc_disable_random_clock_gating() : gr55xx_ll_pkc.h
- ll_pkc_disable_reset() : gr55xx_ll_pkc.h
- ll_pkc_disable_software() : gr55xx_ll_pkc.h
- ll_pkc_disable_software_start() : gr55xx_ll_pkc.h
- ll_pkc_enable() : gr55xx_ll_pkc.h
- ll_pkc_enable_dummy_multi() : gr55xx_ll_pkc.h
- ll_pkc_enable_hardware_start() : gr55xx_ll_pkc.h
- ll_pkc_enable_it_big_add_overflow() : gr55xx_ll_pkc.h
- ll_pkc_enable_it_done() : gr55xx_ll_pkc.h
- ll_pkc_enable_it_err() : gr55xx_ll_pkc.h
- ll_pkc_enable_random_clock_gating() : gr55xx_ll_pkc.h
- ll_pkc_enable_reset() : gr55xx_ll_pkc.h
- ll_pkc_enable_software() : gr55xx_ll_pkc.h
- ll_pkc_enable_software_start() : gr55xx_ll_pkc.h
- ll_pkc_get_ba_a_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_ba_b_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_ba_c_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_bm_a_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_bm_b_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_bm_c_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_constant1_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_constp() : gr55xx_ll_pkc.h
- ll_pkc_get_dummy_multiply_seed() : gr55xx_ll_pkc.h
- ll_pkc_get_ecc_a_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_ecc_b_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_gx_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_gy_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_gz_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_k_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_mas_a_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_mas_b_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_mas_c_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_mas_p_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_mi_u_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_mi_v_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_mi_x1_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_mi_x2_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_mik_output() : gr55xx_ll_pkc.h
- ll_pkc_get_mitmp_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_mm_a_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_mm_b_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_mm_c_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_mm_p_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_operation_mode() : gr55xx_ll_pkc.h
- ll_pkc_get_operation_word_length() : gr55xx_ll_pkc.h
- ll_pkc_get_p_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_r0x_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_r0y_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_r0z_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_r1x_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_r1y_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_r1z_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_r_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_random_clock_gating_seed() : gr55xx_ll_pkc.h
- ll_pkc_get_rsq_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_swmi_tmp_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_tmp1_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_tmp2_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_tmp3_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_tmp4_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_tmp5_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_tmp6_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_tmpk_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_x1_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_x2_pointer() : gr55xx_ll_pkc.h
- ll_pkc_init() : gr55xx_ll_pkc.h
- ll_pkc_init_t : gr55xx_ll_pkc.h
- LL_PKC_INTEN_BAOVF : gr55xx_ll_pkc.h
- LL_PKC_INTEN_DONE : gr55xx_ll_pkc.h
- LL_PKC_INTEN_ERR : gr55xx_ll_pkc.h
- ll_pkc_is_action_flag_busy() : gr55xx_ll_pkc.h
- ll_pkc_is_action_flag_it_big_add_overflow() : gr55xx_ll_pkc.h
- ll_pkc_is_action_flag_it_done() : gr55xx_ll_pkc.h
- ll_pkc_is_action_flag_it_err() : gr55xx_ll_pkc.h
- ll_pkc_is_enable_it_big_add_overflow() : gr55xx_ll_pkc.h
- ll_pkc_is_enable_it_done() : gr55xx_ll_pkc.h
- ll_pkc_is_enable_it_err() : gr55xx_ll_pkc.h
- ll_pkc_is_enabled() : gr55xx_ll_pkc.h
- ll_pkc_is_enabled_dummy_multi() : gr55xx_ll_pkc.h
- ll_pkc_is_enabled_hardware_start() : gr55xx_ll_pkc.h
- ll_pkc_is_enabled_random_clock_gating() : gr55xx_ll_pkc.h
- ll_pkc_is_enabled_reset() : gr55xx_ll_pkc.h
- ll_pkc_is_enabled_software() : gr55xx_ll_pkc.h
- ll_pkc_is_enabled_software_start() : gr55xx_ll_pkc.h
- LL_PKC_operation_mode_ADD : gr55xx_ll_pkc.h
- LL_PKC_operation_mode_BIGINTEGERADD : gr55xx_ll_pkc.h
- LL_PKC_operation_mode_BIGINTEGERMULTIPLY : gr55xx_ll_pkc.h
- LL_PKC_operation_mode_COMPARE : gr55xx_ll_pkc.h
- LL_PKC_operation_mode_INVERTION : gr55xx_ll_pkc.h
- LL_PKC_operation_mode_LEFTSHIFT : gr55xx_ll_pkc.h
- LL_PKC_operation_mode_MULTIPLY : gr55xx_ll_pkc.h
- LL_PKC_operation_mode_SUB : gr55xx_ll_pkc.h
- LL_PKC_ReadReg : gr55xx_ll_pkc.h
- ll_pkc_set_ba_a_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_ba_b_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_ba_c_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_bm_a_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_bm_b_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_bm_c_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_constant1_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_constp() : gr55xx_ll_pkc.h
- ll_pkc_set_dummy_multiply_seed() : gr55xx_ll_pkc.h
- ll_pkc_set_ecc_a_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_ecc_b_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_gx_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_gy_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_gz_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_k_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_mas_a_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_mas_b_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_mas_c_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_mas_p_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_mi_u_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_mi_v_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_mi_x1_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_mi_x2_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_mitmp_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_mm_a_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_mm_b_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_mm_c_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_mm_p_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_operation_mode() : gr55xx_ll_pkc.h
- ll_pkc_set_operation_word_length() : gr55xx_ll_pkc.h
- ll_pkc_set_p_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_r0x_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_r0y_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_r0z_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_r1x_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_r1y_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_r1z_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_r_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_random_clock_gating_seed() : gr55xx_ll_pkc.h
- ll_pkc_set_rsq_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_swmi_tmp_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_tmp1_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_tmp2_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_tmp3_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_tmp4_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_tmp5_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_tmp6_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_tmpk_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_x1_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_x2_pointer() : gr55xx_ll_pkc.h
- ll_pkc_struct_init() : gr55xx_ll_pkc.h
- LL_PKC_WORKSTAT_BUSY : gr55xx_ll_pkc.h
- LL_PKC_WriteReg : gr55xx_ll_pkc.h
- LL_PWM_ACTIONEVENT_CLEAR : gr55xx_ll_pwm.h
- LL_PWM_ACTIONEVENT_NONE : gr55xx_ll_pwm.h
- LL_PWM_ACTIONEVENT_SET : gr55xx_ll_pwm.h
- LL_PWM_ACTIONEVENT_TOGGLE : gr55xx_ll_pwm.h
- LL_PWM_BREATH_MODE : gr55xx_ll_pwm.h
- LL_PWM_BREATH_PRESCALER_UNIT : gr55xx_ll_pwm.h
- LL_PWM_CENTER_ALIGNED : gr55xx_ll_pwm.h
- LL_PWM_CHANNEL_DEFAULT_CONFIG : gr55xx_ll_pwm.h
- ll_pwm_channel_init_t : gr55xx_ll_pwm.h
- LL_PWM_DEFAULT_CONFIG : gr55xx_ll_pwm.h
- ll_pwm_deinit() : gr55xx_ll_pwm.h
- ll_pwm_disable() : gr55xx_ll_pwm.h
- ll_pwm_disable_pause() : gr55xx_ll_pwm.h
- ll_pwm_disable_positive_drive_channel_a() : gr55xx_ll_pwm.h
- ll_pwm_disable_positive_drive_channel_b() : gr55xx_ll_pwm.h
- ll_pwm_disable_positive_drive_channel_c() : gr55xx_ll_pwm.h
- ll_pwm_disable_update_active_event() : gr55xx_ll_pwm.h
- ll_pwm_disable_update_all() : gr55xx_ll_pwm.h
- ll_pwm_disable_update_breath_period() : gr55xx_ll_pwm.h
- ll_pwm_disable_update_compare_a0() : gr55xx_ll_pwm.h
- ll_pwm_disable_update_compare_a1() : gr55xx_ll_pwm.h
- ll_pwm_disable_update_compare_b0() : gr55xx_ll_pwm.h
- ll_pwm_disable_update_compare_b1() : gr55xx_ll_pwm.h
- ll_pwm_disable_update_compare_c0() : gr55xx_ll_pwm.h
- ll_pwm_disable_update_compare_c1() : gr55xx_ll_pwm.h
- ll_pwm_disable_update_hold_period() : gr55xx_ll_pwm.h
- ll_pwm_disable_update_pause() : gr55xx_ll_pwm.h
- ll_pwm_disable_update_period() : gr55xx_ll_pwm.h
- LL_PWM_DRIVEPOLARITY_NEGATIVE : gr55xx_ll_pwm.h
- LL_PWM_DRIVEPOLARITY_POSITIVE : gr55xx_ll_pwm.h
- LL_PWM_EDGE_ALIGNED : gr55xx_ll_pwm.h
- ll_pwm_enable() : gr55xx_ll_pwm.h
- ll_pwm_enable_pause() : gr55xx_ll_pwm.h
- ll_pwm_enable_positive_drive_channel_a() : gr55xx_ll_pwm.h
- ll_pwm_enable_positive_drive_channel_b() : gr55xx_ll_pwm.h
- ll_pwm_enable_positive_drive_channel_c() : gr55xx_ll_pwm.h
- ll_pwm_enable_update_active_event() : gr55xx_ll_pwm.h
- ll_pwm_enable_update_all() : gr55xx_ll_pwm.h
- ll_pwm_enable_update_breath_period() : gr55xx_ll_pwm.h
- ll_pwm_enable_update_compare_a0() : gr55xx_ll_pwm.h
- ll_pwm_enable_update_compare_a1() : gr55xx_ll_pwm.h
- ll_pwm_enable_update_compare_b0() : gr55xx_ll_pwm.h
- ll_pwm_enable_update_compare_b1() : gr55xx_ll_pwm.h
- ll_pwm_enable_update_compare_c0() : gr55xx_ll_pwm.h
- ll_pwm_enable_update_compare_c1() : gr55xx_ll_pwm.h
- ll_pwm_enable_update_hold_period() : gr55xx_ll_pwm.h
- ll_pwm_enable_update_pause() : gr55xx_ll_pwm.h
- ll_pwm_enable_update_period() : gr55xx_ll_pwm.h
- LL_PWM_FLICKER_MODE : gr55xx_ll_pwm.h
- ll_pwm_get_action_event_cmp_a0() : gr55xx_ll_pwm.h
- ll_pwm_get_action_event_cmp_a1() : gr55xx_ll_pwm.h
- ll_pwm_get_action_event_cmp_b0() : gr55xx_ll_pwm.h
- ll_pwm_get_action_event_cmp_b1() : gr55xx_ll_pwm.h
- ll_pwm_get_action_event_cmp_c0() : gr55xx_ll_pwm.h
- ll_pwm_get_action_event_cmp_c1() : gr55xx_ll_pwm.h
- ll_pwm_get_breath_prescaler() : gr55xx_ll_pwm.h
- ll_pwm_get_compare_a0() : gr55xx_ll_pwm.h
- ll_pwm_get_compare_a1() : gr55xx_ll_pwm.h
- ll_pwm_get_compare_b0() : gr55xx_ll_pwm.h
- ll_pwm_get_compare_b1() : gr55xx_ll_pwm.h
- ll_pwm_get_compare_c0() : gr55xx_ll_pwm.h
- ll_pwm_get_compare_c1() : gr55xx_ll_pwm.h
- ll_pwm_get_hold_prescaler() : gr55xx_ll_pwm.h
- ll_pwm_get_mode() : gr55xx_ll_pwm.h
- ll_pwm_get_prescaler() : gr55xx_ll_pwm.h
- LL_PWM_HOLD_PRESCALER_UNIT : gr55xx_ll_pwm.h
- ll_pwm_init() : gr55xx_ll_pwm.h
- ll_pwm_init_t : gr55xx_ll_pwm.h
- ll_pwm_is_active_flag_update_all() : gr55xx_ll_pwm.h
- ll_pwm_is_enabled() : gr55xx_ll_pwm.h
- ll_pwm_is_enabled_pause() : gr55xx_ll_pwm.h
- ll_pwm_is_enabled_positive_drive_channel_a() : gr55xx_ll_pwm.h
- ll_pwm_is_enabled_positive_drive_channel_b() : gr55xx_ll_pwm.h
- ll_pwm_is_enabled_positive_drive_channel_c() : gr55xx_ll_pwm.h
- ll_pwm_is_enabled_update_active_event() : gr55xx_ll_pwm.h
- ll_pwm_is_enabled_update_all() : gr55xx_ll_pwm.h
- ll_pwm_is_enabled_update_breath_period() : gr55xx_ll_pwm.h
- ll_pwm_is_enabled_update_compare_a0() : gr55xx_ll_pwm.h
- ll_pwm_is_enabled_update_compare_a1() : gr55xx_ll_pwm.h
- ll_pwm_is_enabled_update_compare_b0() : gr55xx_ll_pwm.h
- ll_pwm_is_enabled_update_compare_b1() : gr55xx_ll_pwm.h
- ll_pwm_is_enabled_update_compare_c0() : gr55xx_ll_pwm.h
- ll_pwm_is_enabled_update_compare_c1() : gr55xx_ll_pwm.h
- ll_pwm_is_enabled_update_hold_period() : gr55xx_ll_pwm.h
- ll_pwm_is_enabled_update_pause() : gr55xx_ll_pwm.h
- ll_pwm_is_enabled_update_period() : gr55xx_ll_pwm.h
- LL_PWM_PRESCALER_UNIT : gr55xx_ll_pwm.h
- LL_PWM_ReadReg : gr55xx_ll_pwm.h
- ll_pwm_set_action_event_cmp_a0() : gr55xx_ll_pwm.h
- ll_pwm_set_action_event_cmp_a1() : gr55xx_ll_pwm.h
- ll_pwm_set_action_event_cmp_b0() : gr55xx_ll_pwm.h
- ll_pwm_set_action_event_cmp_b1() : gr55xx_ll_pwm.h
- ll_pwm_set_action_event_cmp_c0() : gr55xx_ll_pwm.h
- ll_pwm_set_action_event_cmp_c1() : gr55xx_ll_pwm.h
- ll_pwm_set_breath_prescaler() : gr55xx_ll_pwm.h
- ll_pwm_set_compare_a0() : gr55xx_ll_pwm.h
- ll_pwm_set_compare_a1() : gr55xx_ll_pwm.h
- ll_pwm_set_compare_b0() : gr55xx_ll_pwm.h
- ll_pwm_set_compare_b1() : gr55xx_ll_pwm.h
- ll_pwm_set_compare_c0() : gr55xx_ll_pwm.h
- ll_pwm_set_compare_c1() : gr55xx_ll_pwm.h
- ll_pwm_set_hold_prescaler() : gr55xx_ll_pwm.h
- ll_pwm_set_mode() : gr55xx_ll_pwm.h
- ll_pwm_set_prescaler() : gr55xx_ll_pwm.h
- ll_pwm_struct_init() : gr55xx_ll_pwm.h
- LL_PWM_WriteReg : gr55xx_ll_pwm.h
- ll_pwr_clear_ext_wakeup_status() : gr55xx_ll_pwr.h
- ll_pwr_clear_wakeup_event() : gr55xx_ll_pwr.h
- LL_PWR_CMD_32_TIMER_LD : gr55xx_ll_pwr.h
- LL_PWR_CMD_DEEP_SLEEP : gr55xx_ll_pwr.h
- LL_PWR_CMD_DPAD_LE_HI : gr55xx_ll_pwr.h
- LL_PWR_CMD_DPAD_LE_LO : gr55xx_ll_pwr.h
- LL_PWR_CMD_EF_DIR_OFF : gr55xx_ll_pwr.h
- LL_PWR_CMD_EF_DIR_ON : gr55xx_ll_pwr.h
- LL_PWR_CMD_EXT_CLK : gr55xx_ll_pwr.h
- LL_PWR_CMD_LD_MEM_SLP_CFG : gr55xx_ll_pwr.h
- LL_PWR_CMD_LD_MEM_WKUP_CFG : gr55xx_ll_pwr.h
- LL_PWR_CMD_LOOPBACK : gr55xx_ll_pwr.h
- LL_PWR_CMD_RNG2_CLK : gr55xx_ll_pwr.h
- LL_PWR_CMD_RNG_CLK : gr55xx_ll_pwr.h
- LL_PWR_CMD_RTC_CLK : gr55xx_ll_pwr.h
- LL_PWR_CMD_SLP_TIMER_MODE_DISABLE : gr55xx_ll_pwr.h
- LL_PWR_CMD_SLP_TIMER_MODE_NORMAL : gr55xx_ll_pwr.h
- LL_PWR_CMD_SLP_TIMER_MODE_RELOAD : gr55xx_ll_pwr.h
- LL_PWR_CMD_SLP_TIMER_MODE_SINGLE : gr55xx_ll_pwr.h
- ll_pwr_disable_cache_module() : gr55xx_ll_pwr.h
- ll_pwr_disable_comm_core_deep_sleep() : gr55xx_ll_pwr.h
- ll_pwr_disable_comm_core_ext_wakeup() : gr55xx_ll_pwr.h
- ll_pwr_disable_comm_core_power() : gr55xx_ll_pwr.h
- ll_pwr_disable_comm_core_reset() : gr55xx_ll_pwr.h
- ll_pwr_disable_comm_timer_power() : gr55xx_ll_pwr.h
- ll_pwr_disable_comm_timer_reset() : gr55xx_ll_pwr.h
- ll_pwr_disable_ext_wakeup_pin() : gr55xx_ll_pwr.h
- ll_pwr_disable_osc_sleep() : gr55xx_ll_pwr.h
- ll_pwr_disable_radio_sleep() : gr55xx_ll_pwr.h
- ll_pwr_disable_smc_wakeup_req() : gr55xx_ll_pwr.h
- LL_PWR_DPAD_LE_OFF : gr55xx_ll_pwr.h
- LL_PWR_DPAD_LE_ON : gr55xx_ll_pwr.h
- ll_pwr_enable_comm_core_deep_sleep() : gr55xx_ll_pwr.h
- ll_pwr_enable_comm_core_ext_wakeup() : gr55xx_ll_pwr.h
- ll_pwr_enable_comm_core_power() : gr55xx_ll_pwr.h
- ll_pwr_enable_comm_core_reset() : gr55xx_ll_pwr.h
- ll_pwr_enable_comm_soft_wakeup_req() : gr55xx_ll_pwr.h
- ll_pwr_enable_comm_timer_power() : gr55xx_ll_pwr.h
- ll_pwr_enable_comm_timer_reset() : gr55xx_ll_pwr.h
- ll_pwr_enable_ext_wakeup_pin() : gr55xx_ll_pwr.h
- ll_pwr_enable_osc_sleep() : gr55xx_ll_pwr.h
- ll_pwr_enable_radio_sleep() : gr55xx_ll_pwr.h
- ll_pwr_enable_smc_wakeup_req() : gr55xx_ll_pwr.h
- LL_PWR_EXTWKUP_INVERT_LSB : gr55xx_ll_pwr.h
- LL_PWR_EXTWKUP_PIN0 : gr55xx_ll_pwr.h
- LL_PWR_EXTWKUP_PIN1 : gr55xx_ll_pwr.h
- LL_PWR_EXTWKUP_PIN2 : gr55xx_ll_pwr.h
- LL_PWR_EXTWKUP_PIN3 : gr55xx_ll_pwr.h
- LL_PWR_EXTWKUP_PIN4 : gr55xx_ll_pwr.h
- LL_PWR_EXTWKUP_PIN5 : gr55xx_ll_pwr.h
- LL_PWR_EXTWKUP_PIN6 : gr55xx_ll_pwr.h
- LL_PWR_EXTWKUP_PIN7 : gr55xx_ll_pwr.h
- LL_PWR_EXTWKUP_PIN_ALL : gr55xx_ll_pwr.h
- LL_PWR_EXTWKUP_SRC_EN_LSB : gr55xx_ll_pwr.h
- LL_PWR_EXTWKUP_TYPE_FALLING : gr55xx_ll_pwr.h
- LL_PWR_EXTWKUP_TYPE_HIGH : gr55xx_ll_pwr.h
- LL_PWR_EXTWKUP_TYPE_LOW : gr55xx_ll_pwr.h
- LL_PWR_EXTWKUP_TYPE_LSB : gr55xx_ll_pwr.h
- LL_PWR_EXTWKUP_TYPE_RISING : gr55xx_ll_pwr.h
- ll_pwr_get_comm_sleep_duration() : gr55xx_ll_pwr.h
- ll_pwr_get_comm_wakeup_time() : gr55xx_ll_pwr.h
- ll_pwr_get_ext_wakeup_status() : gr55xx_ll_pwr.h
- ll_pwr_get_ext_wakeup_type() : gr55xx_ll_pwr.h
- ll_pwr_get_sleep_timer_value() : gr55xx_ll_pwr.h
- ll_pwr_get_timer_read_select() : gr55xx_ll_pwr.h
- ll_pwr_get_timer_read_value() : gr55xx_ll_pwr.h
- ll_pwr_get_wakeup_condition() : gr55xx_ll_pwr.h
- ll_pwr_get_wakeup_event() : gr55xx_ll_pwr.h
- ll_pwr_is_active_flag_comm_deep_sleep_stat() : gr55xx_ll_pwr.h
- ll_pwr_is_active_flag_psc_cmd_busy() : gr55xx_ll_pwr.h
- ll_pwr_is_enabled_comm_core_deep_sleep() : gr55xx_ll_pwr.h
- ll_pwr_is_enabled_comm_core_ext_wakeup() : gr55xx_ll_pwr.h
- ll_pwr_is_enabled_comm_core_power() : gr55xx_ll_pwr.h
- ll_pwr_is_enabled_comm_core_reset() : gr55xx_ll_pwr.h
- ll_pwr_is_enabled_comm_timer_power() : gr55xx_ll_pwr.h
- ll_pwr_is_enabled_comm_timer_reset() : gr55xx_ll_pwr.h
- ll_pwr_is_enabled_ext_wakeup_pin() : gr55xx_ll_pwr.h
- ll_pwr_is_enabled_osc_sleep() : gr55xx_ll_pwr.h
- ll_pwr_is_enabled_radio_sleep() : gr55xx_ll_pwr.h
- ll_pwr_is_enabled_smc_wakeup_req() : gr55xx_ll_pwr.h
- ll_pwr_is_enabled_soft_wakeup_req() : gr55xx_ll_pwr.h
- ll_pwr_read_comm_wakeup_timing() : gr55xx_ll_pwr.h
- ll_pwr_read_comm_wakeup_timing_twosc() : gr55xx_ll_pwr.h
- LL_PWR_ReadReg : gr55xx_ll_pwr.h
- ll_pwr_req_excute_psc_command() : gr55xx_ll_pwr.h
- ll_pwr_set_comm_core_wakeup_time() : gr55xx_ll_pwr.h
- ll_pwr_set_comm_wakeup_timing() : gr55xx_ll_pwr.h
- ll_pwr_set_dpad_le_value() : gr55xx_ll_pwr.h
- ll_pwr_set_ext_wakeup_type() : gr55xx_ll_pwr.h
- ll_pwr_set_sleep_timer_value() : gr55xx_ll_pwr.h
- ll_pwr_set_timer_read_select() : gr55xx_ll_pwr.h
- ll_pwr_set_wakeup_condition() : gr55xx_ll_pwr.h
- LL_PWR_TIMER_READ_SEL_AON_WDT : gr55xx_ll_pwr.h
- LL_PWR_TIMER_READ_SEL_CAL_ALARM : gr55xx_ll_pwr.h
- LL_PWR_TIMER_READ_SEL_CAL_TIMER : gr55xx_ll_pwr.h
- LL_PWR_TIMER_READ_SEL_SLP_TIMER : gr55xx_ll_pwr.h
- LL_PWR_WKUP_COND_ALL : gr55xx_ll_pwr.h
- LL_PWR_WKUP_COND_BLE : gr55xx_ll_pwr.h
- LL_PWR_WKUP_COND_BOD_FEDGE : gr55xx_ll_pwr.h
- LL_PWR_WKUP_COND_CALENDAR : gr55xx_ll_pwr.h
- LL_PWR_WKUP_COND_EXT : gr55xx_ll_pwr.h
- LL_PWR_WKUP_COND_MSIO_COMP : gr55xx_ll_pwr.h
- LL_PWR_WKUP_COND_TIMER : gr55xx_ll_pwr.h
- LL_PWR_WKUP_EVENT_ALL : gr55xx_ll_pwr.h
- LL_PWR_WKUP_EVENT_BLE : gr55xx_ll_pwr.h
- LL_PWR_WKUP_EVENT_BOD_FEDGE : gr55xx_ll_pwr.h
- LL_PWR_WKUP_EVENT_CALENDAR : gr55xx_ll_pwr.h
- LL_PWR_WKUP_EVENT_EXT : gr55xx_ll_pwr.h
- LL_PWR_WKUP_EVENT_MSIO_COMP : gr55xx_ll_pwr.h
- LL_PWR_WKUP_EVENT_TIMER : gr55xx_ll_pwr.h
- LL_PWR_WKUP_EVENT_WDT : gr55xx_ll_pwr.h
- LL_PWR_WriteReg : gr55xx_ll_pwr.h
- LL_QSPI_DEFAULT_CONFIG : gr55xx_ll_spi.h
- ll_qspi_deinit() : gr55xx_ll_spi.h
- ll_qspi_init() : gr55xx_ll_spi.h
- ll_qspi_init_t : gr55xx_ll_spi.h
- ll_qspi_struct_init() : gr55xx_ll_spi.h
- ll_rng_clear_flag_sts() : gr55xx_ll_rng.h
- ll_rng_deinit() : gr55xx_ll_rng.h
- ll_rng_disable() : gr55xx_ll_rng.h
- ll_rng_disable_fro() : gr55xx_ll_rng.h
- ll_rng_disable_it() : gr55xx_ll_rng.h
- ll_rng_enable() : gr55xx_ll_rng.h
- ll_rng_enable_fro() : gr55xx_ll_rng.h
- ll_rng_enable_it() : gr55xx_ll_rng.h
- ll_rng_fro_is_enabled() : gr55xx_ll_rng.h
- ll_rng_get_lfsr_mode() : gr55xx_ll_rng.h
- ll_rng_get_lfsr_seed() : gr55xx_ll_rng.h
- ll_rng_get_output_mode() : gr55xx_ll_rng.h
- ll_rng_get_post_mode() : gr55xx_ll_rng.h
- ll_rng_get_trdy_time() : gr55xx_ll_rng.h
- ll_rng_init() : gr55xx_ll_rng.h
- ll_rng_init_t : gr55xx_ll_rng.h
- ll_rng_is_active_flag_lr() : gr55xx_ll_rng.h
- ll_rng_is_active_flag_sts() : gr55xx_ll_rng.h
- ll_rng_is_enabled() : gr55xx_ll_rng.h
- ll_rng_is_enabled_it() : gr55xx_ll_rng.h
- LL_RNG_IT_DISABLE : gr55xx_ll_rng.h
- LL_RNG_IT_ENABLE : gr55xx_ll_rng.h
- LL_RNG_LFSR_MODE_128BIT : gr55xx_ll_rng.h
- LL_RNG_LFSR_MODE_59BIT : gr55xx_ll_rng.h
- LL_RNG_OUTPUT_CYCLIC : gr55xx_ll_rng.h
- LL_RNG_OUTPUT_CYCLIC_PARITY : gr55xx_ll_rng.h
- LL_RNG_OUTPUT_FR0_S0 : gr55xx_ll_rng.h
- LL_RNG_OUTPUT_LFSR : gr55xx_ll_rng.h
- LL_RNG_OUTPUT_LFSR_RNG : gr55xx_ll_rng.h
- LL_RNG_POST_PRO_COUNTING : gr55xx_ll_rng.h
- LL_RNG_POST_PRO_NEUMANN : gr55xx_ll_rng.h
- LL_RNG_POST_PRO_NOT : gr55xx_ll_rng.h
- LL_RNG_POST_PRO_SKIPPING : gr55xx_ll_rng.h
- ll_rng_read_lr_count() : gr55xx_ll_rng.h
- ll_rng_read_random_data32() : gr55xx_ll_rng.h
- LL_RNG_ReadReg : gr55xx_ll_rng.h
- LL_RNG_SEED_FR0_S0 : gr55xx_ll_rng.h
- LL_RNG_SEED_USER : gr55xx_ll_rng.h
- ll_rng_set_lfsr_mode() : gr55xx_ll_rng.h
- ll_rng_set_lfsr_seed() : gr55xx_ll_rng.h
- ll_rng_set_output_mode() : gr55xx_ll_rng.h
- ll_rng_set_post_mode() : gr55xx_ll_rng.h
- ll_rng_set_trdy_time() : gr55xx_ll_rng.h
- ll_rng_set_user_seed() : gr55xx_ll_rng.h
- ll_rng_struct_init() : gr55xx_ll_rng.h
- LL_RNG_WriteReg : gr55xx_ll_rng.h
- ll_spi_clear_flag_all() : gr55xx_ll_spi.h
- ll_spi_clear_flag_mst() : gr55xx_ll_spi.h
- ll_spi_clear_flag_rxo() : gr55xx_ll_spi.h
- ll_spi_clear_flag_rxu() : gr55xx_ll_spi.h
- ll_spi_clear_flag_txo() : gr55xx_ll_spi.h
- ll_spi_disable() : gr55xx_ll_spi.h
- ll_spi_disable_dma_req_rx() : gr55xx_ll_spi.h
- ll_spi_disable_dma_req_tx() : gr55xx_ll_spi.h
- ll_spi_disable_it() : gr55xx_ll_spi.h
- ll_spi_disable_micro_handshake() : gr55xx_ll_spi.h
- ll_spi_disable_salve_out() : gr55xx_ll_spi.h
- ll_spi_disable_ss() : gr55xx_ll_spi.h
- ll_spi_disable_ss_toggle() : gr55xx_ll_spi.h
- ll_spi_disable_test_mode() : gr55xx_ll_spi.h
- ll_spi_enable() : gr55xx_ll_spi.h
- ll_spi_enable_dma_req_rx() : gr55xx_ll_spi.h
- ll_spi_enable_dma_req_tx() : gr55xx_ll_spi.h
- ll_spi_enable_it() : gr55xx_ll_spi.h
- ll_spi_enable_micro_handshake() : gr55xx_ll_spi.h
- ll_spi_enable_slave_out() : gr55xx_ll_spi.h
- ll_spi_enable_ss() : gr55xx_ll_spi.h
- ll_spi_enable_ss_toggle() : gr55xx_ll_spi.h
- ll_spi_enable_test_mode() : gr55xx_ll_spi.h
- ll_spi_get_addr_inst_transfer_format() : gr55xx_ll_spi.h
- ll_spi_get_address_size() : gr55xx_ll_spi.h
- ll_spi_get_baud_rate_prescaler() : gr55xx_ll_spi.h
- ll_spi_get_clock_phase() : gr55xx_ll_spi.h
- ll_spi_get_clock_polarity() : gr55xx_ll_spi.h
- ll_spi_get_control_frame_size() : gr55xx_ll_spi.h
- ll_spi_get_data_size() : gr55xx_ll_spi.h
- ll_spi_get_dma_rx_fifo_threshold() : gr55xx_ll_spi.h
- ll_spi_get_dma_tx_fifo_threshold() : gr55xx_ll_spi.h
- ll_spi_get_frame_format() : gr55xx_ll_spi.h
- ll_spi_get_id_code() : gr55xx_ll_spi.h
- ll_spi_get_instruction_size() : gr55xx_ll_spi.h
- ll_spi_get_it_flag() : gr55xx_ll_spi.h
- ll_spi_get_micro_transfer_direction() : gr55xx_ll_spi.h
- ll_spi_get_micro_transfer_mode() : gr55xx_ll_spi.h
- ll_spi_get_raw_if_flag() : gr55xx_ll_spi.h
- ll_spi_get_receive_size() : gr55xx_ll_spi.h
- ll_spi_get_rx_fifo_level() : gr55xx_ll_spi.h
- ll_spi_get_rx_fifo_threshold() : gr55xx_ll_spi.h
- ll_spi_get_rx_sample_delay() : gr55xx_ll_spi.h
- ll_spi_get_standard() : gr55xx_ll_spi.h
- ll_spi_get_status() : gr55xx_ll_spi.h
- ll_spi_get_transfer_direction() : gr55xx_ll_spi.h
- ll_spi_get_tx_fifo_level() : gr55xx_ll_spi.h
- ll_spi_get_tx_fifo_threshold() : gr55xx_ll_spi.h
- ll_spi_get_version() : gr55xx_ll_spi.h
- ll_spi_get_wait_cycles() : gr55xx_ll_spi.h
- ll_spi_is_active_flag() : gr55xx_ll_spi.h
- ll_spi_is_enabled() : gr55xx_ll_spi.h
- ll_spi_is_enabled_dma_req_rx() : gr55xx_ll_spi.h
- ll_spi_is_enabled_dma_req_tx() : gr55xx_ll_spi.h
- ll_spi_is_enabled_it() : gr55xx_ll_spi.h
- ll_spi_is_enabled_micro_handshake() : gr55xx_ll_spi.h
- ll_spi_is_enabled_slave_out() : gr55xx_ll_spi.h
- ll_spi_is_enabled_ss() : gr55xx_ll_spi.h
- ll_spi_is_enabled_ss_toggle() : gr55xx_ll_spi.h
- ll_spi_is_enabled_test_mode() : gr55xx_ll_spi.h
- ll_spi_is_it_flag() : gr55xx_ll_spi.h
- LL_SPI_ReadReg : gr55xx_ll_spi.h
- ll_spi_receive_data16() : gr55xx_ll_spi.h
- ll_spi_receive_data32() : gr55xx_ll_spi.h
- ll_spi_receive_data8() : gr55xx_ll_spi.h
- ll_spi_set_add_inst_transfer_format() : gr55xx_ll_spi.h
- ll_spi_set_address_size() : gr55xx_ll_spi.h
- ll_spi_set_baud_rate_prescaler() : gr55xx_ll_spi.h
- ll_spi_set_clock_phase() : gr55xx_ll_spi.h
- ll_spi_set_clock_polarity() : gr55xx_ll_spi.h
- ll_spi_set_control_frame_size() : gr55xx_ll_spi.h
- ll_spi_set_data_size() : gr55xx_ll_spi.h
- ll_spi_set_dma_rx_fifo_threshold() : gr55xx_ll_spi.h
- ll_spi_set_dma_tx_fifo_threshold() : gr55xx_ll_spi.h
- ll_spi_set_frame_format() : gr55xx_ll_spi.h
- ll_spi_set_instruction_size() : gr55xx_ll_spi.h
- ll_spi_set_micro_transfer_direction() : gr55xx_ll_spi.h
- ll_spi_set_micro_transfer_mode() : gr55xx_ll_spi.h
- ll_spi_set_receive_size() : gr55xx_ll_spi.h
- ll_spi_set_rx_fifo_threshold() : gr55xx_ll_spi.h
- ll_spi_set_rx_sample_delay() : gr55xx_ll_spi.h
- ll_spi_set_standard() : gr55xx_ll_spi.h
- ll_spi_set_transfer_direction() : gr55xx_ll_spi.h
- ll_spi_set_tx_fifo_threshold() : gr55xx_ll_spi.h
- ll_spi_set_wait_cycles() : gr55xx_ll_spi.h
- ll_spi_transmit_data16() : gr55xx_ll_spi.h
- ll_spi_transmit_data32() : gr55xx_ll_spi.h
- ll_spi_transmit_data8() : gr55xx_ll_spi.h
- LL_SPI_WriteReg : gr55xx_ll_spi.h
- LL_SPIM_DEFAULT_CONFIG : gr55xx_ll_spi.h
- ll_spim_deinit() : gr55xx_ll_spi.h
- ll_spim_init() : gr55xx_ll_spi.h
- ll_spim_init_t : gr55xx_ll_spi.h
- ll_spim_struct_init() : gr55xx_ll_spi.h
- LL_SPIS_DEFAULT_CONFIG : gr55xx_ll_spi.h
- ll_spis_deinit() : gr55xx_ll_spi.h
- ll_spis_init() : gr55xx_ll_spi.h
- ll_spis_init_t : gr55xx_ll_spi.h
- ll_spis_struct_init() : gr55xx_ll_spi.h
- LL_SSI_ADDRSIZE_0BIT : gr55xx_ll_spi.h
- LL_SSI_ADDRSIZE_12BIT : gr55xx_ll_spi.h
- LL_SSI_ADDRSIZE_16BIT : gr55xx_ll_spi.h
- LL_SSI_ADDRSIZE_20BIT : gr55xx_ll_spi.h
- LL_SSI_ADDRSIZE_24BIT : gr55xx_ll_spi.h
- LL_SSI_ADDRSIZE_28BIT : gr55xx_ll_spi.h
- LL_SSI_ADDRSIZE_32BIT : gr55xx_ll_spi.h
- LL_SSI_ADDRSIZE_36BIT : gr55xx_ll_spi.h
- LL_SSI_ADDRSIZE_40BIT : gr55xx_ll_spi.h
- LL_SSI_ADDRSIZE_44BIT : gr55xx_ll_spi.h
- LL_SSI_ADDRSIZE_48BIT : gr55xx_ll_spi.h
- LL_SSI_ADDRSIZE_4BIT : gr55xx_ll_spi.h
- LL_SSI_ADDRSIZE_52BIT : gr55xx_ll_spi.h
- LL_SSI_ADDRSIZE_56BIT : gr55xx_ll_spi.h
- LL_SSI_ADDRSIZE_60BIT : gr55xx_ll_spi.h
- LL_SSI_ADDRSIZE_8BIT : gr55xx_ll_spi.h
- LL_SSI_DATASIZE_10BIT : gr55xx_ll_spi.h
- LL_SSI_DATASIZE_11BIT : gr55xx_ll_spi.h
- LL_SSI_DATASIZE_12BIT : gr55xx_ll_spi.h
- LL_SSI_DATASIZE_13BIT : gr55xx_ll_spi.h
- LL_SSI_DATASIZE_14BIT : gr55xx_ll_spi.h
- LL_SSI_DATASIZE_15BIT : gr55xx_ll_spi.h
- LL_SSI_DATASIZE_16BIT : gr55xx_ll_spi.h
- LL_SSI_DATASIZE_17BIT : gr55xx_ll_spi.h
- LL_SSI_DATASIZE_18BIT : gr55xx_ll_spi.h
- LL_SSI_DATASIZE_19BIT : gr55xx_ll_spi.h
- LL_SSI_DATASIZE_20BIT : gr55xx_ll_spi.h
- LL_SSI_DATASIZE_21BIT : gr55xx_ll_spi.h
- LL_SSI_DATASIZE_22BIT : gr55xx_ll_spi.h
- LL_SSI_DATASIZE_23BIT : gr55xx_ll_spi.h
- LL_SSI_DATASIZE_24BIT : gr55xx_ll_spi.h
- LL_SSI_DATASIZE_25BIT : gr55xx_ll_spi.h
- LL_SSI_DATASIZE_26BIT : gr55xx_ll_spi.h
- LL_SSI_DATASIZE_27BIT : gr55xx_ll_spi.h
- LL_SSI_DATASIZE_28BIT : gr55xx_ll_spi.h
- LL_SSI_DATASIZE_29BIT : gr55xx_ll_spi.h
- LL_SSI_DATASIZE_30BIT : gr55xx_ll_spi.h
- LL_SSI_DATASIZE_31BIT : gr55xx_ll_spi.h
- LL_SSI_DATASIZE_32BIT : gr55xx_ll_spi.h
- LL_SSI_DATASIZE_4BIT : gr55xx_ll_spi.h
- LL_SSI_DATASIZE_5BIT : gr55xx_ll_spi.h
- LL_SSI_DATASIZE_6BIT : gr55xx_ll_spi.h
- LL_SSI_DATASIZE_7BIT : gr55xx_ll_spi.h
- LL_SSI_DATASIZE_8BIT : gr55xx_ll_spi.h
- LL_SSI_DATASIZE_9BIT : gr55xx_ll_spi.h
- LL_SSI_DMA_RX_DIS : gr55xx_ll_spi.h
- LL_SSI_DMA_RX_EN : gr55xx_ll_spi.h
- LL_SSI_DMA_TX_DIS : gr55xx_ll_spi.h
- LL_SSI_DMA_TX_EN : gr55xx_ll_spi.h
- LL_SSI_FRF_DUALSPI : gr55xx_ll_spi.h
- LL_SSI_FRF_QUADSPI : gr55xx_ll_spi.h
- LL_SSI_FRF_SPI : gr55xx_ll_spi.h
- LL_SSI_FULL_DUPLEX : gr55xx_ll_spi.h
- LL_SSI_IM_MST : gr55xx_ll_spi.h
- LL_SSI_IM_RXF : gr55xx_ll_spi.h
- LL_SSI_IM_RXO : gr55xx_ll_spi.h
- LL_SSI_IM_RXU : gr55xx_ll_spi.h
- LL_SSI_IM_TXE : gr55xx_ll_spi.h
- LL_SSI_IM_TXO : gr55xx_ll_spi.h
- LL_SSI_INST_ADDR_ALL_IN_SPI : gr55xx_ll_spi.h
- LL_SSI_INST_ADDR_ALL_IN_SPIFRF : gr55xx_ll_spi.h
- LL_SSI_INST_IN_SPI_ADDR_IN_SPIFRF : gr55xx_ll_spi.h
- LL_SSI_INSTSIZE_0BIT : gr55xx_ll_spi.h
- LL_SSI_INSTSIZE_16BIT : gr55xx_ll_spi.h
- LL_SSI_INSTSIZE_4BIT : gr55xx_ll_spi.h
- LL_SSI_INSTSIZE_8BIT : gr55xx_ll_spi.h
- LL_SSI_IS_MST : gr55xx_ll_spi.h
- LL_SSI_IS_RXF : gr55xx_ll_spi.h
- LL_SSI_IS_RXO : gr55xx_ll_spi.h
- LL_SSI_IS_RXU : gr55xx_ll_spi.h
- LL_SSI_IS_TXE : gr55xx_ll_spi.h
- LL_SSI_IS_TXO : gr55xx_ll_spi.h
- LL_SSI_MICROWIRE_HANDSHAKE_DIS : gr55xx_ll_spi.h
- LL_SSI_MICROWIRE_HANDSHAKE_EN : gr55xx_ll_spi.h
- LL_SSI_MICROWIRE_NON_SEQUENTIAL : gr55xx_ll_spi.h
- LL_SSI_MICROWIRE_RX : gr55xx_ll_spi.h
- LL_SSI_MICROWIRE_SEQUENTIAL : gr55xx_ll_spi.h
- LL_SSI_MICROWIRE_TX : gr55xx_ll_spi.h
- LL_SSI_MW_CMDSIZE_10BIT : gr55xx_ll_spi.h
- LL_SSI_MW_CMDSIZE_11BIT : gr55xx_ll_spi.h
- LL_SSI_MW_CMDSIZE_12BIT : gr55xx_ll_spi.h
- LL_SSI_MW_CMDSIZE_13BIT : gr55xx_ll_spi.h
- LL_SSI_MW_CMDSIZE_14BIT : gr55xx_ll_spi.h
- LL_SSI_MW_CMDSIZE_15BIT : gr55xx_ll_spi.h
- LL_SSI_MW_CMDSIZE_16BIT : gr55xx_ll_spi.h
- LL_SSI_MW_CMDSIZE_1BIT : gr55xx_ll_spi.h
- LL_SSI_MW_CMDSIZE_2BIT : gr55xx_ll_spi.h
- LL_SSI_MW_CMDSIZE_3BIT : gr55xx_ll_spi.h
- LL_SSI_MW_CMDSIZE_4BIT : gr55xx_ll_spi.h
- LL_SSI_MW_CMDSIZE_5BIT : gr55xx_ll_spi.h
- LL_SSI_MW_CMDSIZE_6BIT : gr55xx_ll_spi.h
- LL_SSI_MW_CMDSIZE_7BIT : gr55xx_ll_spi.h
- LL_SSI_MW_CMDSIZE_8BIT : gr55xx_ll_spi.h
- LL_SSI_MW_CMDSIZE_9BIT : gr55xx_ll_spi.h
- LL_SSI_NORMAL_MODE : gr55xx_ll_spi.h
- LL_SSI_PROTOCOL_MICROWIRE : gr55xx_ll_spi.h
- LL_SSI_PROTOCOL_MOTOROLA : gr55xx_ll_spi.h
- LL_SSI_PROTOCOL_TI : gr55xx_ll_spi.h
- LL_SSI_READ_EEPROM : gr55xx_ll_spi.h
- LL_SSI_RIS_MST : gr55xx_ll_spi.h
- LL_SSI_RIS_RXF : gr55xx_ll_spi.h
- LL_SSI_RIS_RXO : gr55xx_ll_spi.h
- LL_SSI_RIS_RXU : gr55xx_ll_spi.h
- LL_SSI_RIS_TXE : gr55xx_ll_spi.h
- LL_SSI_RIS_TXO : gr55xx_ll_spi.h
- LL_SSI_SCPHA_1EDGE : gr55xx_ll_spi.h
- LL_SSI_SCPHA_2EDGE : gr55xx_ll_spi.h
- LL_SSI_SCPOL_HIGH : gr55xx_ll_spi.h
- LL_SSI_SCPOL_LOW : gr55xx_ll_spi.h
- LL_SSI_SIMPLEX_RX : gr55xx_ll_spi.h
- LL_SSI_SIMPLEX_TX : gr55xx_ll_spi.h
- LL_SSI_SLAVE0 : gr55xx_ll_spi.h
- LL_SSI_SLAVE1 : gr55xx_ll_spi.h
- LL_SSI_SLAVE_OUTDIS : gr55xx_ll_spi.h
- LL_SSI_SLAVE_OUTEN : gr55xx_ll_spi.h
- LL_SSI_SR_BUSY : gr55xx_ll_spi.h
- LL_SSI_SR_DCOL : gr55xx_ll_spi.h
- LL_SSI_SR_RFF : gr55xx_ll_spi.h
- LL_SSI_SR_RFNE : gr55xx_ll_spi.h
- LL_SSI_SR_TFE : gr55xx_ll_spi.h
- LL_SSI_SR_TFNF : gr55xx_ll_spi.h
- LL_SSI_SR_TXE : gr55xx_ll_spi.h
- LL_SSI_TEST_MODE : gr55xx_ll_spi.h
- ll_timer_clear_flag_it() : gr55xx_ll_tim.h
- ll_timer_deinit() : gr55xx_ll_tim.h
- ll_timer_disable_counter() : gr55xx_ll_tim.h
- ll_timer_disable_it() : gr55xx_ll_tim.h
- ll_timer_enable_counter() : gr55xx_ll_tim.h
- ll_timer_enable_it() : gr55xx_ll_tim.h
- ll_timer_get_auto_reload() : gr55xx_ll_tim.h
- ll_timer_get_counter() : gr55xx_ll_tim.h
- ll_timer_init() : gr55xx_ll_tim.h
- ll_timer_init_t : gr55xx_ll_tim.h
- ll_timer_is_active_flag_it() : gr55xx_ll_tim.h
- ll_timer_is_enabled_counter() : gr55xx_ll_tim.h
- ll_timer_is_enabled_it() : gr55xx_ll_tim.h
- LL_TIMER_ReadReg : gr55xx_ll_tim.h
- ll_timer_set_auto_reload() : gr55xx_ll_tim.h
- ll_timer_set_counter() : gr55xx_ll_tim.h
- ll_timer_struct_init() : gr55xx_ll_tim.h
- LL_TIMER_WriteReg : gr55xx_ll_tim.h
- ll_uart_clear_line_status_flag() : gr55xx_ll_uart.h
- ll_uart_config_character() : gr55xx_ll_uart.h
- LL_UART_CTSPIN_STATE_ACTIVE : gr55xx_ll_uart.h
- LL_UART_CTSPIN_STATE_INACTIVE : gr55xx_ll_uart.h
- LL_UART_DATABITS_5B : gr55xx_ll_uart.h
- LL_UART_DATABITS_6B : gr55xx_ll_uart.h
- LL_UART_DATABITS_7B : gr55xx_ll_uart.h
- LL_UART_DATABITS_8B : gr55xx_ll_uart.h
- LL_UART_DEFAULT_CONFIG : gr55xx_ll_uart.h
- ll_uart_deinit() : gr55xx_ll_uart.h
- ll_uart_disable_break_sending() : gr55xx_ll_uart.h
- ll_uart_disable_fifo() : gr55xx_ll_uart.h
- ll_uart_disable_it() : gr55xx_ll_uart.h
- ll_uart_disable_it_ms() : gr55xx_ll_uart.h
- ll_uart_disable_it_rda() : gr55xx_ll_uart.h
- ll_uart_disable_it_rls() : gr55xx_ll_uart.h
- ll_uart_disable_it_thre() : gr55xx_ll_uart.h
- ll_uart_dma_get_register_address() : gr55xx_ll_uart.h
- ll_uart_enable_break_sending() : gr55xx_ll_uart.h
- ll_uart_enable_fifo() : gr55xx_ll_uart.h
- ll_uart_enable_it() : gr55xx_ll_uart.h
- ll_uart_enable_it_rda() : gr55xx_ll_uart.h
- ll_uart_enable_it_rls() : gr55xx_ll_uart.h
- ll_uart_enable_it_thre() : gr55xx_ll_uart.h
- ll_uart_enabled_it_ms() : gr55xx_ll_uart.h
- ll_uart_flush_rx_fifo() : gr55xx_ll_uart.h
- ll_uart_flush_tx_fifo() : gr55xx_ll_uart.h
- ll_uart_get_baud_rate() : gr55xx_ll_uart.h
- ll_uart_get_cts_pin_state() : gr55xx_ll_uart.h
- ll_uart_get_data_bits_length() : gr55xx_ll_uart.h
- ll_uart_get_hw_flow_ctrl() : gr55xx_ll_uart.h
- ll_uart_get_it_flag() : gr55xx_ll_uart.h
- ll_uart_get_line_status_flag() : gr55xx_ll_uart.h
- ll_uart_get_parity() : gr55xx_ll_uart.h
- ll_uart_get_rts_pin_state() : gr55xx_ll_uart.h
- ll_uart_get_rx_fifo_level() : gr55xx_ll_uart.h
- ll_uart_get_rx_fifo_threshold() : gr55xx_ll_uart.h
- ll_uart_get_stop_bits_length() : gr55xx_ll_uart.h
- ll_uart_get_tx_fifo_level() : gr55xx_ll_uart.h
- ll_uart_get_tx_fifo_threshold() : gr55xx_ll_uart.h
- LL_UART_HWCONTROL_NONE : gr55xx_ll_uart.h
- LL_UART_HWCONTROL_RTS_CTS : gr55xx_ll_uart.h
- LL_UART_IER_MS : gr55xx_ll_uart.h
- LL_UART_IER_RDA : gr55xx_ll_uart.h
- LL_UART_IER_RLS : gr55xx_ll_uart.h
- LL_UART_IER_THRE : gr55xx_ll_uart.h
- LL_UART_IIR_CTO : gr55xx_ll_uart.h
- LL_UART_IIR_MS : gr55xx_ll_uart.h
- LL_UART_IIR_NIP : gr55xx_ll_uart.h
- LL_UART_IIR_RDA : gr55xx_ll_uart.h
- LL_UART_IIR_RLS : gr55xx_ll_uart.h
- LL_UART_IIR_THRE : gr55xx_ll_uart.h
- ll_uart_init() : gr55xx_ll_uart.h
- ll_uart_init_t : gr55xx_ll_uart.h
- ll_uart_is_active_flag_rff() : gr55xx_ll_uart.h
- ll_uart_is_active_flag_rfne() : gr55xx_ll_uart.h
- ll_uart_is_active_flag_tfe() : gr55xx_ll_uart.h
- ll_uart_is_active_flag_tfnf() : gr55xx_ll_uart.h
- ll_uart_is_changed_cts() : gr55xx_ll_uart.h
- ll_uart_is_enabled_break_sending() : gr55xx_ll_uart.h
- ll_uart_is_enabled_fifo() : gr55xx_ll_uart.h
- ll_uart_is_enabled_it() : gr55xx_ll_uart.h
- ll_uart_is_enabled_it_ms() : gr55xx_ll_uart.h
- ll_uart_is_enabled_it_rda() : gr55xx_ll_uart.h
- ll_uart_is_enabled_it_rls() : gr55xx_ll_uart.h
- ll_uart_is_enabled_it_thre() : gr55xx_ll_uart.h
- LL_UART_LSR_BI : gr55xx_ll_uart.h
- LL_UART_LSR_FE : gr55xx_ll_uart.h
- LL_UART_LSR_OE : gr55xx_ll_uart.h
- LL_UART_LSR_PE : gr55xx_ll_uart.h
- LL_UART_LSR_RFE : gr55xx_ll_uart.h
- LL_UART_LSR_TEMT : gr55xx_ll_uart.h
- LL_UART_LSR_THRE : gr55xx_ll_uart.h
- LL_UART_PARITY_EVEN : gr55xx_ll_uart.h
- LL_UART_PARITY_NONE : gr55xx_ll_uart.h
- LL_UART_PARITY_ODD : gr55xx_ll_uart.h
- LL_UART_PARITY_SP0 : gr55xx_ll_uart.h
- LL_UART_PARITY_SP1 : gr55xx_ll_uart.h
- LL_UART_ReadReg : gr55xx_ll_uart.h
- ll_uart_receive_data8() : gr55xx_ll_uart.h
- ll_uart_reset() : gr55xx_ll_uart.h
- LL_UART_RTSPIN_STATE_ACTIVE : gr55xx_ll_uart.h
- LL_UART_RTSPIN_STATE_INACTIVE : gr55xx_ll_uart.h
- LL_UART_RX_FIFO_TH_CHAR_1 : gr55xx_ll_uart.h
- LL_UART_RX_FIFO_TH_FULL_2 : gr55xx_ll_uart.h
- LL_UART_RX_FIFO_TH_HALF_FULL : gr55xx_ll_uart.h
- LL_UART_RX_FIFO_TH_QUARTER_FULL : gr55xx_ll_uart.h
- ll_uart_set_baud_rate() : gr55xx_ll_uart.h
- ll_uart_set_data_bits_length() : gr55xx_ll_uart.h
- ll_uart_set_hw_flow_ctrl() : gr55xx_ll_uart.h
- ll_uart_set_parity() : gr55xx_ll_uart.h
- ll_uart_set_rts_pin_state() : gr55xx_ll_uart.h
- ll_uart_set_rx_fifo_threshold() : gr55xx_ll_uart.h
- ll_uart_set_stop_bits_length() : gr55xx_ll_uart.h
- ll_uart_set_tx_fifo_threshold() : gr55xx_ll_uart.h
- LL_UART_STOPBITS_1 : gr55xx_ll_uart.h
- LL_UART_STOPBITS_1_5 : gr55xx_ll_uart.h
- LL_UART_STOPBITS_2 : gr55xx_ll_uart.h
- ll_uart_struct_init() : gr55xx_ll_uart.h
- ll_uart_transmit_data8() : gr55xx_ll_uart.h
- LL_UART_TX_FIFO_TH_CHAR_2 : gr55xx_ll_uart.h
- LL_UART_TX_FIFO_TH_EMPTY : gr55xx_ll_uart.h
- LL_UART_TX_FIFO_TH_HALF_FULL : gr55xx_ll_uart.h
- LL_UART_TX_FIFO_TH_QUARTER_FULL : gr55xx_ll_uart.h
- LL_UART_USR_RFF : gr55xx_ll_uart.h
- LL_UART_USR_RFNE : gr55xx_ll_uart.h
- LL_UART_USR_TFE : gr55xx_ll_uart.h
- LL_UART_USR_TFNF : gr55xx_ll_uart.h
- LL_UART_WriteReg : gr55xx_ll_uart.h
- ll_wdt_clear_flag_it() : gr55xx_ll_wdt.h
- ll_wdt_disable() : gr55xx_ll_wdt.h
- ll_wdt_disable_reset() : gr55xx_ll_wdt.h
- ll_wdt_disable_write_access() : gr55xx_ll_wdt.h
- ll_wdt_enable() : gr55xx_ll_wdt.h
- ll_wdt_enable_reset() : gr55xx_ll_wdt.h
- ll_wdt_enable_write_access() : gr55xx_ll_wdt.h
- ll_wdt_get_counter_load() : gr55xx_ll_wdt.h
- ll_wdt_get_counter_value() : gr55xx_ll_wdt.h
- ll_wdt_is_active_flag_it() : gr55xx_ll_wdt.h
- ll_wdt_is_enabled() : gr55xx_ll_wdt.h
- ll_wdt_is_enabled_reset() : gr55xx_ll_wdt.h
- LL_WDT_LOCK_WR_ACCESS_DISABLE : gr55xx_ll_wdt.h
- LL_WDT_LOCK_WR_ACCESS_ENABLE : gr55xx_ll_wdt.h
- LL_WDT_ReadReg : gr55xx_ll_wdt.h
- ll_wdt_reload_counter() : gr55xx_ll_wdt.h
- ll_wdt_set_counter_load() : gr55xx_ll_wdt.h
- LL_WDT_WriteReg : gr55xx_ll_wdt.h
- LL_XQSPI_BAUD_RATE_16M : gr55xx_ll_xqspi.h
- LL_XQSPI_BAUD_RATE_24M : gr55xx_ll_xqspi.h
- LL_XQSPI_BAUD_RATE_32M : gr55xx_ll_xqspi.h
- LL_XQSPI_BAUD_RATE_48M : gr55xx_ll_xqspi.h
- LL_XQSPI_BAUD_RATE_64M : gr55xx_ll_xqspi.h
- LL_XQSPI_CACHE_DIS : gr55xx_ll_xqspi.h
- LL_XQSPI_CACHE_EN : gr55xx_ll_xqspi.h
- LL_XQSPI_CACHE_FIFO_CLEAR : gr55xx_ll_xqspi.h
- LL_XQSPI_CACHE_FIFO_NORMAL : gr55xx_ll_xqspi.h
- LL_XQSPI_CACHE_HITMISS_CLEAR : gr55xx_ll_xqspi.h
- LL_XQSPI_CACHE_HITMISS_NORMAL : gr55xx_ll_xqspi.h
- ll_xqspi_clear_qspi_flag() : gr55xx_ll_xqspi.h
- LL_XQSPI_DEFAULT_CONFIG : gr55xx_ll_xqspi.h
- ll_xqspi_deinit() : gr55xx_ll_xqspi.h
- ll_xqspi_disable_cache() : gr55xx_ll_xqspi.h
- ll_xqspi_disable_cache_dbgmux() : gr55xx_ll_xqspi.h
- ll_xqspi_disable_cache_flush() : gr55xx_ll_xqspi.h
- ll_xqspi_disable_cache_retention() : gr55xx_ll_xqspi.h
- ll_xqspi_disable_exflash_power() : gr55xx_ll_xqspi.h
- ll_xqspi_disable_inhibt_rx() : gr55xx_ll_xqspi.h
- ll_xqspi_disable_inhibt_tx() : gr55xx_ll_xqspi.h
- LL_XQSPI_DISABLE_PRESENT : gr55xx_ll_xqspi.h
- ll_xqspi_disable_qspi() : gr55xx_ll_xqspi.h
- ll_xqspi_disable_qspi_contxfer() : gr55xx_ll_xqspi.h
- ll_xqspi_disable_qspi_contxfer_extend() : gr55xx_ll_xqspi.h
- ll_xqspi_disable_qspi_dma() : gr55xx_ll_xqspi.h
- ll_xqspi_disable_qspi_dummy() : gr55xx_ll_xqspi.h
- ll_xqspi_disable_qspi_it() : gr55xx_ll_xqspi.h
- ll_xqspi_disable_qspi_ssout() : gr55xx_ll_xqspi.h
- ll_xqspi_disable_xip() : gr55xx_ll_xqspi.h
- ll_xqspi_disable_xip_hp() : gr55xx_ll_xqspi.h
- ll_xqspi_disable_xip_it() : gr55xx_ll_xqspi.h
- ll_xqspi_enable_cache() : gr55xx_ll_xqspi.h
- ll_xqspi_enable_cache_dbgmux() : gr55xx_ll_xqspi.h
- ll_xqspi_enable_cache_flush() : gr55xx_ll_xqspi.h
- ll_xqspi_enable_cache_retention() : gr55xx_ll_xqspi.h
- ll_xqspi_enable_exflash_power() : gr55xx_ll_xqspi.h
- ll_xqspi_enable_inhibt_rx() : gr55xx_ll_xqspi.h
- ll_xqspi_enable_inhibt_tx() : gr55xx_ll_xqspi.h
- LL_XQSPI_ENABLE_PRESENT : gr55xx_ll_xqspi.h
- ll_xqspi_enable_qspi() : gr55xx_ll_xqspi.h
- ll_xqspi_enable_qspi_contxfer() : gr55xx_ll_xqspi.h
- ll_xqspi_enable_qspi_contxfer_extend() : gr55xx_ll_xqspi.h
- ll_xqspi_enable_qspi_dma() : gr55xx_ll_xqspi.h
- ll_xqspi_enable_qspi_dummy() : gr55xx_ll_xqspi.h
- ll_xqspi_enable_qspi_it() : gr55xx_ll_xqspi.h
- ll_xqspi_enable_qspi_ssout() : gr55xx_ll_xqspi.h
- ll_xqspi_enable_xip() : gr55xx_ll_xqspi.h
- ll_xqspi_enable_xip_hp() : gr55xx_ll_xqspi.h
- ll_xqspi_enable_xip_it() : gr55xx_ll_xqspi.h
- LL_XQSPI_FLASH_WRITE_128BIT : gr55xx_ll_xqspi.h
- LL_XQSPI_FLASH_WRITE_32BIT : gr55xx_ll_xqspi.h
- ll_xqspi_get_cache_dbgbus() : gr55xx_ll_xqspi.h
- ll_xqspi_get_cache_fifo() : gr55xx_ll_xqspi.h
- ll_xqspi_get_cache_flag() : gr55xx_ll_xqspi.h
- ll_xqspi_get_cache_hitcount() : gr55xx_ll_xqspi.h
- ll_xqspi_get_cache_hitmiss() : gr55xx_ll_xqspi.h
- ll_xqspi_get_cache_misscount() : gr55xx_ll_xqspi.h
- ll_xqspi_get_flag_xip_it() : gr55xx_ll_xqspi.h
- ll_xqspi_get_flash_write() : gr55xx_ll_xqspi.h
- ll_xqspi_get_it_flag() : gr55xx_ll_xqspi.h
- ll_xqspi_get_present_bypass() : gr55xx_ll_xqspi.h
- ll_xqspi_get_qspi_cpha() : gr55xx_ll_xqspi.h
- ll_xqspi_get_qspi_cpol() : gr55xx_ll_xqspi.h
- ll_xqspi_get_qspi_data_order() : gr55xx_ll_xqspi.h
- ll_xqspi_get_qspi_datasize() : gr55xx_ll_xqspi.h
- ll_xqspi_get_qspi_frf() : gr55xx_ll_xqspi.h
- ll_xqspi_get_qspi_rft() : gr55xx_ll_xqspi.h
- ll_xqspi_get_qspi_rx_fifo_level() : gr55xx_ll_xqspi.h
- ll_xqspi_get_qspi_speed() : gr55xx_ll_xqspi.h
- ll_xqspi_get_qspi_sspol() : gr55xx_ll_xqspi.h
- ll_xqspi_get_qspi_status() : gr55xx_ll_xqspi.h
- ll_xqspi_get_qspi_tft() : gr55xx_ll_xqspi.h
- ll_xqspi_get_qspi_tx_fifo_level() : gr55xx_ll_xqspi.h
- ll_xqspi_get_qspi_wait() : gr55xx_ll_xqspi.h
- ll_xqspi_get_req_xip_it() : gr55xx_ll_xqspi.h
- ll_xqspi_get_xip_addr_size() : gr55xx_ll_xqspi.h
- ll_xqspi_get_xip_cmd() : gr55xx_ll_xqspi.h
- ll_xqspi_get_xip_cpha() : gr55xx_ll_xqspi.h
- ll_xqspi_get_xip_cpol() : gr55xx_ll_xqspi.h
- ll_xqspi_get_xip_dummy_hp() : gr55xx_ll_xqspi.h
- ll_xqspi_get_xip_dummycycles() : gr55xx_ll_xqspi.h
- ll_xqspi_get_xip_endian() : gr55xx_ll_xqspi.h
- ll_xqspi_get_xip_flag() : gr55xx_ll_xqspi.h
- ll_xqspi_get_xip_hp_cmd() : gr55xx_ll_xqspi.h
- ll_xqspi_get_xip_ss() : gr55xx_ll_xqspi.h
- ll_xqspi_init() : gr55xx_ll_xqspi.h
- ll_xqspi_init_t : gr55xx_ll_xqspi.h
- ll_xqspi_is_active_qspi_flag() : gr55xx_ll_xqspi.h
- ll_xqspi_is_enable_cache_retention() : gr55xx_ll_xqspi.h
- ll_xqspi_is_enable_exflash_power() : gr55xx_ll_xqspi.h
- ll_xqspi_is_enabled_cache() : gr55xx_ll_xqspi.h
- ll_xqspi_is_enabled_cache_dbgmux() : gr55xx_ll_xqspi.h
- ll_xqspi_is_enabled_cache_flush() : gr55xx_ll_xqspi.h
- ll_xqspi_is_enabled_inhibt_rx() : gr55xx_ll_xqspi.h
- ll_xqspi_is_enabled_inhibt_tx() : gr55xx_ll_xqspi.h
- ll_xqspi_is_enabled_qspi() : gr55xx_ll_xqspi.h
- ll_xqspi_is_enabled_qspi_contxfer() : gr55xx_ll_xqspi.h
- ll_xqspi_is_enabled_qspi_contxfer_extend() : gr55xx_ll_xqspi.h
- ll_xqspi_is_enabled_qspi_dma() : gr55xx_ll_xqspi.h
- ll_xqspi_is_enabled_qspi_dummy() : gr55xx_ll_xqspi.h
- ll_xqspi_is_enabled_qspi_it() : gr55xx_ll_xqspi.h
- ll_xqspi_is_enabled_xip() : gr55xx_ll_xqspi.h
- ll_xqspi_is_enabled_xip_hp() : gr55xx_ll_xqspi.h
- ll_xqspi_is_enabled_xip_it() : gr55xx_ll_xqspi.h
- ll_xqspi_is_qspi_it_flag() : gr55xx_ll_xqspi.h
- LL_XQSPI_MODE_QSPI : gr55xx_ll_xqspi.h
- LL_XQSPI_MODE_XIP : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_DATASIZE_12BIT : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_DATASIZE_16BIT : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_DATASIZE_20BIT : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_DATASIZE_24BIT : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_DATASIZE_28BIT : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_DATASIZE_32BIT : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_DATASIZE_4BIT : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_DATASIZE_8BIT : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_FIFO_DEPTH : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_FIFO_WATERMARK_1_2 : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_FIFO_WATERMARK_1_4 : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_FIFO_WATERMARK_1_8 : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_FIFO_WATERMARK_3_4 : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_FRF_DUALSPI : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_FRF_QUADSPI : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_FRF_SPI : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_IM_DONE : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_IM_RFF : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_IM_RFTF : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_IM_TFE : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_IM_TFTF : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_IS_DONE : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_IS_RFF : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_IS_RFTF : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_IS_TFE : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_IS_TFTF : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_LSB : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_MSB : gr55xx_ll_xqspi.h
- ll_xqspi_qspi_receive_data16() : gr55xx_ll_xqspi.h
- ll_xqspi_qspi_receive_data32() : gr55xx_ll_xqspi.h
- ll_xqspi_qspi_receive_data8() : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_STAT_BUSY : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_STAT_RFE : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_STAT_RFF : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_STAT_RFTF : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_STAT_TFE : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_STAT_TFF : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_STAT_TFTF : gr55xx_ll_xqspi.h
- ll_xqspi_qspi_transmit_data16() : gr55xx_ll_xqspi.h
- ll_xqspi_qspi_transmit_data32() : gr55xx_ll_xqspi.h
- ll_xqspi_qspi_transmit_data8() : gr55xx_ll_xqspi.h
- LL_XQSPI_ReadReg : gr55xx_ll_xqspi.h
- LL_XQSPI_SCPHA_1EDGE : gr55xx_ll_xqspi.h
- LL_XQSPI_SCPHA_2EDGE : gr55xx_ll_xqspi.h
- LL_XQSPI_SCPOL_HIGH : gr55xx_ll_xqspi.h
- LL_XQSPI_SCPOL_LOW : gr55xx_ll_xqspi.h
- ll_xqspi_set_cache_dbgbus() : gr55xx_ll_xqspi.h
- ll_xqspi_set_cache_fifo() : gr55xx_ll_xqspi.h
- ll_xqspi_set_cache_hitmiss() : gr55xx_ll_xqspi.h
- ll_xqspi_set_flash_write() : gr55xx_ll_xqspi.h
- ll_xqspi_set_present_bypass() : gr55xx_ll_xqspi.h
- ll_xqspi_set_qspi_cpha() : gr55xx_ll_xqspi.h
- ll_xqspi_set_qspi_cpol() : gr55xx_ll_xqspi.h
- ll_xqspi_set_qspi_data_order() : gr55xx_ll_xqspi.h
- ll_xqspi_set_qspi_datasize() : gr55xx_ll_xqspi.h
- ll_xqspi_set_qspi_frf() : gr55xx_ll_xqspi.h
- ll_xqspi_set_qspi_rft() : gr55xx_ll_xqspi.h
- ll_xqspi_set_qspi_speed() : gr55xx_ll_xqspi.h
- ll_xqspi_set_qspi_sspol() : gr55xx_ll_xqspi.h
- ll_xqspi_set_qspi_tft() : gr55xx_ll_xqspi.h
- ll_xqspi_set_qspi_wait() : gr55xx_ll_xqspi.h
- ll_xqspi_set_xip_addr_size() : gr55xx_ll_xqspi.h
- ll_xqspi_set_xip_cmd() : gr55xx_ll_xqspi.h
- ll_xqspi_set_xip_cpha() : gr55xx_ll_xqspi.h
- ll_xqspi_set_xip_cpol() : gr55xx_ll_xqspi.h
- ll_xqspi_set_xip_dummy_hp() : gr55xx_ll_xqspi.h
- ll_xqspi_set_xip_dummycycles() : gr55xx_ll_xqspi.h
- ll_xqspi_set_xip_endian() : gr55xx_ll_xqspi.h
- ll_xqspi_set_xip_hp_cmd() : gr55xx_ll_xqspi.h
- ll_xqspi_set_xip_ss() : gr55xx_ll_xqspi.h
- ll_xqspi_struct_init() : gr55xx_ll_xqspi.h
- LL_XQSPI_WriteReg : gr55xx_ll_xqspi.h
- LL_XQSPI_XIP_ADDR_3BYTES : gr55xx_ll_xqspi.h
- LL_XQSPI_XIP_ADDR_4BYTES : gr55xx_ll_xqspi.h
- LL_XQSPI_XIP_CMD_DUAL_IO_READ : gr55xx_ll_xqspi.h
- LL_XQSPI_XIP_CMD_DUAL_OUT_READ : gr55xx_ll_xqspi.h
- LL_XQSPI_XIP_CMD_FAST_READ : gr55xx_ll_xqspi.h
- LL_XQSPI_XIP_CMD_QUAD_IO_READ : gr55xx_ll_xqspi.h
- LL_XQSPI_XIP_CMD_QUAD_OUT_READ : gr55xx_ll_xqspi.h
- LL_XQSPI_XIP_CMD_READ : gr55xx_ll_xqspi.h
- LL_XQSPI_XIP_ENDIAN_BIG : gr55xx_ll_xqspi.h
- LL_XQSPI_XIP_ENDIAN_LITTLE : gr55xx_ll_xqspi.h
- LL_XQSPI_XIP_SS0 : gr55xx_ll_xqspi.h
- LL_XQSPI_XIP_SS1 : gr55xx_ll_xqspi.h
- LL_XQSPI_XIP_SS2 : gr55xx_ll_xqspi.h
- LL_XQSPI_XIP_SS3 : gr55xx_ll_xqspi.h
- lls_alert_level_get() : lls.h
- LLS_ALERT_LEVEL_HIGH_ALERT : lls.h
- LLS_ALERT_LEVEL_MILD_ALERT : lls.h
- LLS_ALERT_LEVEL_NO_ALERT : lls.h
- lls_alert_levels_t : lls.h
- LLS_C_ALERT_LEVEL_HIGH_ALERT : lls_c.h
- LLS_C_ALERT_LEVEL_MILD_ALERT : lls_c.h
- LLS_C_ALERT_LEVEL_NO_ALERT : lls_c.h
- lls_c_alert_level_read() : lls_c.h
- lls_c_alert_level_set() : lls_c.h
- lls_c_alert_level_t : lls_c.h
- LLS_C_CONNECTION_MAX : lls_c.h
- lls_c_disc_srvc_start() : lls_c.h
- LLS_C_EVT_ALERT_LEVEL_RECEIVE : lls_c.h
- LLS_C_EVT_ALERT_LEVEL_SET_ERR : lls_c.h
- LLS_C_EVT_ALERT_LEVEL_SET_SUCCESS : lls_c.h
- LLS_C_EVT_DISCOVERY_COMPLETE : lls_c.h
- LLS_C_EVT_DISCOVERY_FAIL : lls_c.h
- lls_c_evt_handler_t : lls_c.h
- LLS_C_EVT_INVALID : lls_c.h
- lls_c_evt_type_t : lls_c.h
- lls_client_init() : lls_c.h
- lls_evt_handler_t : lls.h
- LLS_EVT_INVALID : lls.h
- LLS_EVT_LINK_LOSS_ALERT : lls.h
- lls_evt_type_t : lls.h
- lls_service_init() : lls.h
- LMS_CONNECTION_MAX : lms.h
- LMS_EVT_CMD_NOTIFICATION_DISABLED : lms.h
- LMS_EVT_CMD_NOTIFICATION_ENABLED : lms.h
- LMS_EVT_CMD_NOTIFY_COMPLETE : lms.h
- LMS_EVT_CMD_RECEIVE_DATA : lms.h
- LMS_EVT_DATA_NOTIFICATION_DISABLED : lms.h
- LMS_EVT_DATA_NOTIFICATION_ENABLED : lms.h
- LMS_EVT_DATA_NOTIFY_COMPLETE : lms.h
- LMS_EVT_DATA_RECEIVE_DATA : lms.h
- lms_evt_handler_t : lms.h
- LMS_EVT_INVALID : lms.h
- lms_evt_type_t : lms.h
- LMS_MAX_DATA_LEN : lms.h
- lms_notify_cmd() : lms.h
- lms_notify_data() : lms.h
- LMS_PATTERN_VALUE : lms.h
- lms_service_init() : lms.h
- LMS_SERVICE_UUID : lms.h
- LNS_CONNECTION_MAX : lns.h
- lns_ctrl_pt_t : lns.h
- LNS_CTRL_PT_TRACE_INFO_CLEAR : lns.h
- LNS_CTRL_PT_TRACE_INFO_DUMP : lns.h
- LNS_CTRL_PT_TRACE_STATUS_GET : lns.h
- LNS_EVT_CTRL_PT_IND_DISABLE : lns.h
- LNS_EVT_CTRL_PT_IND_ENABLE : lns.h
- lns_evt_handler_t : lns.h
- LNS_EVT_INVALID : lns.h
- LNS_EVT_LOG_INFO_NTF_DISABLE : lns.h
- LNS_EVT_LOG_INFO_NTF_ENABLE : lns.h
- LNS_EVT_TRACE_INFO_CLEAR : lns.h
- LNS_EVT_TRACE_INFO_DUMP : lns.h
- LNS_EVT_TRACE_STATUS_GET : lns.h
- lns_evt_type_t : lns.h
- LNS_LOG_CTRL_PT_VAL_LEN : lns.h
- lns_log_info_send() : lns.h
- LNS_LOG_INFO_VAL_LEN : lns.h
- lns_log_status_send() : lns.h
- lns_pay_load_update() : lns.h
- lns_service_init() : lns.h
- LNS_SERVICE_UUID : lns.h
- local_hal_flash_erase() : gr55xx_nvds.h
- local_hal_flash_erase_chip() : gr55xx_nvds.h
- local_hal_flash_get_info() : gr55xx_nvds.h
- local_hal_flash_get_security() : gr55xx_nvds.h
- local_hal_flash_read() : gr55xx_nvds.h
- local_hal_flash_set_security() : gr55xx_nvds.h
- local_hal_flash_write() : gr55xx_nvds.h
- local_hal_flash_write_r() : gr55xx_nvds.h
- LOCAL_INT_DISABLE : gr55xx_hal.h
- LOCAL_INT_RESTORE : gr55xx_hal.h
- local_time_encode() : cts.h
- local_time_universal_decode() : cts.h