### - l -

- lfrc32k_calibration() : platform_sdk.h
- ll_adc_deinit() : gr55xx_ll_adc.h
- ll_adc_disable() : gr55xx_ll_adc.h
- ll_adc_disable_clock() : gr55xx_ll_adc.h
- ll_adc_disable_mas_rst() : gr55xx_ll_adc.h
- ll_adc_disable_ofs_cal() : gr55xx_ll_adc.h
- ll_adc_disable_temp() : gr55xx_ll_adc.h
- ll_adc_disable_vbat() : gr55xx_ll_adc.h
- ll_adc_enable() : gr55xx_ll_adc.h
- ll_adc_enable_clock() : gr55xx_ll_adc.h
- ll_adc_enable_mas_rst() : gr55xx_ll_adc.h
- ll_adc_enable_ofs_cal() : gr55xx_ll_adc.h
- ll_adc_enable_temp() : gr55xx_ll_adc.h
- ll_adc_enable_vbat() : gr55xx_ll_adc.h
- ll_adc_get_channeln() : gr55xx_ll_adc.h
- ll_adc_get_channelp() : gr55xx_ll_adc.h
- ll_adc_get_clock() : gr55xx_ll_adc.h
- ll_adc_get_dynamic_rang() : gr55xx_ll_adc.h
- ll_adc_get_fifo_count() : gr55xx_ll_adc.h
- ll_adc_get_input_mode() : gr55xx_ll_adc.h
- ll_adc_get_ref() : gr55xx_ll_adc.h
- ll_adc_get_ref_current() : gr55xx_ll_adc.h
- ll_adc_get_ref_value() : gr55xx_ll_adc.h
- ll_adc_get_thresh() : gr55xx_ll_adc.h
- ll_adc_init() : gr55xx_ll_adc.h
- ll_adc_is_enabled() : gr55xx_ll_adc.h
- ll_adc_is_enabled_clock() : gr55xx_ll_adc.h
- ll_adc_is_enabled_mas_rst() : gr55xx_ll_adc.h
- ll_adc_is_enabled_ofs_cal() : gr55xx_ll_adc.h
- ll_adc_is_enabled_temp() : gr55xx_ll_adc.h
- ll_adc_is_enabled_vbat() : gr55xx_ll_adc.h
- ll_adc_is_fifo_notempty() : gr55xx_ll_adc.h
- ll_adc_read_fifo() : gr55xx_ll_adc.h
- ll_adc_set_channeln() : gr55xx_ll_adc.h
- ll_adc_set_channelp() : gr55xx_ll_adc.h
- ll_adc_set_clock() : gr55xx_ll_adc.h
- ll_adc_set_dynamic_rang() : gr55xx_ll_adc.h
- ll_adc_set_input_mode() : gr55xx_ll_adc.h
- ll_adc_set_ref() : gr55xx_ll_adc.h
- ll_adc_set_ref_current() : gr55xx_ll_adc.h
- ll_adc_set_ref_value() : gr55xx_ll_adc.h
- ll_adc_set_thresh() : gr55xx_ll_adc.h
- ll_adc_struct_init() : gr55xx_ll_adc.h
- ll_aes_clear_flag_it_done() : gr55xx_ll_aes.h
- ll_aes_deinit() : gr55xx_ll_aes.h
- ll_aes_disable() : gr55xx_ll_aes.h
- ll_aes_disable_dma_start() : gr55xx_ll_aes.h
- ll_aes_disable_encryption() : gr55xx_ll_aes.h
- ll_aes_disable_full_mask() : gr55xx_ll_aes.h
- ll_aes_disable_it_done() : gr55xx_ll_aes.h
- ll_aes_disable_little_endian() : gr55xx_ll_aes.h
- ll_aes_disable_start() : gr55xx_ll_aes.h
- ll_aes_enable() : gr55xx_ll_aes.h
- ll_aes_enable_dma_start() : gr55xx_ll_aes.h
- ll_aes_enable_encryption() : gr55xx_ll_aes.h
- ll_aes_enable_full_mask() : gr55xx_ll_aes.h
- ll_aes_enable_it_done() : gr55xx_ll_aes.h
- ll_aes_enable_little_endian() : gr55xx_ll_aes.h
- ll_aes_enable_read_key() : gr55xx_ll_aes.h
- ll_aes_enable_start() : gr55xx_ll_aes.h
- ll_aes_get_data_127_96() : gr55xx_ll_aes.h
- ll_aes_get_data_31_0() : gr55xx_ll_aes.h
- ll_aes_get_data_63_32() : gr55xx_ll_aes.h
- ll_aes_get_data_95_64() : gr55xx_ll_aes.h
- ll_aes_get_dma_read_address() : gr55xx_ll_aes.h
- ll_aes_get_dma_transfer_block() : gr55xx_ll_aes.h
- ll_aes_get_dma_write_address() : gr55xx_ll_aes.h
- ll_aes_get_key_address() : gr55xx_ll_aes.h
- ll_aes_get_key_size() : gr55xx_ll_aes.h
- ll_aes_get_key_type() : gr55xx_ll_aes.h
- ll_aes_get_operation_mode() : gr55xx_ll_aes.h
- ll_aes_get_seed_Imask() : gr55xx_ll_aes.h
- ll_aes_get_seed_in() : gr55xx_ll_aes.h
- ll_aes_get_seed_Osbox() : gr55xx_ll_aes.h
- ll_aes_get_seed_out() : gr55xx_ll_aes.h
- ll_aes_init() : gr55xx_ll_aes.h
- ll_aes_is_action_flag_dma_done() : gr55xx_ll_aes.h
- ll_aes_is_action_flag_dma_error() : gr55xx_ll_aes.h
- ll_aes_is_action_flag_it_done() : gr55xx_ll_aes.h
- ll_aes_is_action_flag_key_valid() : gr55xx_ll_aes.h
- ll_aes_is_action_flag_ready() : gr55xx_ll_aes.h
- ll_aes_is_enabled() : gr55xx_ll_aes.h
- ll_aes_is_enabled_dma_start() : gr55xx_ll_aes.h
- ll_aes_is_enabled_encryption() : gr55xx_ll_aes.h
- ll_aes_is_enabled_full_mask() : gr55xx_ll_aes.h
- ll_aes_is_enabled_it_done() : gr55xx_ll_aes.h
- ll_aes_is_enabled_little_endian() : gr55xx_ll_aes.h
- ll_aes_is_enabled_start() : gr55xx_ll_aes.h
- ll_aes_set_data_127_96() : gr55xx_ll_aes.h
- ll_aes_set_data_31_0() : gr55xx_ll_aes.h
- ll_aes_set_data_63_32() : gr55xx_ll_aes.h
- ll_aes_set_data_95_64() : gr55xx_ll_aes.h
- ll_aes_set_dma_read_address() : gr55xx_ll_aes.h
- ll_aes_set_dma_transfer_block() : gr55xx_ll_aes.h
- ll_aes_set_dma_write_address() : gr55xx_ll_aes.h
- ll_aes_set_first_block() : gr55xx_ll_aes.h
- ll_aes_set_key_127_96() : gr55xx_ll_aes.h
- ll_aes_set_key_159_128() : gr55xx_ll_aes.h
- ll_aes_set_key_191_160() : gr55xx_ll_aes.h
- ll_aes_set_key_223_192() : gr55xx_ll_aes.h
- ll_aes_set_key_255_224() : gr55xx_ll_aes.h
- ll_aes_set_key_31_0() : gr55xx_ll_aes.h
- ll_aes_set_key_63_32() : gr55xx_ll_aes.h
- ll_aes_set_key_95_64() : gr55xx_ll_aes.h
- ll_aes_set_key_address() : gr55xx_ll_aes.h
- ll_aes_set_key_port_mask() : gr55xx_ll_aes.h
- ll_aes_set_key_size() : gr55xx_ll_aes.h
- ll_aes_set_key_type() : gr55xx_ll_aes.h
- ll_aes_set_load_seed() : gr55xx_ll_aes.h
- ll_aes_set_operation_mode() : gr55xx_ll_aes.h
- ll_aes_set_seed_Imask() : gr55xx_ll_aes.h
- ll_aes_set_seed_in() : gr55xx_ll_aes.h
- ll_aes_set_seed_Osbox() : gr55xx_ll_aes.h
- ll_aes_set_seed_out() : gr55xx_ll_aes.h
- ll_aes_set_vector_127_96() : gr55xx_ll_aes.h
- ll_aes_set_vector_31_0() : gr55xx_ll_aes.h
- ll_aes_set_vector_63_32() : gr55xx_ll_aes.h
- ll_aes_set_vector_95_64() : gr55xx_ll_aes.h
- ll_aes_struct_init() : gr55xx_ll_aes.h
- ll_aon_gpio_clear_flag_it() : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_deinit() : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_disable_it() : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_disable_xo_2mhz_output() : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_enable_falling_trigger() : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_enable_high_trigger() : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_enable_it() : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_enable_low_trigger() : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_enable_rising_trigger() : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_enable_xo_2mhz_output() : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_get_mux_pin_0_7() : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_get_pin_mode() : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_get_pin_pull() : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_init() : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_is_active_flag_it() : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_is_enabled_falling_trigger() : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_is_enabled_high_trigger() : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_is_enabled_it() : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_is_enabled_low_trigger() : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_is_enabled_rising_trigger() : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_is_enabled_xo_2mhz_output() : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_is_input_pin_set() : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_is_output_pin_set() : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_read_flag_it() : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_read_input_port() : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_read_output_port() : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_reset_output_pin() : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_set_mux_pin_0_7() : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_set_output_pin() : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_set_pin_mode() : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_set_pin_pull() : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_struct_init() : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_toggle_pin() : gr55xx_ll_aon_gpio.h
- ll_aon_gpio_write_output_port() : gr55xx_ll_aon_gpio.h
- ll_aon_wdt_clear_flag_reboot() : gr55xx_ll_aon_wdt.h
- ll_aon_wdt_disable() : gr55xx_ll_aon_wdt.h
- ll_aon_wdt_enable() : gr55xx_ll_aon_wdt.h
- ll_aon_wdt_get_alarm_counter() : gr55xx_ll_aon_wdt.h
- ll_aon_wdt_get_counter() : gr55xx_ll_aon_wdt.h
- ll_aon_wdt_is_active_flag_reboot() : gr55xx_ll_aon_wdt.h
- ll_aon_wdt_is_active_flag_running() : gr55xx_ll_aon_wdt.h
- ll_aon_wdt_is_enabled() : gr55xx_ll_aon_wdt.h
- ll_aon_wdt_reload_counter() : gr55xx_ll_aon_wdt.h
- ll_aon_wdt_set_alarm_counter() : gr55xx_ll_aon_wdt.h
- ll_aon_wdt_set_reload_counter() : gr55xx_ll_aon_wdt.h
- ll_bod2_disable() : gr55xx_ll_bod.h
- ll_bod2_enable() : gr55xx_ll_bod.h
- ll_bod2_lvl_ctrl_lv_set() : gr55xx_ll_bod.h
- ll_bod_clear_flag_fedge() : gr55xx_ll_bod.h
- ll_bod_deinit() : gr55xx_ll_bod.h
- ll_bod_disable() : gr55xx_ll_bod.h
- ll_bod_disable_fedge() : gr55xx_ll_bod.h
- ll_bod_enable() : gr55xx_ll_bod.h
- ll_bod_enable_fedge() : gr55xx_ll_bod.h
- ll_bod_init() : gr55xx_ll_bod.h
- ll_bod_is_active_flag_fedge() : gr55xx_ll_bod.h
- ll_bod_static_lv_disable() : gr55xx_ll_bod.h
- ll_bod_static_lv_enable() : gr55xx_ll_bod.h
- ll_bod_struct_init() : gr55xx_ll_bod.h
- ll_calendar_clear_flag_alarm() : gr55xx_ll_calendar.h
- ll_calendar_clear_flag_wrap() : gr55xx_ll_calendar.h
- ll_calendar_disable() : gr55xx_ll_calendar.h
- ll_calendar_enable() : gr55xx_ll_calendar.h
- ll_calendar_get_alarm() : gr55xx_ll_calendar.h
- ll_calendar_get_counter() : gr55xx_ll_calendar.h
- ll_calendar_get_wrapcnt() : gr55xx_ll_calendar.h
- ll_calendar_is_active_flag_alarm() : gr55xx_ll_calendar.h
- ll_calendar_is_active_flag_wrap() : gr55xx_ll_calendar.h
- ll_calendar_is_enabled() : gr55xx_ll_calendar.h
- ll_calendar_it_disable_alarm() : gr55xx_ll_calendar.h
- ll_calendar_it_disable_wrap() : gr55xx_ll_calendar.h
- ll_calendar_it_enable_alarm() : gr55xx_ll_calendar.h
- ll_calendar_it_enable_wrap() : gr55xx_ll_calendar.h
- ll_calendar_it_is_enabled_alarm() : gr55xx_ll_calendar.h
- ll_calendar_it_is_enabled_wrap() : gr55xx_ll_calendar.h
- ll_calendar_reload_alarm() : gr55xx_ll_calendar.h
- ll_calendar_reload_counter() : gr55xx_ll_calendar.h
- ll_calendar_set_clock_div() : gr55xx_ll_calendar.h
- ll_cgc_deinit() : gr55xx_ll_cgc.h
- ll_cgc_disable_force_off_aon_mcusub_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_force_off_apb_sub_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_force_off_ble_brg_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_force_off_dma_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_force_off_gpio_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_force_off_htb_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_force_off_i2c0_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_force_off_i2c1_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_force_off_i2s_m_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_force_off_i2s_s_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_force_off_pwm_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_force_off_qspi0_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_force_off_qspi1_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_force_off_rom_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_force_off_secu_div4_pclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_force_off_secu_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_force_off_serial_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_force_off_sim_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_force_off_snsadc_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_force_off_spim_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_force_off_spis_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_force_off_sram_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_force_off_uart0_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_force_off_uart1_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_force_off_xqspi_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_wfi_off_aon_mcusub_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_wfi_off_apb_sub_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_wfi_off_ble_brg_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_wfi_off_dma_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_wfi_off_gpio_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_wfi_off_htb_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_wfi_off_i2s_s_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_wfi_off_pwm_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_wfi_off_rom_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_wfi_off_secu_div4_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_wfi_off_secu_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_wfi_off_serial_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_wfi_off_sim_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_wfi_off_snsadc_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_wfi_off_sram_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_wfi_off_xqspi_div4_hclk() : gr55xx_ll_cgc.h
- ll_cgc_disable_wfi_off_xqspi_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_force_off_aon_mcusub_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_force_off_apb_sub_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_force_off_ble_brg_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_force_off_dma_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_force_off_gpio_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_force_off_htb_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_force_off_i2c0_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_force_off_i2c1_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_force_off_i2s_m_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_force_off_i2s_s_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_force_off_pwm_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_force_off_qspi0_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_force_off_qspi1_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_force_off_rom_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_force_off_secu_div4_pclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_force_off_secu_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_force_off_serial_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_force_off_sim_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_force_off_snsadc_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_force_off_spim_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_force_off_spis_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_force_off_sram_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_force_off_uart0_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_force_off_uart1_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_force_off_xqspi_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_wfi_off_aon_mcusub_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_wfi_off_apb_sub_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_wfi_off_ble_brg_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_wfi_off_dma_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_wfi_off_gpio_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_wfi_off_htb_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_wfi_off_i2s_s_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_wfi_off_pwm_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_wfi_off_rom_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_wfi_off_secu_div4_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_wfi_off_secu_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_wfi_off_serial_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_wfi_off_sim_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_wfi_off_snsadc_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_wfi_off_sram_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_wfi_off_xqspi_div4_hclk() : gr55xx_ll_cgc.h
- ll_cgc_enable_wfi_off_xqspi_hclk() : gr55xx_ll_cgc.h
- ll_cgc_get_force_off_hclk_0() : gr55xx_ll_cgc.h
- ll_cgc_get_force_off_hclk_1() : gr55xx_ll_cgc.h
- ll_cgc_get_force_off_hclk_2() : gr55xx_ll_cgc.h
- ll_cgc_get_wfi_off_hclk_0() : gr55xx_ll_cgc.h
- ll_cgc_get_wfi_off_hclk_1() : gr55xx_ll_cgc.h
- ll_cgc_get_wfi_off_hclk_2() : gr55xx_ll_cgc.h
- ll_cgc_init() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_force_off_aon_mcusub_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_force_off_apb_sub_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_force_off_ble_brg_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_force_off_dma_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_force_off_gpio_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_force_off_htb_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_force_off_i2c0_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_force_off_i2c1_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_force_off_i2s_m_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_force_off_i2s_s_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_force_off_pwm_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_force_off_qspi0_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_force_off_qspi1_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_force_off_rom_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_force_off_secu_div4_pclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_force_off_secu_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_force_off_serial_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_force_off_sim_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_force_off_snsadc_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_force_off_spim_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_force_off_spis_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_force_off_sram_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_force_off_uart0_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_force_off_uart1_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_force_off_xqspi_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_wfi_off_aon_mcusub_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_wfi_off_apb_sub_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_wfi_off_ble_brg_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_wfi_off_dma_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_wfi_off_gpio_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_wfi_off_htb_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_wfi_off_i2s_s_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_wfi_off_pwm_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_wfi_off_rom_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_wfi_off_secu_div4_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_wfi_off_secu_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_wfi_off_serial_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_wfi_off_sim_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_wfi_off_snsadc_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_wfi_off_sram_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_wfi_off_xqspi_div4_hclk() : gr55xx_ll_cgc.h
- ll_cgc_is_enabled_wfi_off_xqspi_hclk() : gr55xx_ll_cgc.h
- ll_cgc_set_force_off_hclk_0() : gr55xx_ll_cgc.h
- ll_cgc_set_force_off_hclk_1() : gr55xx_ll_cgc.h
- ll_cgc_set_force_off_hclk_2() : gr55xx_ll_cgc.h
- ll_cgc_set_wfi_off_hclk_0() : gr55xx_ll_cgc.h
- ll_cgc_set_wfi_off_hclk_1() : gr55xx_ll_cgc.h
- ll_cgc_set_wfi_off_hclk_2() : gr55xx_ll_cgc.h
- ll_cgc_struct_init() : gr55xx_ll_cgc.h
- ll_comp_clear_flag_it() : gr55xx_ll_comp.h
- ll_comp_deinit() : gr55xx_ll_comp.h
- ll_comp_disable() : gr55xx_ll_comp.h
- ll_comp_enable() : gr55xx_ll_comp.h
- ll_comp_init() : gr55xx_ll_comp.h
- ll_comp_is_active_flag_it() : gr55xx_ll_comp.h
- ll_comp_set_input_src() : gr55xx_ll_comp.h
- ll_comp_set_ref_src() : gr55xx_ll_comp.h
- ll_comp_set_vbatt_lvl() : gr55xx_ll_comp.h
- ll_comp_set_vref_lvl() : gr55xx_ll_comp.h
- ll_comp_struct_init() : gr55xx_ll_comp.h
- ll_dma_clear_flag_blk() : gr55xx_ll_dma.h
- ll_dma_clear_flag_blk0() : gr55xx_ll_dma.h
- ll_dma_clear_flag_blk1() : gr55xx_ll_dma.h
- ll_dma_clear_flag_blk2() : gr55xx_ll_dma.h
- ll_dma_clear_flag_blk3() : gr55xx_ll_dma.h
- ll_dma_clear_flag_blk4() : gr55xx_ll_dma.h
- ll_dma_clear_flag_blk5() : gr55xx_ll_dma.h
- ll_dma_clear_flag_blk6() : gr55xx_ll_dma.h
- ll_dma_clear_flag_blk7() : gr55xx_ll_dma.h
- ll_dma_clear_flag_dstt() : gr55xx_ll_dma.h
- ll_dma_clear_flag_dstt0() : gr55xx_ll_dma.h
- ll_dma_clear_flag_dstt1() : gr55xx_ll_dma.h
- ll_dma_clear_flag_dstt2() : gr55xx_ll_dma.h
- ll_dma_clear_flag_dstt3() : gr55xx_ll_dma.h
- ll_dma_clear_flag_dstt4() : gr55xx_ll_dma.h
- ll_dma_clear_flag_dstt5() : gr55xx_ll_dma.h
- ll_dma_clear_flag_dstt6() : gr55xx_ll_dma.h
- ll_dma_clear_flag_dstt7() : gr55xx_ll_dma.h
- ll_dma_clear_flag_err() : gr55xx_ll_dma.h
- ll_dma_clear_flag_err0() : gr55xx_ll_dma.h
- ll_dma_clear_flag_err1() : gr55xx_ll_dma.h
- ll_dma_clear_flag_err2() : gr55xx_ll_dma.h
- ll_dma_clear_flag_err3() : gr55xx_ll_dma.h
- ll_dma_clear_flag_err4() : gr55xx_ll_dma.h
- ll_dma_clear_flag_err5() : gr55xx_ll_dma.h
- ll_dma_clear_flag_err6() : gr55xx_ll_dma.h
- ll_dma_clear_flag_err7() : gr55xx_ll_dma.h
- ll_dma_clear_flag_srct() : gr55xx_ll_dma.h
- ll_dma_clear_flag_srct0() : gr55xx_ll_dma.h
- ll_dma_clear_flag_srct1() : gr55xx_ll_dma.h
- ll_dma_clear_flag_srct2() : gr55xx_ll_dma.h
- ll_dma_clear_flag_srct3() : gr55xx_ll_dma.h
- ll_dma_clear_flag_srct4() : gr55xx_ll_dma.h
- ll_dma_clear_flag_srct5() : gr55xx_ll_dma.h
- ll_dma_clear_flag_srct6() : gr55xx_ll_dma.h
- ll_dma_clear_flag_srct7() : gr55xx_ll_dma.h
- ll_dma_clear_flag_tfr() : gr55xx_ll_dma.h
- ll_dma_clear_flag_tfr0() : gr55xx_ll_dma.h
- ll_dma_clear_flag_tfr1() : gr55xx_ll_dma.h
- ll_dma_clear_flag_tfr2() : gr55xx_ll_dma.h
- ll_dma_clear_flag_tfr3() : gr55xx_ll_dma.h
- ll_dma_clear_flag_tfr4() : gr55xx_ll_dma.h
- ll_dma_clear_flag_tfr5() : gr55xx_ll_dma.h
- ll_dma_clear_flag_tfr6() : gr55xx_ll_dma.h
- ll_dma_clear_flag_tfr7() : gr55xx_ll_dma.h
- ll_dma_config_address() : gr55xx_ll_dma.h
- ll_dma_config_transfer() : gr55xx_ll_dma.h
- ll_dma_deinit() : gr55xx_ll_dma.h
- ll_dma_disable() : gr55xx_ll_dma.h
- ll_dma_disable_channel() : gr55xx_ll_dma.h
- ll_dma_disable_it() : gr55xx_ll_dma.h
- ll_dma_disable_it_blk() : gr55xx_ll_dma.h
- ll_dma_disable_it_dstt() : gr55xx_ll_dma.h
- ll_dma_disable_it_err() : gr55xx_ll_dma.h
- ll_dma_disable_it_srct() : gr55xx_ll_dma.h
- ll_dma_disable_it_tfr() : gr55xx_ll_dma.h
- ll_dma_enable() : gr55xx_ll_dma.h
- ll_dma_enable_channel() : gr55xx_ll_dma.h
- ll_dma_enable_it() : gr55xx_ll_dma.h
- ll_dma_enable_it_blk() : gr55xx_ll_dma.h
- ll_dma_enable_it_dstt() : gr55xx_ll_dma.h
- ll_dma_enable_it_err() : gr55xx_ll_dma.h
- ll_dma_enable_it_srct() : gr55xx_ll_dma.h
- ll_dma_enable_it_tfr() : gr55xx_ll_dma.h
- ll_dma_get_block_size() : gr55xx_ll_dma.h
- ll_dma_get_channel_priority_level() : gr55xx_ll_dma.h
- ll_dma_get_data_transfer_direction() : gr55xx_ll_dma.h
- ll_dma_get_destination_address() : gr55xx_ll_dma.h
- ll_dma_get_destination_burst_length() : gr55xx_ll_dma.h
- ll_dma_get_destination_increment_mode() : gr55xx_ll_dma.h
- ll_dma_get_destination_peripheral() : gr55xx_ll_dma.h
- ll_dma_get_destination_width() : gr55xx_ll_dma.h
- ll_dma_get_m2m_dst_address() : gr55xx_ll_dma.h
- ll_dma_get_m2m_src_address() : gr55xx_ll_dma.h
- ll_dma_get_mode() : gr55xx_ll_dma.h
- ll_dma_get_source_address() : gr55xx_ll_dma.h
- ll_dma_get_source_burst_length() : gr55xx_ll_dma.h
- ll_dma_get_source_increment_mode() : gr55xx_ll_dma.h
- ll_dma_get_source_peripheral() : gr55xx_ll_dma.h
- ll_dma_get_source_width() : gr55xx_ll_dma.h
- ll_dma_init() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_blk() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_blk0() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_blk1() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_blk2() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_blk3() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_blk4() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_blk5() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_blk6() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_blk7() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_dstt() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_dstt0() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_dstt1() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_dstt2() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_dstt3() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_dstt4() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_dstt5() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_dstt6() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_dstt7() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_err() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_err0() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_err1() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_err2() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_err3() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_err4() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_err5() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_err6() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_err7() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_gblk() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_gdstt() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_gerr() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_gsrct() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_gtfr() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_rblk() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_rdstt() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_rerr() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_rsrct() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_rtfr() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_srct() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_srct0() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_srct1() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_srct2() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_srct3() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_srct4() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_srct5() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_srct6() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_srct7() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_tfr() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_tfr0() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_tfr1() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_tfr2() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_tfr3() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_tfr4() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_tfr5() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_tfr6() : gr55xx_ll_dma.h
- ll_dma_is_active_flag_tfr7() : gr55xx_ll_dma.h
- ll_dma_is_empty_fifo() : gr55xx_ll_dma.h
- ll_dma_is_enable() : gr55xx_ll_dma.h
- ll_dma_is_enable_it_blk() : gr55xx_ll_dma.h
- ll_dma_is_enable_it_dstt() : gr55xx_ll_dma.h
- ll_dma_is_enable_it_err() : gr55xx_ll_dma.h
- ll_dma_is_enable_it_srct() : gr55xx_ll_dma.h
- ll_dma_is_enable_it_tfr() : gr55xx_ll_dma.h
- ll_dma_is_enabled_channel() : gr55xx_ll_dma.h
- ll_dma_is_suspended() : gr55xx_ll_dma.h
- ll_dma_req_dst_burst_transaction() : gr55xx_ll_dma.h
- ll_dma_req_dst_last_burst_transaction() : gr55xx_ll_dma.h
- ll_dma_req_dst_last_single_transaction() : gr55xx_ll_dma.h
- ll_dma_req_dst_single_transaction() : gr55xx_ll_dma.h
- ll_dma_req_src_burst_transaction() : gr55xx_ll_dma.h
- ll_dma_req_src_last_burst_transaction() : gr55xx_ll_dma.h
- ll_dma_req_src_last_single_transaction() : gr55xx_ll_dma.h
- ll_dma_req_src_single_transaction() : gr55xx_ll_dma.h
- ll_dma_resume_channel() : gr55xx_ll_dma.h
- ll_dma_select_handshaking() : gr55xx_ll_dma.h
- ll_dma_set_block_size() : gr55xx_ll_dma.h
- ll_dma_set_channel_priority_level() : gr55xx_ll_dma.h
- ll_dma_set_data_transfer_direction() : gr55xx_ll_dma.h
- ll_dma_set_destination_address() : gr55xx_ll_dma.h
- ll_dma_set_destination_burst_length() : gr55xx_ll_dma.h
- ll_dma_set_destination_increment_mode() : gr55xx_ll_dma.h
- ll_dma_set_destination_peripheral() : gr55xx_ll_dma.h
- ll_dma_set_destination_width() : gr55xx_ll_dma.h
- ll_dma_set_m2m_dst_address() : gr55xx_ll_dma.h
- ll_dma_set_m2m_src_address() : gr55xx_ll_dma.h
- ll_dma_set_mode() : gr55xx_ll_dma.h
- ll_dma_set_source_address() : gr55xx_ll_dma.h
- ll_dma_set_source_burst_length() : gr55xx_ll_dma.h
- ll_dma_set_source_increment_mode() : gr55xx_ll_dma.h
- ll_dma_set_source_peripheral() : gr55xx_ll_dma.h
- ll_dma_set_source_width() : gr55xx_ll_dma.h
- ll_dma_struct_init() : gr55xx_ll_dma.h
- ll_dma_suspend_channel() : gr55xx_ll_dma.h
- ll_dual_timer_clear_flag_it() : gr55xx_ll_dual_tim.h
- ll_dual_timer_deinit() : gr55xx_ll_dual_tim.h
- ll_dual_timer_disable_counter() : gr55xx_ll_dual_tim.h
- ll_dual_timer_disable_it() : gr55xx_ll_dual_tim.h
- ll_dual_timer_disable_oneshot() : gr55xx_ll_dual_tim.h
- ll_dual_timer_enable_counter() : gr55xx_ll_dual_tim.h
- ll_dual_timer_enable_it() : gr55xx_ll_dual_tim.h
- ll_dual_timer_enable_oneshot() : gr55xx_ll_dual_tim.h
- ll_dual_timer_get_auto_reload() : gr55xx_ll_dual_tim.h
- ll_dual_timer_get_background_reload() : gr55xx_ll_dual_tim.h
- ll_dual_timer_get_counter() : gr55xx_ll_dual_tim.h
- ll_dual_timer_get_counter_mode() : gr55xx_ll_dual_tim.h
- ll_dual_timer_get_counter_size() : gr55xx_ll_dual_tim.h
- ll_dual_timer_get_prescaler() : gr55xx_ll_dual_tim.h
- ll_dual_timer_get_raw_it_flag() : gr55xx_ll_dual_tim.h
- ll_dual_timer_init() : gr55xx_ll_dual_tim.h
- ll_dual_timer_is_active_flag_it() : gr55xx_ll_dual_tim.h
- ll_dual_timer_is_enabled_counter() : gr55xx_ll_dual_tim.h
- ll_dual_timer_is_enabled_it() : gr55xx_ll_dual_tim.h
- ll_dual_timer_is_enabled_oneshot() : gr55xx_ll_dual_tim.h
- ll_dual_timer_set_auto_reload() : gr55xx_ll_dual_tim.h
- ll_dual_timer_set_background_reload() : gr55xx_ll_dual_tim.h
- ll_dual_timer_set_counter_mode() : gr55xx_ll_dual_tim.h
- ll_dual_timer_set_counter_size() : gr55xx_ll_dual_tim.h
- ll_dual_timer_set_prescaler() : gr55xx_ll_dual_tim.h
- ll_dual_timer_struct_init() : gr55xx_ll_dual_tim.h
- ll_efuse_disable_controller_power() : gr55xx_ll_efuse.h
- ll_efuse_disable_main_backup() : gr55xx_ll_efuse.h
- ll_efuse_disable_pgenb() : gr55xx_ll_efuse.h
- ll_efuse_disable_power() : gr55xx_ll_efuse.h
- ll_efuse_enable_controller_power_begin() : gr55xx_ll_efuse.h
- ll_efuse_enable_controller_power_stop() : gr55xx_ll_efuse.h
- ll_efuse_enable_main_backup() : gr55xx_ll_efuse.h
- ll_efuse_enable_pgenb() : gr55xx_ll_efuse.h
- ll_efuse_enable_power() : gr55xx_ll_efuse.h
- ll_efuse_get_crc_check_addr() : gr55xx_ll_efuse.h
- ll_efuse_get_crc_check_len() : gr55xx_ll_efuse.h
- ll_efuse_get_crc_check_result() : gr55xx_ll_efuse.h
- ll_efuse_get_interval() : gr55xx_ll_efuse.h
- ll_efuse_get_key_mask() : gr55xx_ll_efuse.h
- ll_efuse_get_test_mode() : gr55xx_ll_efuse.h
- ll_efuse_get_tpro() : gr55xx_ll_efuse.h
- ll_efuse_get_trim_addr() : gr55xx_ll_efuse.h
- ll_efuse_get_trim_length() : gr55xx_ll_efuse.h
- ll_efuse_get_trim_value() : gr55xx_ll_efuse.h
- ll_efuse_is_active_flag() : gr55xx_ll_efuse.h
- ll_efuse_is_controller_power_flag() : gr55xx_ll_efuse.h
- ll_efuse_is_enabled_main_backup() : gr55xx_ll_efuse.h
- ll_efuse_is_enabled_pgenb() : gr55xx_ll_efuse.h
- ll_efuse_set_controller_power_timing() : gr55xx_ll_efuse.h
- ll_efuse_set_crc_check_addr() : gr55xx_ll_efuse.h
- ll_efuse_set_crc_check_len() : gr55xx_ll_efuse.h
- ll_efuse_set_interval() : gr55xx_ll_efuse.h
- ll_efuse_set_key_mask() : gr55xx_ll_efuse.h
- ll_efuse_set_operation() : gr55xx_ll_efuse.h
- ll_efuse_set_tpro() : gr55xx_ll_efuse.h
- ll_efuse_set_trim_addr() : gr55xx_ll_efuse.h
- ll_efuse_set_trim_length() : gr55xx_ll_efuse.h
- ll_gpio_clear_flag_it() : gr55xx_ll_gpio.h
- ll_gpio_deinit() : gr55xx_ll_gpio.h
- ll_gpio_disable_it() : gr55xx_ll_gpio.h
- ll_gpio_enable_falling_trigger() : gr55xx_ll_gpio.h
- ll_gpio_enable_high_trigger() : gr55xx_ll_gpio.h
- ll_gpio_enable_it() : gr55xx_ll_gpio.h
- ll_gpio_enable_low_trigger() : gr55xx_ll_gpio.h
- ll_gpio_enable_rising_trigger() : gr55xx_ll_gpio.h
- ll_gpio_get_mux_pin_0_7() : gr55xx_ll_gpio.h
- ll_gpio_get_mux_pin_8_15() : gr55xx_ll_gpio.h
- ll_gpio_get_pin_mode() : gr55xx_ll_gpio.h
- ll_gpio_get_pin_pull() : gr55xx_ll_gpio.h
- ll_gpio_init() : gr55xx_ll_gpio.h
- ll_gpio_is_active_flag_it() : gr55xx_ll_gpio.h
- ll_gpio_is_enabled_falling_trigger() : gr55xx_ll_gpio.h
- ll_gpio_is_enabled_high_trigger() : gr55xx_ll_gpio.h
- ll_gpio_is_enabled_it() : gr55xx_ll_gpio.h
- ll_gpio_is_enabled_low_trigger() : gr55xx_ll_gpio.h
- ll_gpio_is_enabled_rising_trigger() : gr55xx_ll_gpio.h
- ll_gpio_is_input_pin_set() : gr55xx_ll_gpio.h
- ll_gpio_is_output_pin_set() : gr55xx_ll_gpio.h
- ll_gpio_read_flag_it() : gr55xx_ll_gpio.h
- ll_gpio_read_input_port() : gr55xx_ll_gpio.h
- ll_gpio_read_output_port() : gr55xx_ll_gpio.h
- ll_gpio_reset_output_pin() : gr55xx_ll_gpio.h
- ll_gpio_set_mux_pin_0_7() : gr55xx_ll_gpio.h
- ll_gpio_set_mux_pin_8_15() : gr55xx_ll_gpio.h
- ll_gpio_set_output_pin() : gr55xx_ll_gpio.h
- ll_gpio_set_pin_mode() : gr55xx_ll_gpio.h
- ll_gpio_set_pin_pull() : gr55xx_ll_gpio.h
- ll_gpio_struct_init() : gr55xx_ll_gpio.h
- ll_gpio_toggle_pin() : gr55xx_ll_gpio.h
- ll_gpio_write_output_port() : gr55xx_ll_gpio.h
- ll_hmac_clear_flag_it_done() : gr55xx_ll_hmac.h
- ll_hmac_deinit() : gr55xx_ll_hmac.h
- ll_hmac_disable() : gr55xx_ll_hmac.h
- ll_hmac_disable_dma_start() : gr55xx_ll_hmac.h
- ll_hmac_disable_it_done() : gr55xx_ll_hmac.h
- ll_hmac_disable_little_endian() : gr55xx_ll_hmac.h
- ll_hmac_disable_private() : gr55xx_ll_hmac.h
- ll_hmac_disable_sha() : gr55xx_ll_hmac.h
- ll_hmac_disable_user_hash() : gr55xx_ll_hmac.h
- ll_hmac_enable() : gr55xx_ll_hmac.h
- ll_hmac_enable_dma_start() : gr55xx_ll_hmac.h
- ll_hmac_enable_it_done() : gr55xx_ll_hmac.h
- ll_hmac_enable_last_transfer() : gr55xx_ll_hmac.h
- ll_hmac_enable_little_endian() : gr55xx_ll_hmac.h
- ll_hmac_enable_private() : gr55xx_ll_hmac.h
- ll_hmac_enable_read_key() : gr55xx_ll_hmac.h
- ll_hmac_enable_sha() : gr55xx_ll_hmac.h
- ll_hmac_enable_user_hash() : gr55xx_ll_hmac.h
- ll_hmac_get_data() : gr55xx_ll_hmac.h
- ll_hmac_get_dma_read_address() : gr55xx_ll_hmac.h
- ll_hmac_get_dma_transfer_block() : gr55xx_ll_hmac.h
- ll_hmac_get_dma_write_address() : gr55xx_ll_hmac.h
- ll_hmac_get_key_address() : gr55xx_ll_hmac.h
- ll_hmac_get_key_type() : gr55xx_ll_hmac.h
- ll_hmac_init() : gr55xx_ll_hmac.h
- ll_hmac_is_action_flag_dma_done() : gr55xx_ll_hmac.h
- ll_hmac_is_action_flag_dma_error() : gr55xx_ll_hmac.h
- ll_hmac_is_action_flag_dma_message_done() : gr55xx_ll_hmac.h
- ll_hmac_is_action_flag_hmac_ready() : gr55xx_ll_hmac.h
- ll_hmac_is_action_flag_it_done() : gr55xx_ll_hmac.h
- ll_hmac_is_action_flag_key_valid() : gr55xx_ll_hmac.h
- ll_hmac_is_action_flag_sha_ready() : gr55xx_ll_hmac.h
- ll_hmac_is_enabled() : gr55xx_ll_hmac.h
- ll_hmac_is_enabled_dma_start() : gr55xx_ll_hmac.h
- ll_hmac_is_enabled_it_done() : gr55xx_ll_hmac.h
- ll_hmac_is_enabled_little_endian() : gr55xx_ll_hmac.h
- ll_hmac_is_enabled_private() : gr55xx_ll_hmac.h
- ll_hmac_is_enabled_sha() : gr55xx_ll_hmac.h
- ll_hmac_is_enabled_user_hash() : gr55xx_ll_hmac.h
- ll_hmac_set_data() : gr55xx_ll_hmac.h
- ll_hmac_set_dma_read_address() : gr55xx_ll_hmac.h
- ll_hmac_set_dma_transfer_block() : gr55xx_ll_hmac.h
- ll_hmac_set_dma_write_address() : gr55xx_ll_hmac.h
- ll_hmac_set_key0() : gr55xx_ll_hmac.h
- ll_hmac_set_key1() : gr55xx_ll_hmac.h
- ll_hmac_set_key2() : gr55xx_ll_hmac.h
- ll_hmac_set_key3() : gr55xx_ll_hmac.h
- ll_hmac_set_key4() : gr55xx_ll_hmac.h
- ll_hmac_set_key5() : gr55xx_ll_hmac.h
- ll_hmac_set_key6() : gr55xx_ll_hmac.h
- ll_hmac_set_key7() : gr55xx_ll_hmac.h
- ll_hmac_set_key_address() : gr55xx_ll_hmac.h
- ll_hmac_set_key_port_mask() : gr55xx_ll_hmac.h
- ll_hmac_set_key_type() : gr55xx_ll_hmac.h
- ll_hmac_set_user_hash_127_96() : gr55xx_ll_hmac.h
- ll_hmac_set_user_hash_159_128() : gr55xx_ll_hmac.h
- ll_hmac_set_user_hash_191_160() : gr55xx_ll_hmac.h
- ll_hmac_set_user_hash_223_192() : gr55xx_ll_hmac.h
- ll_hmac_set_user_hash_255_224() : gr55xx_ll_hmac.h
- ll_hmac_set_user_hash_31_0() : gr55xx_ll_hmac.h
- ll_hmac_set_user_hash_63_32() : gr55xx_ll_hmac.h
- ll_hmac_set_user_hash_95_64() : gr55xx_ll_hmac.h
- ll_hmac_struct_init() : gr55xx_ll_hmac.h
- ll_i2c_clear_flag_activity() : gr55xx_ll_i2c.h
- ll_i2c_clear_flag_gen_call() : gr55xx_ll_i2c.h
- ll_i2c_clear_flag_intr() : gr55xx_ll_i2c.h
- ll_i2c_clear_flag_read_req() : gr55xx_ll_i2c.h
- ll_i2c_clear_flag_rx_done() : gr55xx_ll_i2c.h
- ll_i2c_clear_flag_rx_over() : gr55xx_ll_i2c.h
- ll_i2c_clear_flag_rx_under() : gr55xx_ll_i2c.h
- ll_i2c_clear_flag_start_det() : gr55xx_ll_i2c.h
- ll_i2c_clear_flag_stop_det() : gr55xx_ll_i2c.h
- ll_i2c_clear_flag_tx_abort() : gr55xx_ll_i2c.h
- ll_i2c_clear_flag_tx_over() : gr55xx_ll_i2c.h
- ll_i2c_deinit() : gr55xx_ll_i2c.h
- ll_i2c_disable() : gr55xx_ll_i2c.h
- ll_i2c_disable_dma_req_rx() : gr55xx_ll_i2c.h
- ll_i2c_disable_dma_req_tx() : gr55xx_ll_i2c.h
- ll_i2c_disable_general_call() : gr55xx_ll_i2c.h
- ll_i2c_disable_it() : gr55xx_ll_i2c.h
- ll_i2c_disable_it_activity() : gr55xx_ll_i2c.h
- ll_i2c_disable_it_gen_call() : gr55xx_ll_i2c.h
- ll_i2c_disable_it_master_om_hold() : gr55xx_ll_i2c.h
- ll_i2c_disable_it_read_req() : gr55xx_ll_i2c.h
- ll_i2c_disable_it_restart_det() : gr55xx_ll_i2c.h
- ll_i2c_disable_it_rx_done() : gr55xx_ll_i2c.h
- ll_i2c_disable_it_rx_over() : gr55xx_ll_i2c.h
- ll_i2c_disable_it_rx_under() : gr55xx_ll_i2c.h
- ll_i2c_disable_it_start_det() : gr55xx_ll_i2c.h
- ll_i2c_disable_it_stop_det() : gr55xx_ll_i2c.h
- ll_i2c_disable_it_tx_abort() : gr55xx_ll_i2c.h
- ll_i2c_disable_it_tx_empty() : gr55xx_ll_i2c.h
- ll_i2c_disable_it_tx_over() : gr55xx_ll_i2c.h
- ll_i2c_disable_master_mode() : gr55xx_ll_i2c.h
- ll_i2c_disable_master_restart() : gr55xx_ll_i2c.h
- ll_i2c_disable_stop_det_if_addressed() : gr55xx_ll_i2c.h
- ll_i2c_disbale_it_rx_full() : gr55xx_ll_i2c.h
- ll_i2c_dma_get_register_address() : gr55xx_ll_i2c.h
- ll_i2c_enable() : gr55xx_ll_i2c.h
- ll_i2c_enable_dma_req_rx() : gr55xx_ll_i2c.h
- ll_i2c_enable_dma_req_tx() : gr55xx_ll_i2c.h
- ll_i2c_enable_general_call() : gr55xx_ll_i2c.h
- ll_i2c_enable_it() : gr55xx_ll_i2c.h
- ll_i2c_enable_it_activity() : gr55xx_ll_i2c.h
- ll_i2c_enable_it_gen_call() : gr55xx_ll_i2c.h
- ll_i2c_enable_it_master_on_hold() : gr55xx_ll_i2c.h
- ll_i2c_enable_it_read_req() : gr55xx_ll_i2c.h
- ll_i2c_enable_it_restart_det() : gr55xx_ll_i2c.h
- ll_i2c_enable_it_rx_abort() : gr55xx_ll_i2c.h
- ll_i2c_enable_it_rx_done() : gr55xx_ll_i2c.h
- ll_i2c_enable_it_rx_full() : gr55xx_ll_i2c.h
- ll_i2c_enable_it_rx_over() : gr55xx_ll_i2c.h
- ll_i2c_enable_it_rx_under() : gr55xx_ll_i2c.h
- ll_i2c_enable_it_start_det() : gr55xx_ll_i2c.h
- ll_i2c_enable_it_stop_det() : gr55xx_ll_i2c.h
- ll_i2c_enable_it_tx_empty() : gr55xx_ll_i2c.h
- ll_i2c_enable_it_tx_over() : gr55xx_ll_i2c.h
- ll_i2c_enable_master_mode() : gr55xx_ll_i2c.h
- ll_i2c_enable_master_restart() : gr55xx_ll_i2c.h
- ll_i2c_enable_stop_det_if_addressed() : gr55xx_ll_i2c.h
- ll_i2c_enable_transfer_abort() : gr55xx_ll_i2c.h
- ll_i2c_get_abort_source() : gr55xx_ll_i2c.h
- ll_i2c_get_clock_high_period_fs() : gr55xx_ll_i2c.h
- ll_i2c_get_clock_high_period_hs() : gr55xx_ll_i2c.h
- ll_i2c_get_clock_high_period_ss() : gr55xx_ll_i2c.h
- ll_i2c_get_clock_low_period_fs() : gr55xx_ll_i2c.h
- ll_i2c_get_clock_low_period_hs() : gr55xx_ll_i2c.h
- ll_i2c_get_clock_low_period_ss() : gr55xx_ll_i2c.h
- ll_i2c_get_data_rx_hold_time() : gr55xx_ll_i2c.h
- ll_i2c_get_data_setup_time() : gr55xx_ll_i2c.h
- ll_i2c_get_data_tx_hold_time() : gr55xx_ll_i2c.h
- ll_i2c_get_dma_rx_data_level() : gr55xx_ll_i2c.h
- ll_i2c_get_dma_tx_data_level() : gr55xx_ll_i2c.h
- ll_i2c_get_high_speed_master_code() : gr55xx_ll_i2c.h
- ll_i2c_get_it_flag() : gr55xx_ll_i2c.h
- ll_i2c_get_master_addressing_mode() : gr55xx_ll_i2c.h
- ll_i2c_get_raw_it_flag() : gr55xx_ll_i2c.h
- ll_i2c_get_rx_fifo_level() : gr55xx_ll_i2c.h
- ll_i2c_get_rx_fifo_threshold() : gr55xx_ll_i2c.h
- ll_i2c_get_slave_address() : gr55xx_ll_i2c.h
- ll_i2c_get_speed_mode() : gr55xx_ll_i2c.h
- ll_i2c_get_spike_len_fs() : gr55xx_ll_i2c.h
- ll_i2c_get_spike_len_hs() : gr55xx_ll_i2c.h
- ll_i2c_get_transfer_direction() : gr55xx_ll_i2c.h
- ll_i2c_get_tx_fifo_level() : gr55xx_ll_i2c.h
- ll_i2c_get_tx_fifo_threshold() : gr55xx_ll_i2c.h
- ll_i2c_get_tx_flush_count() : gr55xx_ll_i2c.h
- ll_i2c_handle_transfer() : gr55xx_ll_i2c.h
- ll_i2c_init() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_activity() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_gen_call() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_master_on_hold() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_raw_activity() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_raw_gen_call() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_raw_master_on_hold() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_raw_read_req() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_raw_restart_det() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_raw_rx_done() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_raw_rx_full() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_raw_rx_over() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_raw_rx_under() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_raw_start_det() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_raw_stop_det() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_raw_tx_abort() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_raw_tx_empty() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_raw_tx_over() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_read_req() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_restart_det() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_rx_done() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_rx_full() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_rx_over() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_rx_under() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_slave_dis_whl_busy() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_slave_rx_data_lost() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_start_det() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_status_activity() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_status_master_activity() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_status_rff() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_status_rfne() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_status_slave_activity() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_status_tfe() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_status_tfnf() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_stop_det() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_tx_abort() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_tx_empty() : gr55xx_ll_i2c.h
- ll_i2c_is_active_flag_tx_over() : gr55xx_ll_i2c.h
- ll_i2c_is_enable_it_rx_done() : gr55xx_ll_i2c.h
- ll_i2c_is_enabled() : gr55xx_ll_i2c.h
- ll_i2c_is_enabled_dma_req_rx() : gr55xx_ll_i2c.h
- ll_i2c_is_enabled_dma_req_tx() : gr55xx_ll_i2c.h
- ll_i2c_is_enabled_general_call() : gr55xx_ll_i2c.h
- ll_i2c_is_enabled_it() : gr55xx_ll_i2c.h
- ll_i2c_is_enabled_it_activity() : gr55xx_ll_i2c.h
- ll_i2c_is_enabled_it_gen_call() : gr55xx_ll_i2c.h
- ll_i2c_is_enabled_it_master_on_hold() : gr55xx_ll_i2c.h
- ll_i2c_is_enabled_it_read_req() : gr55xx_ll_i2c.h
- ll_i2c_is_enabled_it_restart_det() : gr55xx_ll_i2c.h
- ll_i2c_is_enabled_it_rx_over() : gr55xx_ll_i2c.h
- ll_i2c_is_enabled_it_rx_under() : gr55xx_ll_i2c.h
- ll_i2c_is_enabled_it_start_det() : gr55xx_ll_i2c.h
- ll_i2c_is_enabled_it_stop_det() : gr55xx_ll_i2c.h
- ll_i2c_is_enabled_it_tx_abort() : gr55xx_ll_i2c.h
- ll_i2c_is_enabled_it_tx_empty() : gr55xx_ll_i2c.h
- ll_i2c_is_enabled_it_tx_over() : gr55xx_ll_i2c.h
- ll_i2c_is_enabled_master_mode() : gr55xx_ll_i2c.h
- ll_i2c_is_enabled_master_restart() : gr55xx_ll_i2c.h
- ll_i2c_is_enabled_stop_det_if_addressed() : gr55xx_ll_i2c.h
- ll_i2c_is_enabled_transfer_abort() : gr55xx_ll_i2c.h
- ll_i2c_ls_enabled_it_rx_full() : gr55xx_ll_i2c.h
- ll_i2c_receive_data8() : gr55xx_ll_i2c.h
- ll_i2c_set_clock_high_period_fs() : gr55xx_ll_i2c.h
- ll_i2c_set_clock_high_period_hs() : gr55xx_ll_i2c.h
- ll_i2c_set_clock_high_period_ss() : gr55xx_ll_i2c.h
- ll_i2c_set_clock_low_period_fs() : gr55xx_ll_i2c.h
- ll_i2c_set_clock_low_period_hs() : gr55xx_ll_i2c.h
- ll_i2c_set_clock_low_period_ss() : gr55xx_ll_i2c.h
- ll_i2c_set_data_rx_hold_time() : gr55xx_ll_i2c.h
- ll_i2c_set_data_setup_time() : gr55xx_ll_i2c.h
- ll_i2c_set_data_tx_hold_time() : gr55xx_ll_i2c.h
- ll_i2c_set_dma_rx_data_level() : gr55xx_ll_i2c.h
- ll_i2c_set_dma_tx_data_level() : gr55xx_ll_i2c.h
- ll_i2c_set_high_speed_master_code() : gr55xx_ll_i2c.h
- ll_i2c_set_master_addressing_mode() : gr55xx_ll_i2c.h
- ll_i2c_set_own_address() : gr55xx_ll_i2c.h
- ll_i2c_set_rx_fifo_threshold() : gr55xx_ll_i2c.h
- ll_i2c_set_slave_address() : gr55xx_ll_i2c.h
- ll_i2c_set_speed_mode() : gr55xx_ll_i2c.h
- ll_i2c_set_spike_len_fs() : gr55xx_ll_i2c.h
- ll_i2c_set_spike_len_hs() : gr55xx_ll_i2c.h
- ll_i2c_set_tx_fifo_threshold() : gr55xx_ll_i2c.h
- ll_i2c_struct_init() : gr55xx_ll_i2c.h
- ll_i2c_transmit_data8() : gr55xx_ll_i2c.h
- ll_i2s_clear_it_rxovr() : gr55xx_ll_i2s.h
- ll_i2s_clear_it_txovr() : gr55xx_ll_i2s.h
- ll_i2s_clr_rxfifo_all() : gr55xx_ll_i2s.h
- ll_i2s_clr_rxfifo_channel() : gr55xx_ll_i2s.h
- ll_i2s_clr_txfifo_all() : gr55xx_ll_i2s.h
- ll_i2s_clr_txfifo_channel() : gr55xx_ll_i2s.h
- ll_i2s_deinit() : gr55xx_ll_i2s.h
- ll_i2s_disable() : gr55xx_ll_i2s.h
- ll_i2s_disable_clock() : gr55xx_ll_i2s.h
- ll_i2s_disable_clock_div() : gr55xx_ll_i2s.h
- ll_i2s_disable_dma() : gr55xx_ll_i2s.h
- ll_i2s_disable_it() : gr55xx_ll_i2s.h
- ll_i2s_disable_rx() : gr55xx_ll_i2s.h
- ll_i2s_disable_rxblock() : gr55xx_ll_i2s.h
- ll_i2s_disable_tx() : gr55xx_ll_i2s.h
- ll_i2s_disable_txblock() : gr55xx_ll_i2s.h
- ll_i2s_enable() : gr55xx_ll_i2s.h
- ll_i2s_enable_clock() : gr55xx_ll_i2s.h
- ll_i2s_enable_clock_div() : gr55xx_ll_i2s.h
- ll_i2s_enable_dma() : gr55xx_ll_i2s.h
- ll_i2s_enable_it() : gr55xx_ll_i2s.h
- ll_i2s_enable_rx() : gr55xx_ll_i2s.h
- ll_i2s_enable_rxblock() : gr55xx_ll_i2s.h
- ll_i2s_enable_tx() : gr55xx_ll_i2s.h
- ll_i2s_enable_txblock() : gr55xx_ll_i2s.h
- ll_i2s_get_apb_width() : gr55xx_ll_i2s.h
- ll_i2s_get_clock_div() : gr55xx_ll_i2s.h
- ll_i2s_get_clock_src() : gr55xx_ll_i2s.h
- ll_i2s_get_fifo_depth() : gr55xx_ll_i2s.h
- ll_i2s_get_it_flag() : gr55xx_ll_i2s.h
- ll_i2s_get_master_mode() : gr55xx_ll_i2s.h
- ll_i2s_get_rx_block() : gr55xx_ll_i2s.h
- ll_i2s_get_rx_channels() : gr55xx_ll_i2s.h
- ll_i2s_get_rx_fifo_threshold() : gr55xx_ll_i2s.h
- ll_i2s_get_rx_resolution() : gr55xx_ll_i2s.h
- ll_i2s_get_rxsize() : gr55xx_ll_i2s.h
- ll_i2s_get_sclkg() : gr55xx_ll_i2s.h
- ll_i2s_get_tx_block() : gr55xx_ll_i2s.h
- ll_i2s_get_tx_channels() : gr55xx_ll_i2s.h
- ll_i2s_get_tx_fifo_threshold() : gr55xx_ll_i2s.h
- ll_i2s_get_tx_resolution() : gr55xx_ll_i2s.h
- ll_i2s_get_txsize() : gr55xx_ll_i2s.h
- ll_i2s_get_type() : gr55xx_ll_i2s.h
- ll_i2s_get_version() : gr55xx_ll_i2s.h
- ll_i2s_get_wss() : gr55xx_ll_i2s.h
- ll_i2s_init() : gr55xx_ll_i2s.h
- ll_i2s_is_active_it_flag() : gr55xx_ll_i2s.h
- ll_i2s_is_enabled() : gr55xx_ll_i2s.h
- ll_i2s_is_enabled_clock() : gr55xx_ll_i2s.h
- ll_i2s_is_enabled_clock_div() : gr55xx_ll_i2s.h
- ll_i2s_is_enabled_dma() : gr55xx_ll_i2s.h
- ll_i2s_is_enabled_it() : gr55xx_ll_i2s.h
- ll_i2s_is_enabled_rx() : gr55xx_ll_i2s.h
- ll_i2s_is_enabled_rxblock() : gr55xx_ll_i2s.h
- ll_i2s_is_enabled_tx() : gr55xx_ll_i2s.h
- ll_i2s_is_enabled_txblock() : gr55xx_ll_i2s.h
- ll_i2s_receive_ldata() : gr55xx_ll_i2s.h
- ll_i2s_receive_rdata() : gr55xx_ll_i2s.h
- ll_i2s_rst_rxdma() : gr55xx_ll_i2s.h
- ll_i2s_rst_txdma() : gr55xx_ll_i2s.h
- ll_i2s_set_clock_div() : gr55xx_ll_i2s.h
- ll_i2s_set_clock_src() : gr55xx_ll_i2s.h
- ll_i2s_set_rx_fifo_threshold() : gr55xx_ll_i2s.h
- ll_i2s_set_rxsize() : gr55xx_ll_i2s.h
- ll_i2s_set_sclkg() : gr55xx_ll_i2s.h
- ll_i2s_set_tx_fifo_threshold() : gr55xx_ll_i2s.h
- ll_i2s_set_txsize() : gr55xx_ll_i2s.h
- ll_i2s_set_wss() : gr55xx_ll_i2s.h
- ll_i2s_struct_init() : gr55xx_ll_i2s.h
- ll_i2s_transmit_ldata() : gr55xx_ll_i2s.h
- ll_i2s_transmit_rdata() : gr55xx_ll_i2s.h
- ll_iso7816_check_card_presence() : gr55xx_ll_iso7816.h
- ll_iso7816_clear_flag_all_intr() : gr55xx_ll_iso7816.h
- ll_iso7816_clear_flag_dma_err() : gr55xx_ll_iso7816.h
- ll_iso7816_clear_flag_done() : gr55xx_ll_iso7816.h
- ll_iso7816_clear_flag_presence() : gr55xx_ll_iso7816.h
- ll_iso7816_clear_flag_retry_err() : gr55xx_ll_iso7816.h
- ll_iso7816_clear_flag_rx_err() : gr55xx_ll_iso7816.h
- ll_iso7816_clear_flag_state_err() : gr55xx_ll_iso7816.h
- ll_iso7816_clear_flag_test() : gr55xx_ll_iso7816.h
- ll_iso7816_clear_rx_retry_max() : gr55xx_ll_iso7816.h
- ll_iso7816_clear_tx_retry_max() : gr55xx_ll_iso7816.h
- ll_iso7816_deinit() : gr55xx_ll_iso7816.h
- ll_iso7816_disable_coding_detection() : gr55xx_ll_iso7816.h
- ll_iso7816_enable_coding_detection() : gr55xx_ll_iso7816.h
- ll_iso7816_get_base_addr() : gr55xx_ll_iso7816.h
- ll_iso7816_get_buffer_addr() : gr55xx_ll_iso7816.h
- ll_iso7816_get_clkdiv() : gr55xx_ll_iso7816.h
- ll_iso7816_get_clkstop_level() : gr55xx_ll_iso7816.h
- ll_iso7816_get_coding_convention() : gr55xx_ll_iso7816.h
- ll_iso7816_get_current_addr() : gr55xx_ll_iso7816.h
- ll_iso7816_get_current_addr_frac() : gr55xx_ll_iso7816.h
- ll_iso7816_get_etudiv() : gr55xx_ll_iso7816.h
- ll_iso7816_get_guardtime() : gr55xx_ll_iso7816.h
- ll_iso7816_get_io_states() : gr55xx_ll_iso7816.h
- ll_iso7816_get_it_flag() : gr55xx_ll_iso7816.h
- ll_iso7816_get_power_states() : gr55xx_ll_iso7816.h
- ll_iso7816_get_retry_limit() : gr55xx_ll_iso7816.h
- ll_iso7816_get_rx_end_addr() : gr55xx_ll_iso7816.h
- ll_iso7816_get_rx_end_addr_frac() : gr55xx_ll_iso7816.h
- ll_iso7816_get_rx_endbyte_addr() : gr55xx_ll_iso7816.h
- ll_iso7816_get_rx_retry_max() : gr55xx_ll_iso7816.h
- ll_iso7816_get_start_addr() : gr55xx_ll_iso7816.h
- ll_iso7816_get_tx_end_addr() : gr55xx_ll_iso7816.h
- ll_iso7816_get_tx_end_addr_frac() : gr55xx_ll_iso7816.h
- ll_iso7816_get_tx_endbyte_addr() : gr55xx_ll_iso7816.h
- ll_iso7816_get_tx_retry_max() : gr55xx_ll_iso7816.h
- ll_iso7816_get_waittime() : gr55xx_ll_iso7816.h
- ll_iso7816_init() : gr55xx_ll_iso7816.h
- ll_iso7816_is_active_flag_dma_err() : gr55xx_ll_iso7816.h
- ll_iso7816_is_active_flag_done() : gr55xx_ll_iso7816.h
- ll_iso7816_is_active_flag_presence() : gr55xx_ll_iso7816.h
- ll_iso7816_is_active_flag_retry_err() : gr55xx_ll_iso7816.h
- ll_iso7816_is_active_flag_rx_err() : gr55xx_ll_iso7816.h
- ll_iso7816_is_active_flag_state_err() : gr55xx_ll_iso7816.h
- ll_iso7816_is_active_flag_test() : gr55xx_ll_iso7816.h
- ll_iso7816_is_busy() : gr55xx_ll_iso7816.h
- ll_iso7816_set_action() : gr55xx_ll_iso7816.h
- ll_iso7816_set_base_addr() : gr55xx_ll_iso7816.h
- ll_iso7816_set_buffer_addr() : gr55xx_ll_iso7816.h
- ll_iso7816_set_clkdiv() : gr55xx_ll_iso7816.h
- ll_iso7816_set_clkstop_level() : gr55xx_ll_iso7816.h
- ll_iso7816_set_coding_convention() : gr55xx_ll_iso7816.h
- ll_iso7816_set_etudiv() : gr55xx_ll_iso7816.h
- ll_iso7816_set_guardtime() : gr55xx_ll_iso7816.h
- ll_iso7816_set_retry_limit() : gr55xx_ll_iso7816.h
- ll_iso7816_set_rx_end_addr() : gr55xx_ll_iso7816.h
- ll_iso7816_set_rx_end_addr_frac() : gr55xx_ll_iso7816.h
- ll_iso7816_set_rx_endbyte_addr() : gr55xx_ll_iso7816.h
- ll_iso7816_set_start_addr() : gr55xx_ll_iso7816.h
- ll_iso7816_set_tx_end_addr() : gr55xx_ll_iso7816.h
- ll_iso7816_set_tx_end_addr_frac() : gr55xx_ll_iso7816.h
- ll_iso7816_set_tx_endbyte_addr() : gr55xx_ll_iso7816.h
- ll_iso7816_set_waittime() : gr55xx_ll_iso7816.h
- ll_msio_deinit() : gr55xx_ll_msio.h
- ll_msio_get_pin_direction() : gr55xx_ll_msio.h
- ll_msio_get_pin_mode() : gr55xx_ll_msio.h
- ll_msio_get_pin_mux() : gr55xx_ll_msio.h
- ll_msio_get_pin_pull() : gr55xx_ll_msio.h
- ll_msio_init() : gr55xx_ll_msio.h
- ll_msio_is_input_pin_set() : gr55xx_ll_msio.h
- ll_msio_is_output_pin_set() : gr55xx_ll_msio.h
- ll_msio_read_input_port() : gr55xx_ll_msio.h
- ll_msio_read_output_port() : gr55xx_ll_msio.h
- ll_msio_reset_output_pin() : gr55xx_ll_msio.h
- ll_msio_set_output_pin() : gr55xx_ll_msio.h
- ll_msio_set_pin_direction() : gr55xx_ll_msio.h
- ll_msio_set_pin_mode() : gr55xx_ll_msio.h
- ll_msio_set_pin_mux() : gr55xx_ll_msio.h
- ll_msio_set_pin_pull() : gr55xx_ll_msio.h
- ll_msio_struct_init() : gr55xx_ll_msio.h
- ll_msio_toggle_pin() : gr55xx_ll_msio.h
- ll_msio_write_output_port() : gr55xx_ll_msio.h
- ll_pkc_clear_flag_it_big_add_overflow() : gr55xx_ll_pkc.h
- ll_pkc_clear_flag_it_done() : gr55xx_ll_pkc.h
- ll_pkc_clear_flag_it_err() : gr55xx_ll_pkc.h
- ll_pkc_deinit() : gr55xx_ll_pkc.h
- ll_pkc_disable() : gr55xx_ll_pkc.h
- ll_pkc_disable_dummy_multi() : gr55xx_ll_pkc.h
- ll_pkc_disable_hardware_start() : gr55xx_ll_pkc.h
- ll_pkc_disable_it_big_add_overflow() : gr55xx_ll_pkc.h
- ll_pkc_disable_it_done() : gr55xx_ll_pkc.h
- ll_pkc_disable_it_err() : gr55xx_ll_pkc.h
- ll_pkc_disable_random_clock_gating() : gr55xx_ll_pkc.h
- ll_pkc_disable_reset() : gr55xx_ll_pkc.h
- ll_pkc_disable_software() : gr55xx_ll_pkc.h
- ll_pkc_disable_software_start() : gr55xx_ll_pkc.h
- ll_pkc_enable() : gr55xx_ll_pkc.h
- ll_pkc_enable_dummy_multi() : gr55xx_ll_pkc.h
- ll_pkc_enable_hardware_start() : gr55xx_ll_pkc.h
- ll_pkc_enable_it_big_add_overflow() : gr55xx_ll_pkc.h
- ll_pkc_enable_it_done() : gr55xx_ll_pkc.h
- ll_pkc_enable_it_err() : gr55xx_ll_pkc.h
- ll_pkc_enable_random_clock_gating() : gr55xx_ll_pkc.h
- ll_pkc_enable_reset() : gr55xx_ll_pkc.h
- ll_pkc_enable_software() : gr55xx_ll_pkc.h
- ll_pkc_enable_software_start() : gr55xx_ll_pkc.h
- ll_pkc_get_ba_a_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_ba_b_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_ba_c_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_bm_a_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_bm_b_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_bm_c_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_constant1_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_constp() : gr55xx_ll_pkc.h
- ll_pkc_get_dummy_multiply_seed() : gr55xx_ll_pkc.h
- ll_pkc_get_ecc_a_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_ecc_b_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_gx_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_gy_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_gz_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_k_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_mas_a_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_mas_b_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_mas_c_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_mas_p_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_mi_u_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_mi_v_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_mi_x1_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_mi_x2_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_mik_output() : gr55xx_ll_pkc.h
- ll_pkc_get_mitmp_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_mm_a_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_mm_b_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_mm_c_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_mm_p_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_operation_mode() : gr55xx_ll_pkc.h
- ll_pkc_get_operation_word_length() : gr55xx_ll_pkc.h
- ll_pkc_get_p_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_r0x_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_r0y_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_r0z_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_r1x_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_r1y_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_r1z_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_r_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_random_clock_gating_seed() : gr55xx_ll_pkc.h
- ll_pkc_get_rsq_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_swmi_tmp_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_tmp1_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_tmp2_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_tmp3_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_tmp4_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_tmp5_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_tmp6_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_tmpk_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_x1_pointer() : gr55xx_ll_pkc.h
- ll_pkc_get_x2_pointer() : gr55xx_ll_pkc.h
- ll_pkc_init() : gr55xx_ll_pkc.h
- ll_pkc_is_action_flag_busy() : gr55xx_ll_pkc.h
- ll_pkc_is_action_flag_it_big_add_overflow() : gr55xx_ll_pkc.h
- ll_pkc_is_action_flag_it_done() : gr55xx_ll_pkc.h
- ll_pkc_is_action_flag_it_err() : gr55xx_ll_pkc.h
- ll_pkc_is_enable_it_big_add_overflow() : gr55xx_ll_pkc.h
- ll_pkc_is_enable_it_done() : gr55xx_ll_pkc.h
- ll_pkc_is_enable_it_err() : gr55xx_ll_pkc.h
- ll_pkc_is_enabled() : gr55xx_ll_pkc.h
- ll_pkc_is_enabled_dummy_multi() : gr55xx_ll_pkc.h
- ll_pkc_is_enabled_hardware_start() : gr55xx_ll_pkc.h
- ll_pkc_is_enabled_random_clock_gating() : gr55xx_ll_pkc.h
- ll_pkc_is_enabled_reset() : gr55xx_ll_pkc.h
- ll_pkc_is_enabled_software() : gr55xx_ll_pkc.h
- ll_pkc_is_enabled_software_start() : gr55xx_ll_pkc.h
- ll_pkc_set_ba_a_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_ba_b_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_ba_c_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_bm_a_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_bm_b_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_bm_c_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_constant1_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_constp() : gr55xx_ll_pkc.h
- ll_pkc_set_dummy_multiply_seed() : gr55xx_ll_pkc.h
- ll_pkc_set_ecc_a_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_ecc_b_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_gx_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_gy_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_gz_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_k_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_mas_a_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_mas_b_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_mas_c_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_mas_p_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_mi_u_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_mi_v_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_mi_x1_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_mi_x2_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_mitmp_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_mm_a_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_mm_b_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_mm_c_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_mm_p_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_operation_mode() : gr55xx_ll_pkc.h
- ll_pkc_set_operation_word_length() : gr55xx_ll_pkc.h
- ll_pkc_set_p_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_r0x_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_r0y_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_r0z_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_r1x_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_r1y_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_r1z_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_r_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_random_clock_gating_seed() : gr55xx_ll_pkc.h
- ll_pkc_set_rsq_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_swmi_tmp_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_tmp1_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_tmp2_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_tmp3_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_tmp4_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_tmp5_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_tmp6_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_tmpk_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_x1_pointer() : gr55xx_ll_pkc.h
- ll_pkc_set_x2_pointer() : gr55xx_ll_pkc.h
- ll_pkc_struct_init() : gr55xx_ll_pkc.h
- ll_pwm_deinit() : gr55xx_ll_pwm.h
- ll_pwm_disable() : gr55xx_ll_pwm.h
- ll_pwm_disable_pause() : gr55xx_ll_pwm.h
- ll_pwm_disable_positive_drive_channel_a() : gr55xx_ll_pwm.h
- ll_pwm_disable_positive_drive_channel_b() : gr55xx_ll_pwm.h
- ll_pwm_disable_positive_drive_channel_c() : gr55xx_ll_pwm.h
- ll_pwm_disable_update_active_event() : gr55xx_ll_pwm.h
- ll_pwm_disable_update_all() : gr55xx_ll_pwm.h
- ll_pwm_disable_update_breath_period() : gr55xx_ll_pwm.h
- ll_pwm_disable_update_compare_a0() : gr55xx_ll_pwm.h
- ll_pwm_disable_update_compare_a1() : gr55xx_ll_pwm.h
- ll_pwm_disable_update_compare_b0() : gr55xx_ll_pwm.h
- ll_pwm_disable_update_compare_b1() : gr55xx_ll_pwm.h
- ll_pwm_disable_update_compare_c0() : gr55xx_ll_pwm.h
- ll_pwm_disable_update_compare_c1() : gr55xx_ll_pwm.h
- ll_pwm_disable_update_hold_period() : gr55xx_ll_pwm.h
- ll_pwm_disable_update_pause() : gr55xx_ll_pwm.h
- ll_pwm_disable_update_period() : gr55xx_ll_pwm.h
- ll_pwm_enable() : gr55xx_ll_pwm.h
- ll_pwm_enable_pause() : gr55xx_ll_pwm.h
- ll_pwm_enable_positive_drive_channel_a() : gr55xx_ll_pwm.h
- ll_pwm_enable_positive_drive_channel_b() : gr55xx_ll_pwm.h
- ll_pwm_enable_positive_drive_channel_c() : gr55xx_ll_pwm.h
- ll_pwm_enable_update_active_event() : gr55xx_ll_pwm.h
- ll_pwm_enable_update_all() : gr55xx_ll_pwm.h
- ll_pwm_enable_update_breath_period() : gr55xx_ll_pwm.h
- ll_pwm_enable_update_compare_a0() : gr55xx_ll_pwm.h
- ll_pwm_enable_update_compare_a1() : gr55xx_ll_pwm.h
- ll_pwm_enable_update_compare_b0() : gr55xx_ll_pwm.h
- ll_pwm_enable_update_compare_b1() : gr55xx_ll_pwm.h
- ll_pwm_enable_update_compare_c0() : gr55xx_ll_pwm.h
- ll_pwm_enable_update_compare_c1() : gr55xx_ll_pwm.h
- ll_pwm_enable_update_hold_period() : gr55xx_ll_pwm.h
- ll_pwm_enable_update_pause() : gr55xx_ll_pwm.h
- ll_pwm_enable_update_period() : gr55xx_ll_pwm.h
- ll_pwm_get_action_event_cmp_a0() : gr55xx_ll_pwm.h
- ll_pwm_get_action_event_cmp_a1() : gr55xx_ll_pwm.h
- ll_pwm_get_action_event_cmp_b0() : gr55xx_ll_pwm.h
- ll_pwm_get_action_event_cmp_b1() : gr55xx_ll_pwm.h
- ll_pwm_get_action_event_cmp_c0() : gr55xx_ll_pwm.h
- ll_pwm_get_action_event_cmp_c1() : gr55xx_ll_pwm.h
- ll_pwm_get_breath_prescaler() : gr55xx_ll_pwm.h
- ll_pwm_get_compare_a0() : gr55xx_ll_pwm.h
- ll_pwm_get_compare_a1() : gr55xx_ll_pwm.h
- ll_pwm_get_compare_b0() : gr55xx_ll_pwm.h
- ll_pwm_get_compare_b1() : gr55xx_ll_pwm.h
- ll_pwm_get_compare_c0() : gr55xx_ll_pwm.h
- ll_pwm_get_compare_c1() : gr55xx_ll_pwm.h
- ll_pwm_get_hold_prescaler() : gr55xx_ll_pwm.h
- ll_pwm_get_mode() : gr55xx_ll_pwm.h
- ll_pwm_get_prescaler() : gr55xx_ll_pwm.h
- ll_pwm_init() : gr55xx_ll_pwm.h
- ll_pwm_is_active_flag_update_all() : gr55xx_ll_pwm.h
- ll_pwm_is_enabled() : gr55xx_ll_pwm.h
- ll_pwm_is_enabled_pause() : gr55xx_ll_pwm.h
- ll_pwm_is_enabled_positive_drive_channel_a() : gr55xx_ll_pwm.h
- ll_pwm_is_enabled_positive_drive_channel_b() : gr55xx_ll_pwm.h
- ll_pwm_is_enabled_positive_drive_channel_c() : gr55xx_ll_pwm.h
- ll_pwm_is_enabled_update_active_event() : gr55xx_ll_pwm.h
- ll_pwm_is_enabled_update_all() : gr55xx_ll_pwm.h
- ll_pwm_is_enabled_update_breath_period() : gr55xx_ll_pwm.h
- ll_pwm_is_enabled_update_compare_a0() : gr55xx_ll_pwm.h
- ll_pwm_is_enabled_update_compare_a1() : gr55xx_ll_pwm.h
- ll_pwm_is_enabled_update_compare_b0() : gr55xx_ll_pwm.h
- ll_pwm_is_enabled_update_compare_b1() : gr55xx_ll_pwm.h
- ll_pwm_is_enabled_update_compare_c0() : gr55xx_ll_pwm.h
- ll_pwm_is_enabled_update_compare_c1() : gr55xx_ll_pwm.h
- ll_pwm_is_enabled_update_hold_period() : gr55xx_ll_pwm.h
- ll_pwm_is_enabled_update_pause() : gr55xx_ll_pwm.h
- ll_pwm_is_enabled_update_period() : gr55xx_ll_pwm.h
- ll_pwm_set_action_event_cmp_a0() : gr55xx_ll_pwm.h
- ll_pwm_set_action_event_cmp_a1() : gr55xx_ll_pwm.h
- ll_pwm_set_action_event_cmp_b0() : gr55xx_ll_pwm.h
- ll_pwm_set_action_event_cmp_b1() : gr55xx_ll_pwm.h
- ll_pwm_set_action_event_cmp_c0() : gr55xx_ll_pwm.h
- ll_pwm_set_action_event_cmp_c1() : gr55xx_ll_pwm.h
- ll_pwm_set_breath_prescaler() : gr55xx_ll_pwm.h
- ll_pwm_set_compare_a0() : gr55xx_ll_pwm.h
- ll_pwm_set_compare_a1() : gr55xx_ll_pwm.h
- ll_pwm_set_compare_b0() : gr55xx_ll_pwm.h
- ll_pwm_set_compare_b1() : gr55xx_ll_pwm.h
- ll_pwm_set_compare_c0() : gr55xx_ll_pwm.h
- ll_pwm_set_compare_c1() : gr55xx_ll_pwm.h
- ll_pwm_set_hold_prescaler() : gr55xx_ll_pwm.h
- ll_pwm_set_mode() : gr55xx_ll_pwm.h
- ll_pwm_set_prescaler() : gr55xx_ll_pwm.h
- ll_pwm_struct_init() : gr55xx_ll_pwm.h
- ll_pwr_clear_ext_wakeup_status() : gr55xx_ll_pwr.h
- ll_pwr_clear_wakeup_event() : gr55xx_ll_pwr.h
- ll_pwr_disable_cache_module() : gr55xx_ll_pwr.h
- ll_pwr_disable_comm_core_deep_sleep() : gr55xx_ll_pwr.h
- ll_pwr_disable_comm_core_ext_wakeup() : gr55xx_ll_pwr.h
- ll_pwr_disable_comm_core_power() : gr55xx_ll_pwr.h
- ll_pwr_disable_comm_core_reset() : gr55xx_ll_pwr.h
- ll_pwr_disable_comm_timer_power() : gr55xx_ll_pwr.h
- ll_pwr_disable_comm_timer_reset() : gr55xx_ll_pwr.h
- ll_pwr_disable_ext_wakeup_pin() : gr55xx_ll_pwr.h
- ll_pwr_disable_osc_sleep() : gr55xx_ll_pwr.h
- ll_pwr_disable_radio_sleep() : gr55xx_ll_pwr.h
- ll_pwr_disable_smc_wakeup_req() : gr55xx_ll_pwr.h
- ll_pwr_enable_comm_core_deep_sleep() : gr55xx_ll_pwr.h
- ll_pwr_enable_comm_core_ext_wakeup() : gr55xx_ll_pwr.h
- ll_pwr_enable_comm_core_power() : gr55xx_ll_pwr.h
- ll_pwr_enable_comm_core_reset() : gr55xx_ll_pwr.h
- ll_pwr_enable_comm_soft_wakeup_req() : gr55xx_ll_pwr.h
- ll_pwr_enable_comm_timer_power() : gr55xx_ll_pwr.h
- ll_pwr_enable_comm_timer_reset() : gr55xx_ll_pwr.h
- ll_pwr_enable_ext_wakeup_pin() : gr55xx_ll_pwr.h
- ll_pwr_enable_osc_sleep() : gr55xx_ll_pwr.h
- ll_pwr_enable_radio_sleep() : gr55xx_ll_pwr.h
- ll_pwr_enable_smc_wakeup_req() : gr55xx_ll_pwr.h
- ll_pwr_get_comm_sleep_duration() : gr55xx_ll_pwr.h
- ll_pwr_get_comm_wakeup_time() : gr55xx_ll_pwr.h
- ll_pwr_get_ext_wakeup_status() : gr55xx_ll_pwr.h
- ll_pwr_get_ext_wakeup_type() : gr55xx_ll_pwr.h
- ll_pwr_get_sleep_timer_value() : gr55xx_ll_pwr.h
- ll_pwr_get_timer_read_select() : gr55xx_ll_pwr.h
- ll_pwr_get_timer_read_value() : gr55xx_ll_pwr.h
- ll_pwr_get_wakeup_condition() : gr55xx_ll_pwr.h
- ll_pwr_get_wakeup_event() : gr55xx_ll_pwr.h
- ll_pwr_is_active_flag_comm_deep_sleep_stat() : gr55xx_ll_pwr.h
- ll_pwr_is_active_flag_psc_cmd_busy() : gr55xx_ll_pwr.h
- ll_pwr_is_enabled_comm_core_deep_sleep() : gr55xx_ll_pwr.h
- ll_pwr_is_enabled_comm_core_ext_wakeup() : gr55xx_ll_pwr.h
- ll_pwr_is_enabled_comm_core_power() : gr55xx_ll_pwr.h
- ll_pwr_is_enabled_comm_core_reset() : gr55xx_ll_pwr.h
- ll_pwr_is_enabled_comm_timer_power() : gr55xx_ll_pwr.h
- ll_pwr_is_enabled_comm_timer_reset() : gr55xx_ll_pwr.h
- ll_pwr_is_enabled_ext_wakeup_pin() : gr55xx_ll_pwr.h
- ll_pwr_is_enabled_osc_sleep() : gr55xx_ll_pwr.h
- ll_pwr_is_enabled_radio_sleep() : gr55xx_ll_pwr.h
- ll_pwr_is_enabled_smc_wakeup_req() : gr55xx_ll_pwr.h
- ll_pwr_is_enabled_soft_wakeup_req() : gr55xx_ll_pwr.h
- ll_pwr_read_comm_wakeup_timing() : gr55xx_ll_pwr.h
- ll_pwr_read_comm_wakeup_timing_twosc() : gr55xx_ll_pwr.h
- ll_pwr_req_excute_psc_command() : gr55xx_ll_pwr.h
- ll_pwr_set_comm_core_wakeup_time() : gr55xx_ll_pwr.h
- ll_pwr_set_comm_wakeup_timing() : gr55xx_ll_pwr.h
- ll_pwr_set_dpad_le_value() : gr55xx_ll_pwr.h
- ll_pwr_set_ext_wakeup_type() : gr55xx_ll_pwr.h
- ll_pwr_set_sleep_timer_value() : gr55xx_ll_pwr.h
- ll_pwr_set_timer_read_select() : gr55xx_ll_pwr.h
- ll_pwr_set_wakeup_condition() : gr55xx_ll_pwr.h
- ll_qspi_deinit() : gr55xx_ll_spi.h
- ll_qspi_init() : gr55xx_ll_spi.h
- ll_qspi_struct_init() : gr55xx_ll_spi.h
- ll_rng_clear_flag_sts() : gr55xx_ll_rng.h
- ll_rng_deinit() : gr55xx_ll_rng.h
- ll_rng_disable() : gr55xx_ll_rng.h
- ll_rng_disable_fro() : gr55xx_ll_rng.h
- ll_rng_disable_it() : gr55xx_ll_rng.h
- ll_rng_enable() : gr55xx_ll_rng.h
- ll_rng_enable_fro() : gr55xx_ll_rng.h
- ll_rng_enable_it() : gr55xx_ll_rng.h
- ll_rng_fro_is_enabled() : gr55xx_ll_rng.h
- ll_rng_get_lfsr_mode() : gr55xx_ll_rng.h
- ll_rng_get_lfsr_seed() : gr55xx_ll_rng.h
- ll_rng_get_output_mode() : gr55xx_ll_rng.h
- ll_rng_get_post_mode() : gr55xx_ll_rng.h
- ll_rng_get_trdy_time() : gr55xx_ll_rng.h
- ll_rng_init() : gr55xx_ll_rng.h
- ll_rng_is_active_flag_lr() : gr55xx_ll_rng.h
- ll_rng_is_active_flag_sts() : gr55xx_ll_rng.h
- ll_rng_is_enabled() : gr55xx_ll_rng.h
- ll_rng_is_enabled_it() : gr55xx_ll_rng.h
- ll_rng_read_lr_count() : gr55xx_ll_rng.h
- ll_rng_read_random_data32() : gr55xx_ll_rng.h
- ll_rng_set_lfsr_mode() : gr55xx_ll_rng.h
- ll_rng_set_lfsr_seed() : gr55xx_ll_rng.h
- ll_rng_set_output_mode() : gr55xx_ll_rng.h
- ll_rng_set_post_mode() : gr55xx_ll_rng.h
- ll_rng_set_trdy_time() : gr55xx_ll_rng.h
- ll_rng_set_user_seed() : gr55xx_ll_rng.h
- ll_rng_struct_init() : gr55xx_ll_rng.h
- ll_spi_clear_flag_all() : gr55xx_ll_spi.h
- ll_spi_clear_flag_mst() : gr55xx_ll_spi.h
- ll_spi_clear_flag_rxo() : gr55xx_ll_spi.h
- ll_spi_clear_flag_rxu() : gr55xx_ll_spi.h
- ll_spi_clear_flag_txo() : gr55xx_ll_spi.h
- ll_spi_disable() : gr55xx_ll_spi.h
- ll_spi_disable_dma_req_rx() : gr55xx_ll_spi.h
- ll_spi_disable_dma_req_tx() : gr55xx_ll_spi.h
- ll_spi_disable_it() : gr55xx_ll_spi.h
- ll_spi_disable_micro_handshake() : gr55xx_ll_spi.h
- ll_spi_disable_salve_out() : gr55xx_ll_spi.h
- ll_spi_disable_ss() : gr55xx_ll_spi.h
- ll_spi_disable_ss_toggle() : gr55xx_ll_spi.h
- ll_spi_disable_test_mode() : gr55xx_ll_spi.h
- ll_spi_enable() : gr55xx_ll_spi.h
- ll_spi_enable_dma_req_rx() : gr55xx_ll_spi.h
- ll_spi_enable_dma_req_tx() : gr55xx_ll_spi.h
- ll_spi_enable_it() : gr55xx_ll_spi.h
- ll_spi_enable_micro_handshake() : gr55xx_ll_spi.h
- ll_spi_enable_slave_out() : gr55xx_ll_spi.h
- ll_spi_enable_ss() : gr55xx_ll_spi.h
- ll_spi_enable_ss_toggle() : gr55xx_ll_spi.h
- ll_spi_enable_test_mode() : gr55xx_ll_spi.h
- ll_spi_get_addr_inst_transfer_format() : gr55xx_ll_spi.h
- ll_spi_get_address_size() : gr55xx_ll_spi.h
- ll_spi_get_baud_rate_prescaler() : gr55xx_ll_spi.h
- ll_spi_get_clock_phase() : gr55xx_ll_spi.h
- ll_spi_get_clock_polarity() : gr55xx_ll_spi.h
- ll_spi_get_control_frame_size() : gr55xx_ll_spi.h
- ll_spi_get_data_size() : gr55xx_ll_spi.h
- ll_spi_get_dma_rx_fifo_threshold() : gr55xx_ll_spi.h
- ll_spi_get_dma_tx_fifo_threshold() : gr55xx_ll_spi.h
- ll_spi_get_frame_format() : gr55xx_ll_spi.h
- ll_spi_get_id_code() : gr55xx_ll_spi.h
- ll_spi_get_instruction_size() : gr55xx_ll_spi.h
- ll_spi_get_it_flag() : gr55xx_ll_spi.h
- ll_spi_get_micro_transfer_direction() : gr55xx_ll_spi.h
- ll_spi_get_micro_transfer_mode() : gr55xx_ll_spi.h
- ll_spi_get_raw_if_flag() : gr55xx_ll_spi.h
- ll_spi_get_receive_size() : gr55xx_ll_spi.h
- ll_spi_get_rx_fifo_level() : gr55xx_ll_spi.h
- ll_spi_get_rx_fifo_threshold() : gr55xx_ll_spi.h
- ll_spi_get_rx_sample_delay() : gr55xx_ll_spi.h
- ll_spi_get_standard() : gr55xx_ll_spi.h
- ll_spi_get_status() : gr55xx_ll_spi.h
- ll_spi_get_transfer_direction() : gr55xx_ll_spi.h
- ll_spi_get_tx_fifo_level() : gr55xx_ll_spi.h
- ll_spi_get_tx_fifo_threshold() : gr55xx_ll_spi.h
- ll_spi_get_version() : gr55xx_ll_spi.h
- ll_spi_get_wait_cycles() : gr55xx_ll_spi.h
- ll_spi_is_active_flag() : gr55xx_ll_spi.h
- ll_spi_is_enabled() : gr55xx_ll_spi.h
- ll_spi_is_enabled_dma_req_rx() : gr55xx_ll_spi.h
- ll_spi_is_enabled_dma_req_tx() : gr55xx_ll_spi.h
- ll_spi_is_enabled_it() : gr55xx_ll_spi.h
- ll_spi_is_enabled_micro_handshake() : gr55xx_ll_spi.h
- ll_spi_is_enabled_slave_out() : gr55xx_ll_spi.h
- ll_spi_is_enabled_ss() : gr55xx_ll_spi.h
- ll_spi_is_enabled_ss_toggle() : gr55xx_ll_spi.h
- ll_spi_is_enabled_test_mode() : gr55xx_ll_spi.h
- ll_spi_is_it_flag() : gr55xx_ll_spi.h
- ll_spi_receive_data16() : gr55xx_ll_spi.h
- ll_spi_receive_data32() : gr55xx_ll_spi.h
- ll_spi_receive_data8() : gr55xx_ll_spi.h
- ll_spi_set_add_inst_transfer_format() : gr55xx_ll_spi.h
- ll_spi_set_address_size() : gr55xx_ll_spi.h
- ll_spi_set_baud_rate_prescaler() : gr55xx_ll_spi.h
- ll_spi_set_clock_phase() : gr55xx_ll_spi.h
- ll_spi_set_clock_polarity() : gr55xx_ll_spi.h
- ll_spi_set_control_frame_size() : gr55xx_ll_spi.h
- ll_spi_set_data_size() : gr55xx_ll_spi.h
- ll_spi_set_dma_rx_fifo_threshold() : gr55xx_ll_spi.h
- ll_spi_set_dma_tx_fifo_threshold() : gr55xx_ll_spi.h
- ll_spi_set_frame_format() : gr55xx_ll_spi.h
- ll_spi_set_instruction_size() : gr55xx_ll_spi.h
- ll_spi_set_micro_transfer_direction() : gr55xx_ll_spi.h
- ll_spi_set_micro_transfer_mode() : gr55xx_ll_spi.h
- ll_spi_set_receive_size() : gr55xx_ll_spi.h
- ll_spi_set_rx_fifo_threshold() : gr55xx_ll_spi.h
- ll_spi_set_rx_sample_delay() : gr55xx_ll_spi.h
- ll_spi_set_standard() : gr55xx_ll_spi.h
- ll_spi_set_transfer_direction() : gr55xx_ll_spi.h
- ll_spi_set_tx_fifo_threshold() : gr55xx_ll_spi.h
- ll_spi_set_wait_cycles() : gr55xx_ll_spi.h
- ll_spi_transmit_data16() : gr55xx_ll_spi.h
- ll_spi_transmit_data32() : gr55xx_ll_spi.h
- ll_spi_transmit_data8() : gr55xx_ll_spi.h
- ll_spim_deinit() : gr55xx_ll_spi.h
- ll_spim_init() : gr55xx_ll_spi.h
- ll_spim_struct_init() : gr55xx_ll_spi.h
- ll_spis_deinit() : gr55xx_ll_spi.h
- ll_spis_init() : gr55xx_ll_spi.h
- ll_spis_struct_init() : gr55xx_ll_spi.h
- ll_timer_clear_flag_it() : gr55xx_ll_tim.h
- ll_timer_deinit() : gr55xx_ll_tim.h
- ll_timer_disable_counter() : gr55xx_ll_tim.h
- ll_timer_disable_it() : gr55xx_ll_tim.h
- ll_timer_enable_counter() : gr55xx_ll_tim.h
- ll_timer_enable_it() : gr55xx_ll_tim.h
- ll_timer_get_auto_reload() : gr55xx_ll_tim.h
- ll_timer_get_counter() : gr55xx_ll_tim.h
- ll_timer_init() : gr55xx_ll_tim.h
- ll_timer_is_active_flag_it() : gr55xx_ll_tim.h
- ll_timer_is_enabled_counter() : gr55xx_ll_tim.h
- ll_timer_is_enabled_it() : gr55xx_ll_tim.h
- ll_timer_set_auto_reload() : gr55xx_ll_tim.h
- ll_timer_set_counter() : gr55xx_ll_tim.h
- ll_timer_struct_init() : gr55xx_ll_tim.h
- ll_uart_clear_line_status_flag() : gr55xx_ll_uart.h
- ll_uart_config_character() : gr55xx_ll_uart.h
- ll_uart_deinit() : gr55xx_ll_uart.h
- ll_uart_disable_break_sending() : gr55xx_ll_uart.h
- ll_uart_disable_fifo() : gr55xx_ll_uart.h
- ll_uart_disable_it() : gr55xx_ll_uart.h
- ll_uart_disable_it_ms() : gr55xx_ll_uart.h
- ll_uart_disable_it_rda() : gr55xx_ll_uart.h
- ll_uart_disable_it_rls() : gr55xx_ll_uart.h
- ll_uart_disable_it_thre() : gr55xx_ll_uart.h
- ll_uart_dma_get_register_address() : gr55xx_ll_uart.h
- ll_uart_enable_break_sending() : gr55xx_ll_uart.h
- ll_uart_enable_fifo() : gr55xx_ll_uart.h
- ll_uart_enable_it() : gr55xx_ll_uart.h
- ll_uart_enable_it_rda() : gr55xx_ll_uart.h
- ll_uart_enable_it_rls() : gr55xx_ll_uart.h
- ll_uart_enable_it_thre() : gr55xx_ll_uart.h
- ll_uart_enabled_it_ms() : gr55xx_ll_uart.h
- ll_uart_flush_rx_fifo() : gr55xx_ll_uart.h
- ll_uart_flush_tx_fifo() : gr55xx_ll_uart.h
- ll_uart_get_baud_rate() : gr55xx_ll_uart.h
- ll_uart_get_cts_pin_state() : gr55xx_ll_uart.h
- ll_uart_get_data_bits_length() : gr55xx_ll_uart.h
- ll_uart_get_hw_flow_ctrl() : gr55xx_ll_uart.h
- ll_uart_get_it_flag() : gr55xx_ll_uart.h
- ll_uart_get_line_status_flag() : gr55xx_ll_uart.h
- ll_uart_get_parity() : gr55xx_ll_uart.h
- ll_uart_get_rts_pin_state() : gr55xx_ll_uart.h
- ll_uart_get_rx_fifo_level() : gr55xx_ll_uart.h
- ll_uart_get_rx_fifo_threshold() : gr55xx_ll_uart.h
- ll_uart_get_stop_bits_length() : gr55xx_ll_uart.h
- ll_uart_get_tx_fifo_level() : gr55xx_ll_uart.h
- ll_uart_get_tx_fifo_threshold() : gr55xx_ll_uart.h
- ll_uart_init() : gr55xx_ll_uart.h
- ll_uart_is_active_flag_rff() : gr55xx_ll_uart.h
- ll_uart_is_active_flag_rfne() : gr55xx_ll_uart.h
- ll_uart_is_active_flag_tfe() : gr55xx_ll_uart.h
- ll_uart_is_active_flag_tfnf() : gr55xx_ll_uart.h
- ll_uart_is_changed_cts() : gr55xx_ll_uart.h
- ll_uart_is_enabled_break_sending() : gr55xx_ll_uart.h
- ll_uart_is_enabled_fifo() : gr55xx_ll_uart.h
- ll_uart_is_enabled_it() : gr55xx_ll_uart.h
- ll_uart_is_enabled_it_ms() : gr55xx_ll_uart.h
- ll_uart_is_enabled_it_rda() : gr55xx_ll_uart.h
- ll_uart_is_enabled_it_rls() : gr55xx_ll_uart.h
- ll_uart_is_enabled_it_thre() : gr55xx_ll_uart.h
- ll_uart_receive_data8() : gr55xx_ll_uart.h
- ll_uart_reset() : gr55xx_ll_uart.h
- ll_uart_set_baud_rate() : gr55xx_ll_uart.h
- ll_uart_set_data_bits_length() : gr55xx_ll_uart.h
- ll_uart_set_hw_flow_ctrl() : gr55xx_ll_uart.h
- ll_uart_set_parity() : gr55xx_ll_uart.h
- ll_uart_set_rts_pin_state() : gr55xx_ll_uart.h
- ll_uart_set_rx_fifo_threshold() : gr55xx_ll_uart.h
- ll_uart_set_stop_bits_length() : gr55xx_ll_uart.h
- ll_uart_set_tx_fifo_threshold() : gr55xx_ll_uart.h
- ll_uart_struct_init() : gr55xx_ll_uart.h
- ll_uart_transmit_data8() : gr55xx_ll_uart.h
- ll_wdt_clear_flag_it() : gr55xx_ll_wdt.h
- ll_wdt_disable() : gr55xx_ll_wdt.h
- ll_wdt_disable_reset() : gr55xx_ll_wdt.h
- ll_wdt_disable_write_access() : gr55xx_ll_wdt.h
- ll_wdt_enable() : gr55xx_ll_wdt.h
- ll_wdt_enable_reset() : gr55xx_ll_wdt.h
- ll_wdt_enable_write_access() : gr55xx_ll_wdt.h
- ll_wdt_get_counter_load() : gr55xx_ll_wdt.h
- ll_wdt_get_counter_value() : gr55xx_ll_wdt.h
- ll_wdt_is_active_flag_it() : gr55xx_ll_wdt.h
- ll_wdt_is_enabled() : gr55xx_ll_wdt.h
- ll_wdt_is_enabled_reset() : gr55xx_ll_wdt.h
- ll_wdt_reload_counter() : gr55xx_ll_wdt.h
- ll_wdt_set_counter_load() : gr55xx_ll_wdt.h
- ll_xqspi_clear_qspi_flag() : gr55xx_ll_xqspi.h
- ll_xqspi_deinit() : gr55xx_ll_xqspi.h
- ll_xqspi_disable_cache() : gr55xx_ll_xqspi.h
- ll_xqspi_disable_cache_dbgmux() : gr55xx_ll_xqspi.h
- ll_xqspi_disable_cache_flush() : gr55xx_ll_xqspi.h
- ll_xqspi_disable_cache_retention() : gr55xx_ll_xqspi.h
- ll_xqspi_disable_exflash_power() : gr55xx_ll_xqspi.h
- ll_xqspi_disable_inhibt_rx() : gr55xx_ll_xqspi.h
- ll_xqspi_disable_inhibt_tx() : gr55xx_ll_xqspi.h
- ll_xqspi_disable_qspi() : gr55xx_ll_xqspi.h
- ll_xqspi_disable_qspi_contxfer() : gr55xx_ll_xqspi.h
- ll_xqspi_disable_qspi_contxfer_extend() : gr55xx_ll_xqspi.h
- ll_xqspi_disable_qspi_dma() : gr55xx_ll_xqspi.h
- ll_xqspi_disable_qspi_dummy() : gr55xx_ll_xqspi.h
- ll_xqspi_disable_qspi_it() : gr55xx_ll_xqspi.h
- ll_xqspi_disable_qspi_ssout() : gr55xx_ll_xqspi.h
- ll_xqspi_disable_xip() : gr55xx_ll_xqspi.h
- ll_xqspi_disable_xip_hp() : gr55xx_ll_xqspi.h
- ll_xqspi_disable_xip_it() : gr55xx_ll_xqspi.h
- ll_xqspi_enable_cache() : gr55xx_ll_xqspi.h
- ll_xqspi_enable_cache_dbgmux() : gr55xx_ll_xqspi.h
- ll_xqspi_enable_cache_flush() : gr55xx_ll_xqspi.h
- ll_xqspi_enable_cache_retention() : gr55xx_ll_xqspi.h
- ll_xqspi_enable_exflash_power() : gr55xx_ll_xqspi.h
- ll_xqspi_enable_inhibt_rx() : gr55xx_ll_xqspi.h
- ll_xqspi_enable_inhibt_tx() : gr55xx_ll_xqspi.h
- ll_xqspi_enable_qspi() : gr55xx_ll_xqspi.h
- ll_xqspi_enable_qspi_contxfer() : gr55xx_ll_xqspi.h
- ll_xqspi_enable_qspi_contxfer_extend() : gr55xx_ll_xqspi.h
- ll_xqspi_enable_qspi_dma() : gr55xx_ll_xqspi.h
- ll_xqspi_enable_qspi_dummy() : gr55xx_ll_xqspi.h
- ll_xqspi_enable_qspi_it() : gr55xx_ll_xqspi.h
- ll_xqspi_enable_qspi_ssout() : gr55xx_ll_xqspi.h
- ll_xqspi_enable_xip() : gr55xx_ll_xqspi.h
- ll_xqspi_enable_xip_hp() : gr55xx_ll_xqspi.h
- ll_xqspi_enable_xip_it() : gr55xx_ll_xqspi.h
- ll_xqspi_get_cache_dbgbus() : gr55xx_ll_xqspi.h
- ll_xqspi_get_cache_fifo() : gr55xx_ll_xqspi.h
- ll_xqspi_get_cache_flag() : gr55xx_ll_xqspi.h
- ll_xqspi_get_cache_hitcount() : gr55xx_ll_xqspi.h
- ll_xqspi_get_cache_hitmiss() : gr55xx_ll_xqspi.h
- ll_xqspi_get_cache_misscount() : gr55xx_ll_xqspi.h
- ll_xqspi_get_flag_xip_it() : gr55xx_ll_xqspi.h
- ll_xqspi_get_flash_write() : gr55xx_ll_xqspi.h
- ll_xqspi_get_it_flag() : gr55xx_ll_xqspi.h
- ll_xqspi_get_present_bypass() : gr55xx_ll_xqspi.h
- ll_xqspi_get_qspi_cpha() : gr55xx_ll_xqspi.h
- ll_xqspi_get_qspi_cpol() : gr55xx_ll_xqspi.h
- ll_xqspi_get_qspi_data_order() : gr55xx_ll_xqspi.h
- ll_xqspi_get_qspi_datasize() : gr55xx_ll_xqspi.h
- ll_xqspi_get_qspi_frf() : gr55xx_ll_xqspi.h
- ll_xqspi_get_qspi_rft() : gr55xx_ll_xqspi.h
- ll_xqspi_get_qspi_rx_fifo_level() : gr55xx_ll_xqspi.h
- ll_xqspi_get_qspi_speed() : gr55xx_ll_xqspi.h
- ll_xqspi_get_qspi_sspol() : gr55xx_ll_xqspi.h
- ll_xqspi_get_qspi_status() : gr55xx_ll_xqspi.h
- ll_xqspi_get_qspi_tft() : gr55xx_ll_xqspi.h
- ll_xqspi_get_qspi_tx_fifo_level() : gr55xx_ll_xqspi.h
- ll_xqspi_get_qspi_wait() : gr55xx_ll_xqspi.h
- ll_xqspi_get_req_xip_it() : gr55xx_ll_xqspi.h
- ll_xqspi_get_xip_addr_size() : gr55xx_ll_xqspi.h
- ll_xqspi_get_xip_cmd() : gr55xx_ll_xqspi.h
- ll_xqspi_get_xip_cpha() : gr55xx_ll_xqspi.h
- ll_xqspi_get_xip_cpol() : gr55xx_ll_xqspi.h
- ll_xqspi_get_xip_dummy_hp() : gr55xx_ll_xqspi.h
- ll_xqspi_get_xip_dummycycles() : gr55xx_ll_xqspi.h
- ll_xqspi_get_xip_endian() : gr55xx_ll_xqspi.h
- ll_xqspi_get_xip_flag() : gr55xx_ll_xqspi.h
- ll_xqspi_get_xip_hp_cmd() : gr55xx_ll_xqspi.h
- ll_xqspi_get_xip_ss() : gr55xx_ll_xqspi.h
- ll_xqspi_init() : gr55xx_ll_xqspi.h
- ll_xqspi_is_active_qspi_flag() : gr55xx_ll_xqspi.h
- ll_xqspi_is_enable_cache_retention() : gr55xx_ll_xqspi.h
- ll_xqspi_is_enable_exflash_power() : gr55xx_ll_xqspi.h
- ll_xqspi_is_enabled_cache() : gr55xx_ll_xqspi.h
- ll_xqspi_is_enabled_cache_dbgmux() : gr55xx_ll_xqspi.h
- ll_xqspi_is_enabled_cache_flush() : gr55xx_ll_xqspi.h
- ll_xqspi_is_enabled_inhibt_rx() : gr55xx_ll_xqspi.h
- ll_xqspi_is_enabled_inhibt_tx() : gr55xx_ll_xqspi.h
- ll_xqspi_is_enabled_qspi() : gr55xx_ll_xqspi.h
- ll_xqspi_is_enabled_qspi_contxfer() : gr55xx_ll_xqspi.h
- ll_xqspi_is_enabled_qspi_contxfer_extend() : gr55xx_ll_xqspi.h
- ll_xqspi_is_enabled_qspi_dma() : gr55xx_ll_xqspi.h
- ll_xqspi_is_enabled_qspi_dummy() : gr55xx_ll_xqspi.h
- ll_xqspi_is_enabled_qspi_it() : gr55xx_ll_xqspi.h
- ll_xqspi_is_enabled_xip() : gr55xx_ll_xqspi.h
- ll_xqspi_is_enabled_xip_hp() : gr55xx_ll_xqspi.h
- ll_xqspi_is_enabled_xip_it() : gr55xx_ll_xqspi.h
- ll_xqspi_is_qspi_it_flag() : gr55xx_ll_xqspi.h
- ll_xqspi_qspi_receive_data16() : gr55xx_ll_xqspi.h
- ll_xqspi_qspi_receive_data32() : gr55xx_ll_xqspi.h
- ll_xqspi_qspi_receive_data8() : gr55xx_ll_xqspi.h
- ll_xqspi_qspi_transmit_data16() : gr55xx_ll_xqspi.h
- ll_xqspi_qspi_transmit_data32() : gr55xx_ll_xqspi.h
- ll_xqspi_qspi_transmit_data8() : gr55xx_ll_xqspi.h
- ll_xqspi_set_cache_dbgbus() : gr55xx_ll_xqspi.h
- ll_xqspi_set_cache_fifo() : gr55xx_ll_xqspi.h
- ll_xqspi_set_cache_hitmiss() : gr55xx_ll_xqspi.h
- ll_xqspi_set_flash_write() : gr55xx_ll_xqspi.h
- ll_xqspi_set_present_bypass() : gr55xx_ll_xqspi.h
- ll_xqspi_set_qspi_cpha() : gr55xx_ll_xqspi.h
- ll_xqspi_set_qspi_cpol() : gr55xx_ll_xqspi.h
- ll_xqspi_set_qspi_data_order() : gr55xx_ll_xqspi.h
- ll_xqspi_set_qspi_datasize() : gr55xx_ll_xqspi.h
- ll_xqspi_set_qspi_frf() : gr55xx_ll_xqspi.h
- ll_xqspi_set_qspi_rft() : gr55xx_ll_xqspi.h
- ll_xqspi_set_qspi_speed() : gr55xx_ll_xqspi.h
- ll_xqspi_set_qspi_sspol() : gr55xx_ll_xqspi.h
- ll_xqspi_set_qspi_tft() : gr55xx_ll_xqspi.h
- ll_xqspi_set_qspi_wait() : gr55xx_ll_xqspi.h
- ll_xqspi_set_xip_addr_size() : gr55xx_ll_xqspi.h
- ll_xqspi_set_xip_cmd() : gr55xx_ll_xqspi.h
- ll_xqspi_set_xip_cpha() : gr55xx_ll_xqspi.h
- ll_xqspi_set_xip_cpol() : gr55xx_ll_xqspi.h
- ll_xqspi_set_xip_dummy_hp() : gr55xx_ll_xqspi.h
- ll_xqspi_set_xip_dummycycles() : gr55xx_ll_xqspi.h
- ll_xqspi_set_xip_endian() : gr55xx_ll_xqspi.h
- ll_xqspi_set_xip_hp_cmd() : gr55xx_ll_xqspi.h
- ll_xqspi_set_xip_ss() : gr55xx_ll_xqspi.h
- ll_xqspi_struct_init() : gr55xx_ll_xqspi.h
- lls_alert_level_get() : lls.h
- lls_c_alert_level_read() : lls_c.h
- lls_c_alert_level_set() : lls_c.h
- lls_c_disc_srvc_start() : lls_c.h
- lls_client_init() : lls_c.h
- lls_service_init() : lls.h
- lms_notify_cmd() : lms.h
- lms_notify_data() : lms.h
- lms_service_init() : lms.h
- lns_log_info_send() : lns.h
- lns_log_status_send() : lns.h
- lns_pay_load_update() : lns.h
- lns_service_init() : lns.h
- local_hal_flash_erase() : gr55xx_nvds.h
- local_hal_flash_erase_chip() : gr55xx_nvds.h
- local_hal_flash_get_info() : gr55xx_nvds.h
- local_hal_flash_get_security() : gr55xx_nvds.h
- local_hal_flash_read() : gr55xx_nvds.h
- local_hal_flash_set_security() : gr55xx_nvds.h
- local_hal_flash_write() : gr55xx_nvds.h
- local_hal_flash_write_r() : gr55xx_nvds.h
- local_time_encode() : cts.h
- local_time_universal_decode() : cts.h