Data Structures
Here are the classes, structs, unions and interfaces with brief descriptions:
[detail level 1 2]

C_adc_handle | ADC handle Structure definition
C_aes_handle | AES handle Structure definition
C_aes_init | AES Init Structure definition
C_aon_gpio_init | AON_GPIO init structure definition
C_aon_wdt_handle | AON_WDT handle Structure definition
C_aon_wdt_init | AON_WDT_Configuration init structure definition
C_bod_handle | BOD handle Structure definition
C_calendar_alarm | CALENDAR_Alarm calendar alarm structure definition
C_calendar_handle | CALENDAR handle Structure definition
C_calendar_time | CALENDAR_Time calendar time structure definition
C_cgc_init | CGC init structure definition
C_comp_handle | COMP handle Structure definition
C_dma_handle | DMA handle Structure definition
C_dma_init | DMA Configuration Structure definition
C_dual_timer_handle | DUAL_TIMER handle Structure definition
C_dual_timer_init | DUAL TIMER init Structure definition
C_efuse_handle | EFuse handle Structure definition
C_efuse_init | EFuse init Structure definition
C_exflash_handle | ExFlash handle Structure definition
C_gpio_init | GPIO init structure definition
C_hal_adc_callback | HAL ADC Callback function definition
C_hal_aes_callback | HAL AES Callback function definition
C_hal_aon_gpio_callback | HAL AON_GPIO Callback function definition
C_hal_aon_wdt_callback | HAL_AON_WDT Callback function definition
C_hal_calendar_callback | HAL_CALENDAR Callback function definition
C_hal_callback | HAL_HAL Callback function definition
C_hal_comp_callback | HAL COMP Callback function definition
C_hal_dual_timer_callback | HAL_DUAL_TIMER Callback function definition
C_hal_efuse_callback | HAL_EFUSE Callback function definition
C_hal_exflash_callback | HAL_EXFLASH Callback function definition
C_hal_gpio_callback | HAL_GPIO Callback function definition
C_hal_hmac_callback | HAL_HMAC Callback function definition
C_hal_i2c_callback | HAL_I2C Callback function definition
C_hal_i2s_callback | HAL_I2S Callback function definition
C_hal_iso7816_callback | HAL_ISO7816 Callback function definition
C_hal_pkc_callback | HAL_PKC Callback function definition
C_hal_pwm_callback | HAL_PWM Callback function definition
C_hal_pwr_handler | PWR callback handle Structure definition
C_hal_qspi_callback | HAL_QSPI Callback function definition
C_hal_rng_callback | HAL_RNG Callback function definition
C_hal_spi_callback | HAL_SPI Callback function definition
C_hal_timer_callback | HAL_TIMER Callback function definition
C_hal_uart_callback | HAL_UART Callback function definition
C_hal_wdt_callback | HAL_WDT Callback function definition
C_hal_xqspi_callback | HAL_XQSPI Callback function definition
C_hmac_handle | HMAC handle Structure definition
C_hmac_init | HMAC init Structure definition
C_i2c_handle | I2C handle Structure definition
C_i2c_init | I2C Configuration Structure definition
C_i2s_handle | I2S handle Structure definition
C_i2s_init | I2S init Structure definition
C_iso7816_handle_t | ISO7816 handle Structure definition
C_keyram_mask | EFuse Keyram Structure definition
C_ll_adc_init | LL ADC init Structure definition
C_ll_aes_init | LL AES Init Structure definition
C_ll_aon_gpio_init | LL AON_GPIO init Structure definition
C_ll_bod_init | LL BOD init Structure definition
C_ll_cgc_init_t | LL CGC init Structure definition
C_ll_comp_init | LL COMP init Structure definition
C_ll_dma_init | LL DMA init Structure definition
C_ll_dual_timer_init | LL DUAL TIMER init Structure definition
C_ll_ecc_curve_init | LL PKC ECC P-256 Elliptic Curve Init Structure definition
C_ll_ecc_point | LL PKC ECC Point Structure definition
C_ll_gpio_init | LL GPIO init configuration definition
C_ll_hmac_init_t | LL HMAC Init Structure definition
C_ll_i2c_init | LL I2C init Structure definition
C_ll_i2s_init_t | LL I2S init structures definition
C_ll_iso7816_init | ISO7816_LL_init_structure LL ISO7816 init Structure definition
C_ll_msio_init | LL MSIO init Structure definition
C_ll_pkc_init | LL PKC Init Structure definition
C_ll_pwm_channel_init_t | LL PWM Output Channel init Structure definition
C_ll_pwm_init_t | LL PWM init Structure definition
C_ll_qspi_init_t | QSPI init structures definition
C_ll_rng_init | LL RNG Init Structure definition
C_ll_spim_init_t | LL SPIM init structures definition
C_ll_spis_init_t | SPIS init structures definition
C_ll_timer_init_t | LL TIMER init Structure definition
C_ll_uart_init_t | LL UART init Structure definition
C_ll_xqspi_init_t | XQSPI init structures definition
C_msio_init | MSIO init structure definition
C_pkc_big_number_add | PKC Big Number Addition expression input
C_pkc_big_number_multi | PKC Big Number Multiplication expression input
C_pkc_ecc_point_multi | PKC ECC Point Multiplication expression input
C_pkc_handle | PKC handle Structure definition
C_pkc_modular_add | PKC Modular Addition expression input
C_pkc_modular_compare | PKC Modular Comparison expression input
C_pkc_modular_shift | PKC Modular Left Shift expression input
C_pkc_modular_sub | PKC Modular Subtraction expression input
C_pkc_montgomery_inversion | PKC Montgomery Inversion expression input
C_pkc_montgomery_multi | PKC Montgomery Modular Multiplication expression input
C_pkc_rsa_modular_exponent | PKC RSA Modular Exponentiation expression input
C_qspi_command_t | QSPI command Structure definition
C_qspi_handle | QSPI handle Structure definition
C_qspi_init_t | QSPI init Structure definition
C_rng_handle | RNG handle Structure definition
C_rng_init | RNG init structure definition
C_spi_handle | SPI handle Structure definition
C_spi_init | SPI init Structure definition
C_timer_handle | TIMER handle Structure definition
C_timer_init | TIMER init Structure definition
C_uart_handle | UART handle Structure definition
C_uart_init | UART init structure definition
C_wdt_handle | WDT handle Structure definition
C_wdt_init | WDT init structure definition
C_xqspi_command_t | XQSPI command Structure definition
C_xqspi_handle_t | XQSPI handle Structure definition
C_xqspi_init_t | XQSPI init Structure definition
C adc_env_t | ADC device structure definition
C adc_trim_info_t | ADC trim parameter information definition
C aes_env_t | AES event structure definition
C ags_ack_packet_t | Alexa Gadget Service ACK packet
C ags_evt_t | Alexa Gadget Service event
C ags_header_base_t | Alexa Gadget Service base part of data packet header
C ags_header_first_ext_t | Alexa Gadget Service extended version of header in first packet
C ags_header_first_t | Alexa Gadget Service header in first packet
C ags_header_subs_ext_t | Alexa Gadget Service extended version of header in subsequent packets
C ags_header_subs_t | Alexa Gadget Service header in subsequent packets
C ags_init_t | Alexa Gadget Service init stucture
C ags_stream_env_t | Alexa Gadget Service gadget stream enviorenment variable
C ams_c_attr_info_t | Structure that stores attribute information
C ams_c_cmd_list_t | Structure that stores new command list
C ams_c_cplt_attr_data_t | Complete attribution's value
C ams_c_ett_attr_id_t | Structure that stores the attribute to be concerned or to display completely
C ams_c_evt_t | Apple Media Service Client event
C ams_c_handles_t | Handles on the connected peer device needed to interact with it
C ancs_c_att_handles_t | Ancs handle structure
C ancs_c_evt_t | ANCS Client event
C ancs_ntf_flags_t | Notification flags that can be performed for iOS notifications
C ans_c_ctrl_pt_t | Alert Notification Service Client Control Point value
C ans_c_evt_t | Alert Notification Service Client event
C ans_c_handles_t | Handles on the connected peer device needed to interact with it
C ans_c_new_alert_t | Alert Notification Service Client decoded New Alert value
C ans_c_unread_alert_t | Alert Notification Service Client decoded Unread Alert Status value
C ans_ctrl_pt_t | Alert Notification Service Control Point value
C ans_evt_t | Alert Notification Service event
C ans_init_t | Alert Notification Service init stucture
C ans_new_alert_t | Alert Notification Service New Alert value
C ans_unread_alert_t | Alert Notification Service Unread Alert Status value
C aon_aon_wdt_env_t | AON_WDT device structure definition
C app_adc_dma_cfg_t | ADC DMA configuration Structures
C app_adc_evt_t | ADC event structure definition
C app_adc_params_t | ADC parameters structure definition
C app_adc_pin_cfg_t | ADC pins config Structures
C app_adc_pin_t | ADC pins Structures
C app_aes_evt_t | AES event structure definition
C app_aes_params_t | AES parameters structure definition
C app_aon_wdt_params_t | AON_WDT parameters structure definition
C app_comp_params_t | COMP parameters structure definition
C app_comp_pin_cfg_t | COMP pins config Structures
C app_comp_pin_t | COMP pins Structures
C app_dma_params_t | DMA parameters structure definition
C app_dual_tim_params_t | DUAL_TIM parameters structure definition
C app_gpiote_param_t | GPIOTE Interrupt parameters structure definition
C app_hmac_evt_t | HMAC event structure definition
C app_hmac_params_t | HMAC parameters structure definition
C app_i2c_dma_cfg_t | I2C operate mode Enumerations definition
C app_i2c_evt_t | I2C event structure definition
C app_i2c_params_t | I2C parameters structure definition
C app_i2c_pin_cfg_t | I2C pins config Structures
C app_i2c_pin_t | I2C pins Structures
C app_i2s_dma_cfg_t | I2S operate mode Enumerations definition
C app_i2s_evt_t | I2S event structure definition
C app_i2s_params_t | I2S parameters structure definition
C app_i2s_pin_cfg_t | I2S pins config Structures
C app_i2s_pin_t | I2S pins Structures
C app_io_evt_t | GPIO Interrupt event Structure definition
C app_io_init_t | GPIO parameter structure definition
C app_iso7816_evt_t | ISO7816 event structure definition
C app_iso7816_params_t | ISO7816 parameters structure definition
C app_iso7816_pin_cfg_t | ISO7816 pin configure structure definition
C app_iso7816_pin_t | ISO7816 IO configuration Structures
C app_pkc_evt_t | PKC event structure definition
C app_pkc_params_t | PKC parameters structure definition
C app_pwm_channel_init_t | PWM Channel init Structure definition
C app_pwm_params_t | PWM parameters structure definition
C app_pwm_pin_cfg_t | PWM configuration Structures
C app_pwm_pin_t | PWM IO configuration Structures
C app_qspi_dma_cfg_t | QSPI DMA configuration structure definition
C app_qspi_evt_t | QSPI event structure definition
C app_qspi_params_t | QSPI parameters structure definition
C app_qspi_pin_cfg_t | QSPI configuration Structures
C app_qspi_pin_t | QSPI IO configuration Structures
C app_rng_evt_t | RNG event structure definition
C app_rng_params_t | RNG parameters structure definition
C app_rtc_evt_t | RTC event structure definition
C app_sleep_callbacks_t | PWR sleep check function Structure
C app_spi_dma_cfg_t | SPI configuration definition
C app_spi_evt_t | SPI event structure definition
C app_spi_params_t | SPI parameters structure definition
C app_spi_pin_cfg_t | SPI IO configuration Structures
C app_spi_pin_t | SPI IO Structures
C app_spi_screen_config_t | SPI SCreen Config Structures
C app_tim_params_t | TIM parameters structure definition
C app_uart_dma_cfg_t | UART DMA configuration structure definition
C app_uart_evt_t | UART event structure definition
C app_uart_params_t | UART parameters structure definition
C app_uart_pin_cfg_t | UART pins config Structures
C app_uart_pin_t | UART pins Structures
C app_uart_tx_buf_t | UART buffer structure definition
C bas_c_evt_t | Battery Service Client event
C bas_c_handles_t | Handles on the connected peer device needed to interact with it
C bas_evt_t | Battery Service event
C bas_init_t | Battery Service init structure
C bcs_evt_t | Body Composition Service event
C bcs_init_t | Body Composition Service Init variable
C bcs_meas_flag_t | Body composition Measurement flag data
C bcs_meas_val_t | Body composition Measurement data
C birth_date_t | UDS Characteristic - birthdate's structure
C ble_dis_c_read_rsp_t | Device Information Service Client Read Response encode structure
C ble_evt_t | BLE Event Information
C ble_gap_addr_t | The struct of address
C ble_gap_adv_param_t | Advertising parameters for legacy advertising
C ble_gap_adv_period_cfg_t | Configuration for periodic advertising
C ble_gap_adv_prim_cfg_t | Configuration for advertising on primary channel
C ble_gap_adv_second_cfg_t | Configuration for advertising on secondary channel
C ble_gap_adv_time_param_t | Advertising timing parameter
C ble_gap_bdaddr_t | The struct of broadcast address with broadcast type
C ble_gap_bond_dev_list_t | Bonded device list
C ble_gap_chnl_map_t | Channel map structure
C ble_gap_con_plan_tag_t | The Structure for BLE Connection Arrangement
C ble_gap_conn_info_t | Connection info
C ble_gap_conn_param_t | The parameter of connection
C ble_gap_conn_update_param_t | The parameter of update connection
C ble_gap_dev_adv_tx_power_t | TX power info struct
C ble_gap_dev_info_t | Device info
C ble_gap_dev_rf_path_comp_ind_t | RF path compensation values info
C ble_gap_dev_tx_power_t | TX power info struct
C ble_gap_dev_version_ind_t | The struct of device version
C ble_gap_evt_adv_report_t | Advertising report event for BLE_GAPM_EVT_ADV_REPORT
C ble_gap_evt_adv_stop_t | Advertising Stop info
C ble_gap_evt_conn_info_t | Get Connection info event for BLE_GAPC_EVT_CONN_INFO_GOT
C ble_gap_evt_conn_param_update_req_t | Connection parameter update request event for BLE_GAPC_EVT_CONN_PARAM_UPDATE_REQ
C ble_gap_evt_conn_param_updated_t | Connection parameter updated event for BLE_GAPC_EVT_CONN_PARAM_UPDATED
C ble_gap_evt_connected_t | Connection complete event for BLE_GAPC_EVT_CONNECTED
C ble_gap_evt_data_length_t | Data Length Updated event for BLE_GAPC_EVT_DATA_LENGTH_UPDATED
C ble_gap_evt_dev_info_get_t | Get device info event for BLE_GAPC_EVT_DEV_INFO_GOT
C ble_gap_evt_disconnected_t | Disconnection event for BLE_GAPC_EVT_DISCONNECTED
C ble_gap_evt_peer_info_t | Get peer info event for BLE_GAPC_EVT_PEER_INFO_GOT
C ble_gap_evt_peer_name_get_t | Name of peer device indication event for BLE_GAPC_EVT_PEER_NAME_GOT
C ble_gap_evt_phy_update_t | PHY update event for BLE_GAPC_EVT_PHY_UPDATED
C ble_gap_evt_rslv_addr_read_t | Read resolvable address event for BLE_GAPM_EVT_READ_RSLV_ADDR
C ble_gap_evt_rslv_addr_report_t | Resolvable address report event for BLE_GAPM_EVT_RSLV_ADDR_REPORT
C ble_gap_evt_scan_req_t | Scan request info
C ble_gap_evt_scan_stop_t | Scan Stop info struct
C ble_gap_evt_sync_established_t | Sync established event for BLE_GAPM_EVT_SYNC_ESTABLISH
C ble_gap_ext_adv_param_t | Advertising parameters for extended advertising and periodic advertising
C ble_gap_ext_conn_param_t | Connection parameters
C ble_gap_ext_init_param_t | Extended initiating parameters
C ble_gap_ext_scan_param_t | Parameters for extended scanning
C ble_gap_get_bd_addr_t | Get broadcast address struct
C ble_gap_init_param_t | Legacy initiating parameters
C ble_gap_le_phy_ind_t | PHY info
C ble_gap_lepsm_register_t | LE Protocol/Service Multiplexer information
C ble_gap_max_adv_data_len_ind_t | Maximum advertising data length info
C ble_gap_max_data_len_t | Max data length info struct
C ble_gap_nb_adv_sets_t | Number of available advertising sets info
C ble_gap_peer_features_ind_t | LE features info
C ble_gap_peer_info_t | LE peer info
C ble_gap_peer_version_ind_t | Peer version info
C ble_gap_per_sync_param_t | Periodic advertising synchronization parameters
C ble_gap_period_adv_addr_cfg_t | Periodic advertising information
C ble_gap_period_adv_list_t | Periodic advertising list
C ble_gap_ral_dev_info_t | RPA list item info
C ble_gap_ral_dev_list_t | RPA list info
C ble_gap_scan_param_t | Parameters for legacy scanning
C ble_gap_scan_wd_op_param_t | Scan Window operation parameters
C ble_gap_sec_key_t | Security key
C ble_gap_set_pref_slave_evt_dur_param_t | Set preference slave event duration
C ble_gap_sugg_dflt_data_len_t | Suggested default data length info
C ble_gap_white_list_t | White list
C ble_gapc_evt_t | BLE GAPC event structure
C ble_gapm_evt_t | BLE GAPM event structure
C ble_gatt_common_evt_mtu_exchange_t | GATT MTU Exchange event for BLE_GATT_COMMON_EVT_MTU_EXCHANGE
C ble_gatt_common_evt_prf_reg_t | GATT Server Profile Register event for BLE_GATT_COMMON_EVT_PRF_REGISTER
C ble_gatt_common_evt_t | GATT Common structure
C ble_gattc_browse_attr_char_t | GATTC Browse information about Characteristic
C ble_gattc_browse_attr_info | GATTC Browse attribute information
C ble_gattc_browse_attr_t | GATTC Browse information about Attribute
C ble_gattc_browse_inc_srvc_t | GATTC Browse information about Included Service
C ble_gattc_char_t | GATT characteristic
C ble_gattc_desc_t | GATT descriptor
C ble_gattc_disc_char_t | GATTC discovery characteristic structure
C ble_gattc_evt_browse_srvc_t | GATTC Browse service(s) event for BLE_GATTC_EVT_SRVC_BROWSE
C ble_gattc_evt_char_desc_disc_t | GATT characteristic descriptor discovery event for BLE_GATTC_EVT_CHAR_DESC_DISC
C ble_gattc_evt_char_disc_t | GATT characteristic discovery event for BLE_GATTC_EVT_CHAR_DISC
C ble_gattc_evt_incl_disc_t | GATT include discovery event for BLE_GATTC_EVT_INCLUDE_SRVC_DISC
C ble_gattc_evt_ntf_ind_t | GATTC Notification and Indication event for BLE_GATTC_EVT_NTF_IND
C ble_gattc_evt_read_t | GATT Client Read response event for BLE_GATTC_EVT_READ_RSP
C ble_gattc_evt_srvc_disc_t | GATT service discovery event for BLE_GATTC_EVT_PRIMARY_SRVC_DISC
C ble_gattc_evt_t | BLE GATTC event structure
C ble_gattc_evt_write_t | GATT Client Write Response event for BLE_GATTC_EVT_WRITE_RSP
C ble_gattc_include_t | GATT include
C ble_gattc_multiple_att_t | Read Multiple Handles
C ble_gattc_read_by_uuid_t | GATTC read by characteristic UUID structure
C ble_gattc_read_multiple_t | GATTC Read Multiple
C ble_gattc_read_value_t | GATT Client Read value
C ble_gattc_service_t | GATT service
C ble_gattc_write_attr_value_t | GATTC write attribute value structure
C ble_gattc_write_no_resp_t | GATTC write without response structure
C ble_gatts_attm_desc_128_t | Service(128 bits UUID) description
C ble_gatts_attm_desc_t | Service(16-bit UUID) description
►C ble_gatts_create_db_t | Parameter of Added service description
C attribute_table | < Attribute table
C ble_gatts_evt_cccd_rec_t | Gatt cccd recovery event for BLE_GATTS_EVT_CCCD_RECOVERY
C ble_gatts_evt_inited_ind_t | GATTS Database Inited Indication event structure
C ble_gatts_evt_ntf_ind_t | Gatt Notification or indication event for BLE_GATTS_EVT_NTF_IND
C ble_gatts_evt_prep_write_t | GATT prepare write request event for BLE_GATTS_EVT_PREP_WRITE_REQUEST
C ble_gatts_evt_read_t | GATT read request event for BLE_GATTS_EVT_READ_REQUEST
C ble_gatts_evt_t | BLE GATTS event structure
C ble_gatts_evt_write_t | GATT write request event for BLE_GATTS_EVT_WRITE_REQUEST
C ble_gatts_noti_ind_t | GATT sending Notification or Indication event param description
C ble_gatts_prep_write_cfm_t | GATT prepare write result description
C ble_gatts_read_cfm_t | GATT read attribute result description
C ble_gatts_write_cfm_t | GATT write attribute result description
C ble_l2cap_evt_add_credits_cplt_t | L2cap Credits Add Completed event for BLE_GATTC_EVT_NTF_IND
C ble_l2cap_evt_add_credits_ind_t | L2cap Credits Add Indicate event for BLE_L2CAP_EVT_ADD_CREDITS_IND
C ble_l2cap_evt_conn_ind_t | L2cap Connected Indicate event for BLE_L2CAP_EVT_CONN_IND
C ble_l2cap_evt_conn_req_t | L2cap Connect Request event for BLE_L2CAP_EVT_CONN_REQ
C ble_l2cap_evt_disconnect_t | L2cap disconnect event for BLE_L2CAP_EVT_DISCONNECTED
C ble_l2cap_evt_sdu_recv_t | L2cap SDU Receive event for BLE_L2CAP_EVT_SDU_RECV
C ble_l2cap_evt_sdu_send_t | L2cap SDU Send event for BLE_L2CAP_EVT_SDU_SEND
C ble_l2cap_evt_t | BLE L2cap event structure
C ble_l2cap_lecb_add_credits_t | LE flow control credit packet parameter
C ble_l2cap_lecb_cfm_conn_t | LE credit based connection confirm parameter
C ble_l2cap_lecb_conn_req_t | The parameter of LE credit based connection request packet sending
C ble_l2cap_lecb_sdu_t | SDU packet parameter
C ble_sch_config_t | BLE Scheduler configure defination
C ble_sec_cfm_enc_data_t | SEC Confirm encryption data
C ble_sec_cfm_enc_t | SEC Confirm encryption
C ble_sec_enc_req_data_t | SEC encryption request data
C ble_sec_evt_enc_ind_t | Link Encrypted event for BLE_SEC_EVT_LINK_ENCRYPTED
C ble_sec_evt_enc_req_t | Link Encrypte Request event for BLE_SEC_EVT_LINK_ENC_REQUEST
C ble_sec_evt_key_missing_t | Key Missing event for BLE_SEC_EVT_KEY_MISSING
C ble_sec_evt_keypress_notify_t | Key Press Notify event for BLE_SEC_EVT_KEY_PRESS_NTF
C ble_sec_evt_t | BLE Security event structure
C ble_sec_nc_t | SEC number comparison value
C ble_sec_oob_t | SEC OOB value
C ble_sec_param_t | SEC Parameter
C ble_sec_tk_t | TK value
C ble_slp_config_t | BLE Sleep configure defination
C ble_uuid_t | GATT UUID structure
C bps_ieee_float16_t | SFLOAT format (IEEE-11073 16-bit FLOAT, defined as a 16-bit value with 12-bit mantissa and 4-bit exponent
C bps_init_t | Blood Pressure Service init stucture
C bps_meas_t | Blood Pressure measurement structure
C comp_env_t | COMP device structure definition
C cscs_evt_t | Cycling Speed and Cadence Service event
C cscs_init_t | Cycling Speed and Cadence Service init stucture
C cscs_meas_val_t | Cycling Speed and Cadence Measurement Character value structure
C cts_adj_info_t | CTS Adjust information
C cts_c_cur_time_t | Current Time value
C cts_c_evt_t | Current Time Service Client event
C cts_c_exact_time_256_t | Exact Time 256
C cts_c_handles_t | Handles on the connected peer device needed to interact with it
C cts_c_loc_time_info_t | Local Time Information
C cts_c_ref_time_info_t | Reference Time Information
C cts_cur_time_t | CTS Current Time value
C cts_evt_t | Current Time Service event
C cts_exact_time_256_t | CTS Exact Time 256
C cts_init_t | Current Time Service init structure
C cts_loc_time_info_t | CTS Local Time Information
C cts_ref_time_info_t | CTS Reference Time Information
C cts_updata_ref_time_info_t | CTS Reference Time Updata Information
C dfu_boot_info_t | Boot information definition
C dfu_func_t | DFU used functions config definition
C dfu_image_info_t | Image information definition
C dfu_pro_callback_t | DFU program state callback definition
C dfu_receive_frame_t | DFU frame information definition
C dfu_spi_flash_func_t | SPI used functions config definition
C dis_c_evt_t | Device Information Service Client event
C dis_c_handles_t | Handles on the connected peer device needed to interact with it
C dis_c_pnp_id_t | Response data for PnP ID parameters
C dis_c_reg_cert_data_list_t | Response data for IEEE 11073-20601 Regulatory Certification Data List Structure
C dis_c_string_t | Response data for string-based DIS characteristics
C dis_c_sys_id_t | Response data for System ID parameters
C dis_init_t | Device Information Service init structure
C dis_pnp_id_t | PnP ID parameters
C dis_reg_cert_data_list_t | IEEE 11073-20601 Regulatory Certification Data List Structure
C dis_string_t | UTF-8 string data type
C dis_sys_id_t | System ID parameters
C dma_env_t | DMA device structure definition
C dss_evt_t | Device Synchronize Service Synchronize event
C dual_tim_env_t | DUAL_TIM device structure definition
C gap_slv_pref_t | Slave preferred connection parameters
C gdx_lcp_config_t | LCP Parameter
C gls_evt_t | Glucose Service event
C gls_ieee_float16_t | SFLOAT format (IEEE-11073 16-bit FLOAT, defined as a 16-bit value with 12-bit mantissa and 4-bit exponent)
C gls_init_t | Glucose Service init stucture
C gls_meas_ctx_t | Glucose measurement context structure
C gls_meas_val_t | Glucose Measurement structure
C gls_racp_filter_t | Glucose Recoerd Access Control Point filter value
C gls_racp_req_t | Glucose Recoerd Access Control Point request value
C gls_racp_rsp_t | Glucose Recoerd Access Control Point response value
C gls_rec_t | Glucose measurement record
C gr55xx_chip_config_t | GR55XX Chip configure defination
C gus_c_evt_t | Goodix UART Service Client event
C gus_c_handles_t | Handles on the connected peer device needed to interact with it
C gus_evt_t | Goodix UART Service event
C gus_init_t | Goodix UART Service init stucture
C hci_uart_call_t | The function pointers for HCI UART
C hids_evt_t | HID Service event
C hids_hid_info_t | HID Information characteristic value
C hids_init_t | HID Service initialization variable
C hids_report_int_t | HID Service Report characteristic define
C hids_report_map_t | HID Service Report Map characteristic value
C hids_report_ref_t | Value of a Report Reference descriptor
C hmac_env_t | HMAC event structure definition
C hrrcps_evt_t | HRS RSCS Relay Control Point Service event
C hrrcps_rsp_val_t | HRS RSCS Relay Control Point Response value
C hrs_c_evt_t | Heart Rate Service Client event
C hrs_c_handles_t | Handles on the connected peer device needed to interact with it
C hrs_c_hr_meas_t | Heart Rate Measurement characteristic value structure
C hrs_evt_t | Heart Rate Service event
C hrs_init_t | Heart Rate Service Init variable
C hts_evt_t | Health Thermometer Service event
C hts_init_t | Health Thermometer Service init stucture
C hts_meas_val_t | Health Theromometer Measurement Character value structure
C i2c_env_t | I2C device structure definition
C i2s_env_t | I2S device structure definition
C ias_c_evt_t | Immediate Alert Service Client event
C ias_c_handles_t | Handles on the connected peer device needed to interact with it
C ias_evt_t | Immediate Alert Service event
C ias_init_t | Immediate Alert Service init stucture
C ieee_float32_t | SFLOAT format (IEEE-11073 32-bit FLOAT, defined as a 32-bit vlue with 24-bit mantissa and 8-bit exponent
C iso7816_env_t | ISO7816 device structure definition
C iso7816_init_t | ISO7816_init_structure ISO7816 init structure definition
C link_node | ADC sample-node definition
C link_rx_info_t | Link RX information definition
C lls_c_evt_t | Link Loss Service Client event
C lls_c_handles_t | Handles on the connected peer device needed to interact with it
C lls_evt_t | Link Loss Service event
C lls_init_t | Link Loss Service init stucture
C lms_evt_t | LMS Service event
C lms_init_t | LMS Service initialization variable
C lns_evt_t | Log Notification Service event
C lns_log_data_t | Log Information data
C mlmr_c_evt_t | Multi Link Multi Role Service Client event
C mlmr_c_handles_t | Handles on the connected peer device needed to interact with it
C mlmr_evt_t | Multi Link Multi Role Service event
C mlmr_init_t | Multi Link Multi Role Service init stucture
C ndcs_time_dst_t | Time with DST
C ntf_source_pdu_t | IOS notification structure
C otas_c_evt_t | OTA Service Client event
C otas_c_handles_t | Handles on the connected peer device needed to interact with it
C otas_evt_t | OTA Service event
C otas_init_t | OTA Service initialization variable
C pass_c_evt_t | Phone Alert Status Client Service event
C pass_c_handles_t | Handles on the connected peer device needed to interact with it
C pass_evt_t | Phone Alert Status Service event
C pass_init_t | Phone Alert Status Service init stucture
C pcs_evt_t | PCS Service event
C pcs_init_t | PCS Service init stucture
C pkc_env_t | PKC device structure definition
C pkc_init_t | PKC Init Structure definition
C pmu_trim_info_t | PMU trim parameter information definition
C prf_att_info_t | Attribute information
C prf_char_pres_fmt_t | Characteristic Presentation Format Descriptor structure
C prf_date_time_t | The date and time structure
C pwm_channel_init_t | PWM Channel init Structure definition
C pwm_env_t | PWM device structure definition
C pwm_handle_t | PWM handle Structure definition
C pwm_init_t | PWM init Structure definition
C pwr_mgmt_var_box_t | Power manager setting parameter
C pwr_table_t | Parameter configuration table
C qspi_env_t | QSPI device structure definition
C rf_trim_info_t | RF trim parameter information definition
C rng_env_t | RNG device structure definition
C rscs_c_evt_t | Running Speed and Cadence Service Client event
C rscs_c_handles_t | Handles on the connected peer device needed to interact with it
C rscs_c_meas_val_t | Running Speed and Cadence Measurement Character value structure
C rscs_evt_t | Running Speed and Cadence Service event
C rscs_init_t | Running Speed and Cadence Service init stucture
C rscs_meas_val_t | Running Speed and Cadence Measurement Character value structure
C rtus_evt_t | RTUS Event data
C rtus_init_t | Reference Time Update Service init structure
C rtus_update_state_t | RTUS Time Update State
C samples_evt_t | Sample Service event
C samples_init_t | Sample Service init stucture
C sdk_version_t | SDK version definition
C spi_env_t | SPI device structure definition
C stack_heaps_table_t | The table contains the pointers to four arrays which are used as heap memory by BLE stack in ROM
C sys_assert_cb_t | Assert callbacks
C ths_c_evt_t | Throughput Service Client event
C ths_c_handles_t | Handles on the connected peer device needed to interact with it
C ths_evt_t | Throughput Service event
C ths_init_t | Throughput Service init stucture
C thscps_adv_param_t | THS Control Point Advertising Parameters
C thscps_evt_t | THS Control Point Service event
C thscps_rsp_val_t | THS Control Point Response value
C thscps_setting_t | THS Setting Information value
C thscps_test_conn_info_t | THS connect Information value
C thscps_test_info_t | THS Test Information value
C tim_env_t | TIM device structure definition
C tps_c_evt_t | Tx Power Service Client event
C tps_c_handles_t | Handles on the connected peer device needed to interact with it
C tps_init_t | Tx Power Servic init stucture
C uart_env_t | UART device structure definition
C uds_chars_flag_t | UDS Characteristics Flags structure
C uds_chars_val_t | UDS Characteristics value structure
C uds_evt_t | User Data Service event
C uds_init_t | User Data Service init structure
C uds_regi_user_data_flag_t | Registered User Data Flags structure
C uds_regi_user_data_stream_t | UDS Registered User Data stream
C wechat_data_t | WeChat service data
C wechat_evt_t | WeChat Service event
C wechat_init_t | WeChat Service Init variable
C wechat_pedo_meas_t | WeChat current pedometer measurement variable
C wechat_pedo_target_t | WeChat pedometer target variable
C wss_evt_t | Weight Scale Service event
C wss_init_t | Weight Scale Service Init variable
C wss_meas_val_t | Weight Scale Measurement data