Enumerations
HAL ADC State
Peripheral Driver » HAL Driver » ADC » Enumerations
Collaboration diagram for HAL ADC State:

## Enumerations
enum | hal_adc_state_t { HAL_ADC_STATE_RESET = 0x00, HAL_ADC_STATE_READY = 0x01, HAL_ADC_STATE_BUSY = 0x02, HAL_ADC_STATE_ERROR = 0x04 }
| HAL ADC State Enumerations definition. More...

## Detailed Description

## Enumeration Type Documentation

## ◆ hal_adc_state_t

enum hal_adc_state_t

HAL ADC State Enumerations definition.

Enumerator
HAL_ADC_STATE_RESET | Peripheral not initialized
HAL_ADC_STATE_READY | Peripheral initialized and ready for use
HAL_ADC_STATE_BUSY | An internal process is ongoing
HAL_ADC_STATE_ERROR | Peripheral in error

Definition at line 76 of file gr55xx_hal_adc.h.