### - h -

- H : _ll_ecc_curve_init
- handle : adc_env_t , aes_env_t , aon_aon_wdt_env_t , ble_gattc_browse_attr_char_t , ble_gattc_evt_ntf_ind_t , ble_gattc_evt_write_t , ble_gattc_multiple_att_t , ble_gattc_read_value_t , ble_gattc_write_attr_value_t , ble_gattc_write_no_resp_t , ble_gatts_evt_cccd_rec_t , ble_gatts_evt_ntf_ind_t , ble_gatts_evt_prep_write_t , ble_gatts_evt_read_t , ble_gatts_evt_write_t , ble_gatts_noti_ind_t , ble_gatts_prep_write_cfm_t , ble_gatts_read_cfm_t , ble_gatts_write_cfm_t , comp_env_t , dma_env_t , dual_tim_env_t , hmac_env_t , i2c_env_t , i2s_env_t , iso7816_env_t , pkc_env_t , prf_att_info_t , pwm_env_t , qspi_env_t , rng_env_t , rscs_c_evt_t , spi_env_t , tim_env_t , uart_env_t
- handle_count : ble_gattc_read_multiple_t
- handle_decl : ble_gattc_char_t
- handle_value : ble_gattc_char_t
- hba1c : gls_meas_ctx_t
- hci_subver : ble_gap_dev_version_ind_t
- hci_ver : ble_gap_dev_version_ind_t
- header_base : ags_ack_packet_t , ags_header_first_ext_t , ags_header_first_t , ags_header_subs_ext_t , ags_header_subs_t
- height : bcs_meas_val_t , uds_chars_val_t , wss_meas_val_t
- height_present : bcs_meas_flag_t , uds_chars_flag_t
- hid_info : hids_init_t
- hmac_done_callback : _hal_hmac_callback
- hmac_env : app_hmac_params_t
- hmac_error_callback : _hal_hmac_callback
- hmac_mask : _keyram_mask
- hmac_msp_deinit : _hal_hmac_callback
- hmac_msp_init : _hal_hmac_callback
- hmac_state : hmac_env_t
- host_subver : ble_gap_dev_version_ind_t
- host_ver : ble_gap_dev_version_ind_t
- hour : _calendar_alarm , _calendar_time , prf_date_time_t
- hours_since_update : cts_c_ref_time_info_t , cts_ref_time_info_t
- hperiod : pwm_init_t
- hprescaler : _ll_pwm_init_t
- hr_meas_buff : hrs_c_evt_t
- hr_value : hrs_c_hr_meas_t
- hrs_ctrl_point_handle : hrs_c_handles_t
- hrs_hr_meas_cccd_handle : hrs_c_handles_t
- hrs_hr_meas_handle : hrs_c_handles_t
- hrs_sensor_loc_handle : hrs_c_handles_t
- hrs_srvc_end_handle : hrs_c_handles_t
- hrs_srvc_start_handle : hrs_c_handles_t
- hw_flow_ctrl : _ll_uart_init_t , _uart_init
- hw_rev_str : dis_init_t