Public Attributes | List of all members
hids_hid_info_t Struct Reference
BLE Services » Human Input Device Service (HIDS) » Typedefs

HID Information characteristic value. More...

`#include <hids.h>`

## Public Attributes
uint16_t | bcd_hid
| 16-bit unsigned integer representing version number of base USB HID Specification implemented by HID Device More...
uint8_t | b_country_code
| Identifies which country the hardware is localized for. More...
uint8_t | flags
| See http://developer.bluetooth.org/gatt/characteristics/Pages/CharacteristicViewer.aspx?u=org.bluetooth.characteristic.hid_information.xml. More...

## Detailed Description

HID Information characteristic value.

Definition at line 157 of file hids.h.

## Member Data Documentation

## ◆ b_country_code

uint8_t hids_hid_info_t::b_country_code

Identifies which country the hardware is localized for.

Most hardware is not localized and thus this value would be zero (0).

Definition at line 160 of file hids.h.

## ◆ bcd_hid

uint16_t hids_hid_info_t::bcd_hid

16-bit unsigned integer representing version number of base USB HID Specification implemented by HID Device

Definition at line 159 of file hids.h.

## ◆ flags

uint8_t hids_hid_info_t::flags

See http://developer.bluetooth.org/gatt/characteristics/Pages/CharacteristicViewer.aspx?u=org.bluetooth.characteristic.hid_information.xml.

Definition at line 161 of file hids.h.

The documentation for this struct was generated from the following file:

- hids.h