Macros
ADC Buffered Internal Reference Value
Peripheral Driver » LL Driver » ADC » Defines » ADC Exported Constants
Collaboration diagram for ADC Buffered Internal Reference Value:

## Macros
#define | LL_ADC_REF_VALUE_0P8 (0x3UL << AON_SNSADC_CFG_REF_VALUE_Pos)
| Reference = 0.85 V. More...
#define | LL_ADC_REF_VALUE_1P2 (0x7UL << AON_SNSADC_CFG_REF_VALUE_Pos)
| Reference = 1.28 V. More...
#define | LL_ADC_REF_VALUE_1P6 (0xAUL << AON_SNSADC_CFG_REF_VALUE_Pos)
| Reference = 1.60 V. More...

## Detailed Description

## Macro Definition Documentation

## ◆ LL_ADC_REF_VALUE_0P8

#define LL_ADC_REF_VALUE_0P8 (0x3UL << AON_SNSADC_CFG_REF_VALUE_Pos)

Reference = 0.85 V.

Definition at line 138 of file gr55xx_ll_adc.h.

## ◆ LL_ADC_REF_VALUE_1P2

#define LL_ADC_REF_VALUE_1P2 (0x7UL << AON_SNSADC_CFG_REF_VALUE_Pos)

Reference = 1.28 V.

Definition at line 139 of file gr55xx_ll_adc.h.

## ◆ LL_ADC_REF_VALUE_1P6

#define LL_ADC_REF_VALUE_1P6 (0xAUL << AON_SNSADC_CFG_REF_VALUE_Pos)

Reference = 1.60 V.

Definition at line 140 of file gr55xx_ll_adc.h.