### - r -

- RNG_LFSR_MODE_128BIT : gr55xx_hal_rng.h
- RNG_LFSR_MODE_59BIT : gr55xx_hal_rng.h
- RNG_OUTPUT_CYCLIC : gr55xx_hal_rng.h
- RNG_OUTPUT_CYCLIC_PARITY : gr55xx_hal_rng.h
- RNG_OUTPUT_FR0_S0 : gr55xx_hal_rng.h
- RNG_OUTPUT_LFSR : gr55xx_hal_rng.h
- RNG_OUTPUT_LFSR_RNG : gr55xx_hal_rng.h
- RNG_POST_PRO_COUNTING : gr55xx_hal_rng.h
- RNG_POST_PRO_NEUMANN : gr55xx_hal_rng.h
- RNG_POST_PRO_NOT : gr55xx_hal_rng.h
- RNG_POST_PRO_SKIPPING : gr55xx_hal_rng.h
- RNG_SEED_FR0_S0 : gr55xx_hal_rng.h
- RNG_SEED_USER : gr55xx_hal_rng.h
- RSA_U32_LENGTH : gr55xx_ll_pkc.h
- RSCS_C_CONNECTION_MAX : rscs_c.h
- RSCS_C_ERROR_CCCD_INVALID : rscs_c.h
- RSCS_C_ERROR_PROC_IN_PROGRESS : rscs_c.h
- RSCS_C_FEAT_CALIBRATION_PROCEDURE_BIT : rscs_c.h
- RSCS_C_FEAT_INSTANT_STRIDE_LEN_BIT : rscs_c.h
- RSCS_C_FEAT_MULTIPLE_SENSORS_BIT : rscs_c.h
- RSCS_C_FEAT_RUNNING_OR_WALKING_STATUS_BIT : rscs_c.h
- RSCS_C_FEAT_TOTAL_DISTANCE_BIT : rscs_c.h
- RSCS_C_MEAS_FLAG_INST_STRIDE_LEN_BIT : rscs_c.h
- RSCS_C_MEAS_FLAG_RUNNING_OR_WALKING_BIT : rscs_c.h
- RSCS_C_MEAS_FLAG_TOTAL_DISTANCE_BIT : rscs_c.h
- RSCS_C_PT_RSP_LEN_MAX : rscs_c.h
- RSCS_CHAR_FULL : rscs.h
- RSCS_CHAR_MANDATORY : rscs.h
- RSCS_CHAR_SC_CTRL_POINT : rscs.h
- RSCS_CHAR_SENSOR_LOC_SUP : rscs.h
- RSCS_CONNECTION_MAX : rscs.h
- RSCS_CTRL_PT_RSP_LEN_MIN : rscs.h
- RSCS_CTRL_PT_VAL_LEN_MAX : rscs.h
- RSCS_ERROR_CCCD_INVALID : rscs.h
- RSCS_ERROR_PROC_IN_PROGRESS : rscs.h
- RSCS_FEAR_FULL_BIT : rscs.h
- RSCS_FEAT_CALIBRATION_PROCEDURE_BIT : rscs.h
- RSCS_FEAT_INSTANT_STRIDE_LEN_BIT : rscs.h
- RSCS_FEAT_MULTIPLE_SENSORS_BIT : rscs.h
- RSCS_FEAT_RUNNING_OR_WALKING_STATUS_BIT : rscs.h
- RSCS_FEAT_TOTAL_DISTANCE_BIT : rscs.h
- RSCS_FEAT_VAL_LEN_MAX : rscs.h
- RSCS_MEAS_FLAG_INST_STRIDE_LEN_BIT : rscs.h
- RSCS_MEAS_FLAG_RUNNING_OR_WALKING_BIT : rscs.h
- RSCS_MEAS_FLAG_TOTAL_DISTANCE_BIT : rscs.h
- RSCS_MEAS_VAL_LEN_MAX : rscs.h
- RSCS_SENSOR_LOC_VAL_LEN_MAX : rscs.h
- RTUS_CHAR_FULL : rtus.h
- RTUS_CONNECTION_MAX : rtus.h
- RTUS_CTRL_PT_VAL_LEN : rtus.h
- RTUS_UPDATE_STATE_VAL_LEN : rtus.h