Functions
FLAG Management
Peripheral Driver » LL Driver » RNG » Functions
Collaboration diagram for FLAG Management:

## Functions
__STATIC_INLINE uint32_t | ll_rng_is_active_flag_lr (rng_regs_t *RNGx)
| Indicate if the Flag of RNG long run test is set or not. More...
__STATIC_INLINE uint32_t | ll_rng_is_active_flag_sts (rng_regs_t *RNGx)
| Indicate if the RNG Status Flag is set or not. More...
__STATIC_INLINE void | ll_rng_clear_flag_sts (rng_regs_t *RNGx)
| Clear RNG Status flag. More...

## Detailed Description

## Function Documentation

## ◆ ll_rng_clear_flag_sts()

__STATIC_INLINE void ll_rng_clear_flag_sts | ( | rng_regs_t * | RNGx | ) |

Clear RNG Status flag.

\rst +-------------------—+--------------------------------—+ | Register | BitsName | +======================+===================================+ | STATUS | RNG_READY | +-------------------—+--------------------------------—+ \endrst

Parameters

  RNGx | RNG instance.

Return values

  None |

Definition at line 600 of file gr55xx_ll_rng.h.

## ◆ ll_rng_is_active_flag_lr()

__STATIC_INLINE uint32_t ll_rng_is_active_flag_lr | ( | rng_regs_t * | RNGx | ) |

Indicate if the Flag of RNG long run test is set or not.

Register | BitsName
--- | ---
LR_STATUS | RNG_LR_FLAG

Parameters

  RNGx | RNG instance.

Return values

  State | of bit (1 or 0).

Definition at line 562 of file gr55xx_ll_rng.h.

## ◆ ll_rng_is_active_flag_sts()

__STATIC_INLINE uint32_t ll_rng_is_active_flag_sts | ( | rng_regs_t * | RNGx | ) |

Indicate if the RNG Status Flag is set or not.

\rst +-------------------—+--------------------------------—+ | Register | BitsName | +======================+===================================+ | STATUS | RNG_READY | +-------------------—+--------------------------------—+ \endrst

Parameters

  RNGx | RNG instance.

Return values

  State | of bit (1 or 0).

Definition at line 581 of file gr55xx_ll_rng.h.