Enumerations
Enumerations
Peripheral Driver » APP DRIVER » SPI
Collaboration diagram for Enumerations:

## Enumerations
enum | app_spi_id_t { APP_SPI_ID_SLAVE, APP_SPI_ID_MASTER, APP_SPI_ID_MAX }
| SPI module Enumerations definition. More...
enum | app_spi_evt_type_t { APP_SPI_EVT_ERROR, APP_SPI_EVT_TX_CPLT, APP_SPI_EVT_RX_CPLT, APP_SPI_EVT_TX_RX_CPLT, APP_SPI_EVT_ABORT }
| SPI event Enumerations definition. More...
enum | app_spi_state_t { APP_SPI_INVALID = 0, APP_SPI_ACTIVITY }
| App spi state types. More...
enum | app_spi_dma_state_t { APP_SPI_DMA_INVALID = 0, APP_SPI_DMA_ACTIVITY }
| App spi dma state types. More...

## Detailed Description

## Enumeration Type Documentation

## ◆ app_spi_dma_state_t

enum app_spi_dma_state_t

App spi dma state types.

Enumerator
APP_SPI_DMA_INVALID |
APP_SPI_DMA_ACTIVITY |

Definition at line 192 of file app_spi.h.

## ◆ app_spi_evt_type_t

enum app_spi_evt_type_t

SPI event Enumerations definition.

Enumerator
APP_SPI_EVT_ERROR | Error reported by UART peripheral.
APP_SPI_EVT_TX_CPLT | Requested TX transfer completed.
APP_SPI_EVT_RX_CPLT | Requested RX transfer completed.
APP_SPI_EVT_TX_RX_CPLT | Requested TX/RX transfer completed.
APP_SPI_EVT_ABORT | Abort reported by SPI peripheral.

Definition at line 100 of file app_spi.h.

## ◆ app_spi_id_t

enum app_spi_id_t

SPI module Enumerations definition.

Note
  : 1. When the SPI device is configured as a Slave mode, the pull-up or pull-down mode of the CS pin should be set according to the clock polarity: if the clock polarity is configured for low level active, the CS pin should be configured as pull-up mode; if the clock polarity is configured for high level active, the CS pin should be configured as pull-down mode.
  1. It is recommended that when initializing the SPI Slave device, the SPI Master device should first be initialized and in a stable state to avoid interference to the Slave device from I/O signal changes during the Master device's initialization.

Enumerator
APP_SPI_ID_SLAVE | SPI slave module.
APP_SPI_ID_MASTER | SPI master module.
APP_SPI_ID_MAX | Only for check parameter, not used as input parameters.

Definition at line 89 of file app_spi.h.

## ◆ app_spi_state_t

enum app_spi_state_t

App spi state types.

Enumerator
APP_SPI_INVALID |
APP_SPI_ACTIVITY |

Definition at line 182 of file app_spi.h.