Macros
RTS Pin State
Peripheral Driver » LL Driver » UART » Defines » UART Exported Constants
Collaboration diagram for RTS Pin State:

## Macros
#define | LL_UART_RTSPIN_STATE_ACTIVE 0x00000001U
| RTS pin active(Logic 1) More...
#define | LL_UART_RTSPIN_STATE_INACTIVE 0x00000000U
| RTS pin inactive(Logic 0) More...

## Detailed Description

## Macro Definition Documentation

## ◆ LL_UART_RTSPIN_STATE_ACTIVE

#define LL_UART_RTSPIN_STATE_ACTIVE 0x00000001U

RTS pin active(Logic 1)

Definition at line 207 of file gr55xx_ll_uart.h.

## ◆ LL_UART_RTSPIN_STATE_INACTIVE

#define LL_UART_RTSPIN_STATE_INACTIVE 0x00000000U

RTS pin inactive(Logic 0)

Definition at line 208 of file gr55xx_ll_uart.h.