Enumerations
Enumerations
SYSTEM » Non-Volatile Data Storage
Collaboration diagram for Enumerations:

## Enumerations
enum | NVDS_STATUS { NVDS_SUCCESS, NVDS_FAIL, NVDS_TAG_NOT_EXISTED, NVDS_SPACE_NOT_ENOUGH, NVDS_LENGTH_OUT_OF_RANGE, NVDS_INVALID_PARA, NVDS_INVALID_START_ADDR, NVDS_INVALID_SECTORS, NVDS_COMPACT_FAILED, NVDS_STORAGE_ACCESS_FAILED, NVDS_GC_COMPLETE, NVDS_NOT_INIT, NVDS_POINTER_NULL }
| NVDS Returned Status. More...

## Detailed Description

## Enumeration Type Documentation

## ◆ NVDS_STATUS

enum NVDS_STATUS

NVDS Returned Status.

Enumerator
NVDS_SUCCESS | NVDS succeeds.
NVDS_FAIL | NVDS failed.
NVDS_TAG_NOT_EXISTED | NVDS tag does not exist.
NVDS_SPACE_NOT_ENOUGH | NVDS space is not enough.
NVDS_LENGTH_OUT_OF_RANGE | NVDS length out of range.
NVDS_INVALID_PARA | NVDS invalid params.
NVDS_INVALID_START_ADDR | NVDS invalid start address.
NVDS_INVALID_SECTORS | NVDS invalid sector.
NVDS_COMPACT_FAILED | NVDS failed to compact sectors.
NVDS_STORAGE_ACCESS_FAILED | NVDS failed to access storage.
NVDS_GC_COMPLETE | NVDS garbage collection complete.
NVDS_NOT_INIT | NVDS not initialize.
NVDS_POINTER_NULL | NVDS or driver function repalce error: NULL.

Definition at line 68 of file gr55xx_nvds.h.