Macros
XQSPI Instruction Size, only in QSPI mode
Peripheral Driver » HAL Driver » XQSPI » Defines » XQSPI Exported Constants
Collaboration diagram for XQSPI Instruction Size, only in QSPI mode:

## Macros
#define | XQSPI_INSTSIZE_00_BITS (0)
| 0-bit (No Instruction) More...
#define | XQSPI_INSTSIZE_08_BITS (1)
| 8-bit Instruction More...
#define | XQSPI_INSTSIZE_16_BITS (2)
| 16-bit Instruction More...

## Detailed Description

## Macro Definition Documentation

## ◆ XQSPI_INSTSIZE_00_BITS

#define XQSPI_INSTSIZE_00_BITS (0)

0-bit (No Instruction)

Definition at line 307 of file gr55xx_hal_xqspi.h.

## ◆ XQSPI_INSTSIZE_08_BITS

#define XQSPI_INSTSIZE_08_BITS (1)

8-bit Instruction

Definition at line 308 of file gr55xx_hal_xqspi.h.

## ◆ XQSPI_INSTSIZE_16_BITS

#define XQSPI_INSTSIZE_16_BITS (2)

16-bit Instruction

Definition at line 309 of file gr55xx_hal_xqspi.h.