Macros
XQSPI Clock Speed
Peripheral Driver » HAL Driver » XQSPI » Defines » XQSPI Exported Constants
Collaboration diagram for XQSPI Clock Speed:

## Macros
#define | XQSPI_BAUD_RATE_64M LL_XQSPI_BAUD_RATE_64M
| Serial clock speed is 64 MHz More...
#define | XQSPI_BAUD_RATE_48M LL_XQSPI_BAUD_RATE_48M
| Serial clock speed is 48 MHz More...
#define | XQSPI_BAUD_RATE_32M LL_XQSPI_BAUD_RATE_32M
| Serial clock speed is 32 MHz More...
#define | XQSPI_BAUD_RATE_24M LL_XQSPI_BAUD_RATE_24M
| Serial clock speed is 24 MHz More...
#define | XQSPI_BAUD_RATE_16M LL_XQSPI_BAUD_RATE_16M
| Serial clock speed is 16 MHz More...

## Detailed Description

## Macro Definition Documentation

## ◆ XQSPI_BAUD_RATE_16M

#define XQSPI_BAUD_RATE_16M LL_XQSPI_BAUD_RATE_16M

Serial clock speed is 16 MHz

Definition at line 283 of file gr55xx_hal_xqspi.h.

## ◆ XQSPI_BAUD_RATE_24M

#define XQSPI_BAUD_RATE_24M LL_XQSPI_BAUD_RATE_24M

Serial clock speed is 24 MHz

Definition at line 282 of file gr55xx_hal_xqspi.h.

## ◆ XQSPI_BAUD_RATE_32M

#define XQSPI_BAUD_RATE_32M LL_XQSPI_BAUD_RATE_32M

Serial clock speed is 32 MHz

Definition at line 281 of file gr55xx_hal_xqspi.h.

## ◆ XQSPI_BAUD_RATE_48M

#define XQSPI_BAUD_RATE_48M LL_XQSPI_BAUD_RATE_48M

Serial clock speed is 48 MHz

Definition at line 280 of file gr55xx_hal_xqspi.h.

## ◆ XQSPI_BAUD_RATE_64M

#define XQSPI_BAUD_RATE_64M LL_XQSPI_BAUD_RATE_64M

Serial clock speed is 64 MHz

Definition at line 279 of file gr55xx_hal_xqspi.h.