Modules
Health Thermometer Service (HTS)
BLE Services

Definitions and prototypes for the HTS interface. More...

Collaboration diagram for Health Thermometer Service (HTS):

## Modules
| Defines
| Enumerations
| Structures
| Typedefs
| Functions

## Detailed Description

Definitions and prototypes for the HTS interface.

The Health Thermometer Service exposes temperature and other data related to a thermometer used for healthcare applications. This module implements the Health Thermometer Service with the Temperature Meaturement, Temperature Type, Intermediate Temperature, and Measurement Interval characteristics.

After hts_init_t variable is initialized, the application must call hts_service_init() to optionally add the Health Thermometer Service, Temperature Meaturement, Temperature Type, Intermediate Temperature, and Measurement Interval characteristics to the BLE stack database according to hts_init_t::char_mask. However the value of Temperature Type is stored within hts_init_t::temp_type which locates in user space.