Public Attributes | List of all members
_aon_wdt_init Struct Reference
Peripheral Driver » HAL Driver » AON_WDT » Structures » AON_WDT Configuration

AON_WDT_Configuration init structure definition. More...

`#include <gr55xx_hal_aon_wdt.h>`

## Public Attributes
uint32_t | counter
| Specifies the AON_WDT free-running downcounter value. More...
uint32_t | alarm_counter
| Specifies the AON_WDT downcounter alarm value before system reset. More...

## Detailed Description

AON_WDT_Configuration init structure definition.

Definition at line 75 of file gr55xx_hal_aon_wdt.h.

## Member Data Documentation

## ◆ alarm_counter

uint32_t _aon_wdt_init::alarm_counter

Specifies the AON_WDT downcounter alarm value before system reset.

When counter counts down to the alarm value, AON_WDT will generate an interrupt. After counter counts down to 0, AON_WDT will then request a SoC Reset.

This parameter can be a number ranging between 0x0U ~ 0x1FU, and the default value is 20U.

Definition at line 80 of file gr55xx_hal_aon_wdt.h.

## ◆ counter

uint32_t _aon_wdt_init::counter

Specifies the AON_WDT free-running downcounter value.

This parameter can be a number ranging between 0x0U ~ 0xFFFFFFFFU.

Definition at line 77 of file gr55xx_hal_aon_wdt.h.

The documentation for this struct was generated from the following file:

- gr55xx_hal_aon_wdt.h