pcs.h
Go to the documentation of this file.
1 /**
2 *****************************************************************************************
3 *
4 * @file pcs.h
5 *
6 * @brief Power Consumption Service API
7 *
8 *****************************************************************************************
9 * @attention
10 #####Copyright (c) 2019 GOODIX
11 All rights reserved.
12
13 Redistribution and use in source and binary forms, with or without
14 modification, are permitted provided that the following conditions are met:
15 * Redistributions of source code must retain the above copyright
16 notice, this list of conditions and the following disclaimer.
17 * Redistributions in binary form must reproduce the above copyright
18 notice, this list of conditions and the following disclaimer in the
19 documentation and/or other materials provided with the distribution.
20 * Neither the name of GOODIX nor the names of its contributors may be used
21 to endorse or promote products derived from this software without
22 specific prior written permission.
23
24 THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS"
25 AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE
26 IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE
27 ARE DISCLAIMED. IN NO EVENT SHALL COPYRIGHT HOLDERS AND CONTRIBUTORS BE
28 LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR
29 CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF
30 SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS
31 INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN
32 CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE)
33 ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE
34 POSSIBILITY OF SUCH DAMAGE.
35 *****************************************************************************************
36 */
37
38 /**
39 * @addtogroup BLE_SRV BLE Services
40 * @{
41 * @brief Definitions and prototypes for the BLE Service interface.
42 */
43
44 /**
45 * @defgroup BLE_SDK_PCS Power Consumption Service (PCS)
46 * @{
47 * @brief Definitions and prototypes for the PCS interface.
48 *
49 * @details The Power Consumption Service is a customized GATT-based service with TX and Setting
50 * characteristics. The application uses the service to notify data to peer and receive
51 * some BLE parameters such as advertising interval, connect interval, PHY and so on,
52 * which can simulate different application scenes for power consumption test.
53 *
54 * After \ref pcs_init_t variable is initialized , the application must call \ref pcs_service_init()
55 * to add the ower Consumption Service and TX, Setting characteristics to the BLE Stack database.
56 */
57
58 #ifndef __PCS_H__
59 #define __PCS_H__
60
61 #include "gr_includes.h"
62 #include "custom_config.h"
63
64 /**
65 * @defgroup PCS_MACRO Defines
66 * @{
67 */
68 #define PCS_CONNECTION_MAX 10 /**< Maximum number of Power Consumption Service connections. */
69 #define PCS_MAX_DATA_LEN 244 /**< Maximum length of application data packet which is transmitted via PCS. */
70 #define PCS_SERVICE_UUID 0x1B, 0xD7, 0x90, 0xEC, 0xE8, 0xB9, 0x75, 0x80,\
71 0x0A, 0x46, 0x44, 0xD3, 0x01, 0x05, 0xED, 0xA6 /**< The UUID of Power Consumption Service for setting advertising data. */
72
73 #define PCS_SET_PARAM_SUCCESS 0x00 /**< PCS parameters set successfully. */
74 #define PCS_SET_PARAM_FAIL 0x81 /**< PCS parameters set unsuccessfully. */
75
76 #define PCS_SET_ADV_DATA_3B 0x03 /**< Set 3 byte advertising data. */
77 #define PCS_SET_ADV_DATA_10B 0x0a /**< Set 10 byte advertising data. */
78 #define PCS_SET_ADV_DATA_17B 0x11 /**< Set 17 byte advertising data. */
79 #define PCS_SET_ADV_DATA_24B 0x18 /**< Set 24 byte advertising data. */
80 #define PCS_SET_ADV_DATA_31B 0x1f /**< Set 31 byte advertising data. */
81 /** @} */
82
83 /**
84 * @defgroup PCS_ENUM Enumerations
85 * @{
86 */
87 /**@brief PCS Service event types. */
88 typedef enum
89 {
90 PCS_EVT_INVALID, /**< Invalid PCS event. */
91 PCS_EVT_TX_ENABLE, /**< TX notify has been enabled. */
92 PCS_EVT_TX_DISABLE, /**< TX notify has been disabled. */
93 PCS_EVT_SETTING_ENABLE, /**< Setting notify has been enabled. */
94 PCS_EVT_SETTING_DISABLE, /**< Setting notify has been disabled. */
95 PCS_EVT_TX_DATA_SENT, /**< Data has been notitied completely. */
96 PCS_EVT_PARAM_SET, /**< BLE parameters set. */
97 PCS_EVT_DISCONNECTED, /**< Disconnected. */
98 } pcs_evt_type_t;
99
100 /**@brief PCS Service settings types. */
101 typedef enum
102 {
103 PCS_SETTING_TYPE_ADV_INTERVAL, /**< BLE Advertising Interval parameter. */
104 PCS_SETTING_TYPE_CONN_PARAM, /**< BLE Connection parameter. */
105 PCS_SETTING_TYPE_PHY, /**< Radio Phy mode, 1M, 2M, Encoded. */
106 PCS_SETTING_TYPE_ADV_DATA, /**< BLE advertising data. */
107 PCS_SETTING_TYPE_TX_POWER, /**< Tx Power. */
108 } pcs_setting_type_t;
109 /** @} */
110
111 /**
112 * @defgroup PCS_STRUCT Structures
113 * @{
114 */
115 /**@brief PCS Service event. */
116 typedef struct
117 {
118 uint8_t conn_idx; /**< The index of the connection. */
119 pcs_evt_type_t evt_type; /**< The PCS event type. */
120 uint8_t *p_data; /**< Pointer to data. */
121 uint16_t length; /**< Length of data. */
122 } pcs_evt_t;
123 /** @} */
124
125 /**
126 * @defgroup pPCS_TYPEDEF Typedefs
127 * @{
128 */
129 /**@brief PCS Service event handler type. */
130 typedef void (*pcs_evt_handler_t)(pcs_evt_t *p_evt);
131 /** @} */
132
133 /**
134 * @addtogroup PCS_STRUCT Structures
135 * @{
136 */
137 /**@brief PCS Service init stucture. This contains all option and data needed for initialization of the service. */
138 typedef struct
139 {
140 pcs_evt_handler_t evt_handler; /**< PCS Service event handler. */
141 } pcs_init_t;
142 /** @} */
143
144 /**
145 * @defgroup PCS_FUNCTION Functions
146 * @{
147 */
148 /**
149 *****************************************************************************************
150 * @brief Initialize a PCS Service instance and add in the database.
151 *
152 * @param[in] p_pcs_init: Pointer to PCS Service initialization variables.
153 *
154 * @return Result of service initialization.
155 *****************************************************************************************
156 */
157 sdk_err_t pcs_service_init(pcs_init_t *p_pcs_init);
158
159 /**
160 *****************************************************************************************
161 * @brief Send data to peer device.
162 *
163 * @param[in] conn_idx: Index of the connection.
164 * @param[in] p_data: Pointer to sent data.
165 * @param[in] length: Length of sent data.
166 *
167 * @return Result of sending data.
168 *****************************************************************************************
169 */
170 sdk_err_t pcs_tx_data_send(uint8_t conn_idx, uint8_t *p_data, uint16_t length);
171
172 /**
173 *****************************************************************************************
174 * @brief Reply parameters set result.
175 *
176 * @param[in] conn_idx: Index of the connection.
177 * @param[in] p_data: Pointer to sent data.
178 * @param[in] length: Length of sent data.
179 *
180 * @return Result of sending data.
181 *****************************************************************************************
182 */
183 sdk_err_t pcs_setting_reply(uint8_t conn_idx, uint8_t *p_data, uint16_t length);
184 /** @} */
185
186 #endif
187 /** @} */
188 /** @} */
PCS_SETTING_TYPE_ADV_DATA
@ PCS_SETTING_TYPE_ADV_DATA
BLE advertising data.
Definition: pcs.h:106
PCS_EVT_SETTING_DISABLE
@ PCS_EVT_SETTING_DISABLE
Setting notify has been disabled.
Definition: pcs.h:94
pcs_evt_t::conn_idx
uint8_t conn_idx
The index of the connection.
Definition: pcs.h:118
PCS_SETTING_TYPE_ADV_INTERVAL
@ PCS_SETTING_TYPE_ADV_INTERVAL
BLE Advertising Interval parameter.
Definition: pcs.h:103
PCS_EVT_INVALID
@ PCS_EVT_INVALID
Invalid PCS event.
Definition: pcs.h:90
PCS_EVT_DISCONNECTED
@ PCS_EVT_DISCONNECTED
Disconnected.
Definition: pcs.h:97
pcs_evt_t::length
uint16_t length
Length of data.
Definition: pcs.h:121
pcs_setting_type_t
pcs_setting_type_t
PCS Service settings types.
Definition: pcs.h:102
pcs_evt_t::evt_type
pcs_evt_type_t evt_type
The PCS event type.
Definition: pcs.h:119
gr_includes.h
Include Files API.
PCS_EVT_TX_DISABLE
@ PCS_EVT_TX_DISABLE
TX notify has been disabled.
Definition: pcs.h:92
PCS_EVT_TX_ENABLE
@ PCS_EVT_TX_ENABLE
TX notify has been enabled.
Definition: pcs.h:91
PCS_EVT_SETTING_ENABLE
@ PCS_EVT_SETTING_ENABLE
Setting notify has been enabled.
Definition: pcs.h:93
PCS_SETTING_TYPE_CONN_PARAM
@ PCS_SETTING_TYPE_CONN_PARAM
BLE Connection parameter.
Definition: pcs.h:104
pcs_evt_t
PCS Service event.
Definition: pcs.h:117
pcs_init_t::evt_handler
pcs_evt_handler_t evt_handler
PCS Service event handler.
Definition: pcs.h:140
PCS_EVT_TX_DATA_SENT
@ PCS_EVT_TX_DATA_SENT
Data has been notitied completely.
Definition: pcs.h:95
PCS_EVT_PARAM_SET
@ PCS_EVT_PARAM_SET
BLE parameters set.
Definition: pcs.h:96
pcs_evt_handler_t
void(* pcs_evt_handler_t)(pcs_evt_t *p_evt)
PCS Service event handler type.
Definition: pcs.h:130
pcs_init_t
PCS Service init stucture.
Definition: pcs.h:139
pcs_evt_t::p_data
uint8_t * p_data
Pointer to data.
Definition: pcs.h:120
pcs_setting_reply
sdk_err_t pcs_setting_reply(uint8_t conn_idx, uint8_t *p_data, uint16_t length)
Reply parameters set result.
sdk_err_t
uint16_t sdk_err_t
SDK API result type.
Definition: ble_error.h:274
PCS_SETTING_TYPE_TX_POWER
@ PCS_SETTING_TYPE_TX_POWER
Tx Power.
Definition: pcs.h:107
pcs_service_init
sdk_err_t pcs_service_init(pcs_init_t *p_pcs_init)
Initialize a PCS Service instance and add in the database.
PCS_SETTING_TYPE_PHY
@ PCS_SETTING_TYPE_PHY
Radio Phy mode, 1M, 2M, Encoded.
Definition: pcs.h:105
pcs_tx_data_send
sdk_err_t pcs_tx_data_send(uint8_t conn_idx, uint8_t *p_data, uint16_t length)
Send data to peer device.
pcs_evt_type_t
pcs_evt_type_t
PCS Service event types.
Definition: pcs.h:89