Public Attributes | List of all members
gus_evt_t Struct Reference
BLE Services » Goodix UART Service (GUS) » Structures

Goodix UART Service event. More...

`#include <gus.h>`

## Public Attributes
gus_evt_type_t | evt_type
| The GUS event. More...
uint8_t | conn_idx
| The index of the connection for the data transmission. More...
uint8_t * | p_data
| Pointer to the buffer within received data. More...
uint16_t | length
| Length of received data. More...

## Detailed Description

Goodix UART Service event.

Definition at line 111 of file gus.h.

## Member Data Documentation

## ◆ conn_idx

uint8_t gus_evt_t::conn_idx

The index of the connection for the data transmission.

Definition at line 114 of file gus.h.

## ◆ evt_type

gus_evt_type_t gus_evt_t::evt_type

The GUS event.

Definition at line 113 of file gus.h.

## ◆ length

uint16_t gus_evt_t::length

Length of received data.

Definition at line 116 of file gus.h.

## ◆ p_data

uint8_t* gus_evt_t::p_data

Pointer to the buffer within received data.

Definition at line 115 of file gus.h.

The documentation for this struct was generated from the following file:

- gus.h