Macros
InitStruct default configuartion
Peripheral Driver » LL Driver » ADC » Defines » ADC Private Macros
Collaboration diagram for InitStruct default configuartion:

## Macros
#define | LL_ADC_DEFAULT_CONFIG
| LL ADC InitStrcut default configuartion. More...

## Detailed Description

## Macro Definition Documentation

## ◆ LL_ADC_DEFAULT_CONFIG

#define LL_ADC_DEFAULT_CONFIG

Value:
{ \
.channel_p = LL_ADC_INPUT_SRC_IO0, \
.channel_n = LL_ADC_INPUT_SRC_IO1, \
.input_mode = LL_ADC_INPUT_DIFFERENTIAL, \
.ref_source = LL_ADC_REF_SRC_BUF_INT, \
.ref_value = LL_ADC_REF_VALUE_1P5, \
.clock = LL_ADC_CLK_16 \
}

LL ADC InitStrcut default configuartion.

Definition at line 222 of file gr55xx_ll_adc.h.

LL_ADC_INPUT_SRC_IO0
#define LL_ADC_INPUT_SRC_IO0
Select MSIO0 as input
Definition: gr55xx_ll_adc.h:154
LL_ADC_CLK_16
#define LL_ADC_CLK_16
16 MHz
Definition: gr55xx_ll_adc.h:127
LL_ADC_REF_SRC_BUF_INT
#define LL_ADC_REF_SRC_BUF_INT
Select buffered internal reference as reference
Definition: gr55xx_ll_adc.h:168
LL_ADC_INPUT_SRC_IO1
#define LL_ADC_INPUT_SRC_IO1
Select MSIO1 as input
Definition: gr55xx_ll_adc.h:155
LL_ADC_INPUT_DIFFERENTIAL
#define LL_ADC_INPUT_DIFFERENTIAL
Differential mode.
Definition: gr55xx_ll_adc.h:148