Enumerations
HAL COMP state
Peripheral Driver » HAL Driver » COMP » Enumerations
Collaboration diagram for HAL COMP state:

## Enumerations
enum | hal_comp_state_t { HAL_COMP_STATE_RESET = 0x00, HAL_COMP_STATE_READY = 0x01, HAL_COMP_STATE_BUSY = 0x02, HAL_COMP_STATE_ERROR = 0x04 }
| HAL COMP State Enumerations definition. More...

## Detailed Description

## Enumeration Type Documentation

## ◆ hal_comp_state_t

enum hal_comp_state_t

HAL COMP State Enumerations definition.

Enumerator
HAL_COMP_STATE_RESET | Peripheral not initialized
HAL_COMP_STATE_READY | Peripheral initialized and ready for use
HAL_COMP_STATE_BUSY | An internal process is ongoing
HAL_COMP_STATE_ERROR | Peripheral in error

Definition at line 75 of file gr55xx_hal_comp.h.