Public Attributes | List of all members
_aes_init Struct Reference
Peripheral Driver » HAL Driver » AES » Structures » AES Configuration

AES Init Structure definition. More...

`#include <gr55xx_hal_aes.h>`

## Public Attributes
uint32_t | key_size
| 128, 192 or 256-bits key length. More...
uint32_t | operation_mode
| AES operating mode. More...
uint32_t | chaining_mode
| AES chaining mode. More...
uint32_t * | p_key
| Encryption/Decryption Key. More...
uint32_t * | p_init_vector
| Initialization Vector used for CBC modes. More...
uint32_t | dpa_mode
| DPA Mode. More...
uint32_t * | p_seed
| Random seeds. More...

## Detailed Description

AES Init Structure definition.

Definition at line 100 of file gr55xx_hal_aes.h.

## Member Data Documentation

## ◆ chaining_mode

uint32_t _aes_init::chaining_mode

AES chaining mode.

This parameter can be a value of AES Chaining Mode

Definition at line 108 of file gr55xx_hal_aes.h.

## ◆ dpa_mode

uint32_t _aes_init::dpa_mode

DPA Mode.

Definition at line 116 of file gr55xx_hal_aes.h.

## ◆ key_size

uint32_t _aes_init::key_size

128, 192 or 256-bits key length.

This parameter can be a value of AES Key Size

Definition at line 102 of file gr55xx_hal_aes.h.

## ◆ operation_mode

uint32_t _aes_init::operation_mode

AES operating mode.

This parameter can be a value of AES Operation Mode

Definition at line 105 of file gr55xx_hal_aes.h.

## ◆ p_init_vector

uint32_t* _aes_init::p_init_vector

Initialization Vector used for CBC modes.

Definition at line 114 of file gr55xx_hal_aes.h.

## ◆ p_key

uint32_t* _aes_init::p_key

Encryption/Decryption Key.

Normally, it should be a global pointer.

Definition at line 111 of file gr55xx_hal_aes.h.

## ◆ p_seed

uint32_t* _aes_init::p_seed

Random seeds.

Definition at line 118 of file gr55xx_hal_aes.h.

The documentation for this struct was generated from the following file:

- gr55xx_hal_aes.h