Macros
InitStrcut default configuartion
Peripheral Driver » LL Driver » GPIO » Defines » GPIO Exported Constants
Collaboration diagram for InitStrcut default configuartion:

## Macros
#define | LL_GPIO_DEFAULT_CONFIG
| LL GPIO InitStrcut default configuartion. More...

## Detailed Description

## Macro Definition Documentation

## ◆ LL_GPIO_DEFAULT_CONFIG

#define LL_GPIO_DEFAULT_CONFIG

Value:
{ \
.pin = LL_GPIO_PIN_ALL, \
.mode = LL_GPIO_MODE_INPUT, \
.pull = LL_GPIO_PULL_DOWN, \
.mux = LL_GPIO_MUX_7, \
.trigger = LL_GPIO_TRIGGER_NONE, \
}

LL GPIO InitStrcut default configuartion.

Definition at line 185 of file gr55xx_ll_gpio.h.

LL_GPIO_MUX_7
#define LL_GPIO_MUX_7
Definition: gr55xx_ll_gpio.h:164
LL_GPIO_TRIGGER_NONE
#define LL_GPIO_TRIGGER_NONE
Definition: gr55xx_ll_gpio.h:171
LL_GPIO_PULL_DOWN
#define LL_GPIO_PULL_DOWN
Definition: gr55xx_ll_gpio.h:151
LL_GPIO_MODE_INPUT
#define LL_GPIO_MODE_INPUT
Definition: gr55xx_ll_gpio.h:141
LL_GPIO_PIN_ALL
#define LL_GPIO_PIN_ALL
Definition: gr55xx_ll_gpio.h:135