### - r -

- reference_time_encode() : cts.h
- restore_sys_context() : gr55xx_sys.h
- rng_calibration() : gr55xx_sys.h
- rscs_c_ctrl_pt_indicate_set() : rscs_c.h
- rscs_c_ctrl_pt_set() : rscs_c.h
- rscs_c_disc_srvc_start() : rscs_c.h
- rscs_c_rsc_feature_read() : rscs_c.h
- rscs_c_rsc_meas_notify_set() : rscs_c.h
- rscs_c_sensor_loc_read() : rscs_c.h
- rscs_client_init() : rscs_c.h
- rscs_ctrl_pt_rsp_send() : rscs.h
- rscs_measurement_send() : rscs.h
- rscs_sensor_loc_update() : rscs.h
- rscs_service_init() : rscs.h
- rtc_calibration() : gr55xx_sys.h
- rtus_current_state_set() : rtus.h
- rtus_service_init() : rtus.h
- rtus_update_result_set() : rtus.h