Functions
Functions
Peripheral Driver » APP DRIVER » AON WDT
Collaboration diagram for Functions:

## Functions
uint16_t | app_aon_wdt_init (app_aon_wdt_params_t *p_params, app_aon_wdt_evt_handler_t evt_handler)
| Initialize the APP AON WDT DRIVER. More...
uint16_t | app_aon_wdt_deinit (void)
| De-initialize the APP AON WDT DRIVER. More...
uint16_t | app_aon_wdt_refresh (void)
| Refresh the AON WDT. More...

## Detailed Description

## Function Documentation

## ◆ app_aon_wdt_deinit()

uint16_t app_aon_wdt_deinit | ( | void |  | ) |

De-initialize the APP AON WDT DRIVER.

Returns
  Result of De-initialization.

## ◆ app_aon_wdt_init()

uint16_t app_aon_wdt_init | ( | app_aon_wdt_params_t * | p_params,
|  | app_aon_wdt_evt_handler_t | evt_handler
| ) |  |

Initialize the APP AON WDT DRIVER.

Parameters

  [in] | p_params | Pointer to app_aon_wdt_params_t parameter which contains the configuration information for the specified AON WDT module.
  [in] | evt_handler | AON WDT user callback function.

Returns
  Result of initialization.

## ◆ app_aon_wdt_refresh()

uint16_t app_aon_wdt_refresh | ( | void |  | ) |

Refresh the AON WDT.

Returns
  Result of operation.