Modules | Macros
Defines
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Connection Control
Collaboration diagram for Defines:

## Modules
| GAP Address types
| GAP PHY OPTIONS (bitmask)

## Macros
#define | BLE_GAP_CHNL_MAP_LEN 0x05
| The length of channel map. More...
#define | BLE_GAP_FEATS_LEN 0x08
| The length of features. More...
#define | BLE_GAP_ADDR_LEN 0x06
| The length of address. More...
#define | BLE_GAP_INVALID_CONN_INDEX 0xFF
| Invalid connection index. More...

## Detailed Description

## Macro Definition Documentation

## ◆ BLE_GAP_ADDR_LEN

#define BLE_GAP_ADDR_LEN 0x06

The length of address.

Definition at line 70 of file ble_gapc.h.

## ◆ BLE_GAP_CHNL_MAP_LEN

#define BLE_GAP_CHNL_MAP_LEN 0x05

The length of channel map.

Definition at line 68 of file ble_gapc.h.

## ◆ BLE_GAP_FEATS_LEN

#define BLE_GAP_FEATS_LEN 0x08

The length of features.

Definition at line 69 of file ble_gapc.h.

## ◆ BLE_GAP_INVALID_CONN_INDEX

#define BLE_GAP_INVALID_CONN_INDEX 0xFF

Invalid connection index.

Definition at line 71 of file ble_gapc.h.