Macros
InitStrcut default configuartion
Peripheral Driver » LL Driver » UART » Defines » UART Exported Constants
Collaboration diagram for InitStrcut default configuartion:

## Macros
#define | LL_UART_DEFAULT_CONFIG
| LL UART InitStrcut default configuartion. More...

## Detailed Description

## Macro Definition Documentation

## ◆ LL_UART_DEFAULT_CONFIG

#define LL_UART_DEFAULT_CONFIG

Value:
{ \
.baud_rate = 9600U, \
.data_bits = LL_UART_DATABITS_8B, \
.stop_bits = LL_UART_STOPBITS_1, \
.parity = LL_UART_PARITY_NONE, \
.hw_flow_ctrl = LL_UART_HWCONTROL_NONE, \
}

LL UART InitStrcut default configuartion.

Definition at line 225 of file gr55xx_ll_uart.h.

LL_UART_PARITY_NONE
#define LL_UART_PARITY_NONE
Parity control disabled.
Definition: gr55xx_ll_uart.h:155
LL_UART_HWCONTROL_NONE
#define LL_UART_HWCONTROL_NONE
CTS and RTS hardware flow control disabled.
Definition: gr55xx_ll_uart.h:182
LL_UART_DATABITS_8B
#define LL_UART_DATABITS_8B
8 bits word length : Start bit, 8 data bits, n stop bits
Definition: gr55xx_ll_uart.h:168
LL_UART_STOPBITS_1
#define LL_UART_STOPBITS_1
1 stop bit
Definition: gr55xx_ll_uart.h:174