### - c -

- CALENDAR_ALARM_DISABLE_ALL : gr55xx_hal_calendar.h
- CALENDAR_ALARM_DISABLE_DATE : gr55xx_hal_calendar.h
- CALENDAR_ALARM_DISABLE_TICK : gr55xx_hal_calendar.h
- CALENDAR_ALARM_SEL_DATE : gr55xx_hal_calendar.h
- CALENDAR_ALARM_SEL_WEEKDAY : gr55xx_hal_calendar.h
- CALENDAR_ALARM_WEEKDAY_FRI : gr55xx_hal_calendar.h
- CALENDAR_ALARM_WEEKDAY_MON : gr55xx_hal_calendar.h
- CALENDAR_ALARM_WEEKDAY_SAT : gr55xx_hal_calendar.h
- CALENDAR_ALARM_WEEKDAY_SUN : gr55xx_hal_calendar.h
- CALENDAR_ALARM_WEEKDAY_THU : gr55xx_hal_calendar.h
- CALENDAR_ALARM_WEEKDAY_TUE : gr55xx_hal_calendar.h
- CALENDAR_ALARM_WEEKDAY_WED : gr55xx_hal_calendar.h
- CALENDAR_FLAG_ALARM : gr55xx_hal_calendar.h
- CALENDAR_FLAG_WARP : gr55xx_hal_calendar.h
- CALENDAR_IT_ALARM : gr55xx_hal_calendar.h
- CALENDAR_IT_WARP : gr55xx_hal_calendar.h
- CFG_ANCS_ATTRIBUTE_MAXLEN : ancs_protocol.h
- CGC_DEFAULT_CONFIG : gr55xx_hal_cgc.h
- CGC_FRC_ALL_CLK : gr55xx_hal_cgc.h
- CGC_FRC_AON_MCUSUB_HCLK : gr55xx_hal_cgc.h
- CGC_FRC_APB_SUB_HCLK : gr55xx_hal_cgc.h
- CGC_FRC_BLE_BRG_HCLK : gr55xx_hal_cgc.h
- CGC_FRC_DMA_HCLK : gr55xx_hal_cgc.h
- CGC_FRC_GPIO_HCLK : gr55xx_hal_cgc.h
- CGC_FRC_HTB_HCLK : gr55xx_hal_cgc.h
- CGC_FRC_I2C0_HCLK : gr55xx_hal_cgc.h
- CGC_FRC_I2C1_HCLK : gr55xx_hal_cgc.h
- CGC_FRC_I2S_HCLK : gr55xx_hal_cgc.h
- CGC_FRC_I2S_S_HCLK : gr55xx_hal_cgc.h
- CGC_FRC_PWM_HCLK : gr55xx_hal_cgc.h
- CGC_FRC_QSPI0_HCLK : gr55xx_hal_cgc.h
- CGC_FRC_QSPI1_HCLK : gr55xx_hal_cgc.h
- CGC_FRC_ROM_HCLK : gr55xx_hal_cgc.h
- CGC_FRC_SECU_DIV4_PCLK : gr55xx_hal_cgc.h
- CGC_FRC_SECU_HCLK : gr55xx_hal_cgc.h
- CGC_FRC_SERIAL_HCLK : gr55xx_hal_cgc.h
- CGC_FRC_SIM_HCLK : gr55xx_hal_cgc.h
- CGC_FRC_SNSADC_HCLK : gr55xx_hal_cgc.h
- CGC_FRC_SPIM_HCLK : gr55xx_hal_cgc.h
- CGC_FRC_SPIS_HCLK : gr55xx_hal_cgc.h
- CGC_FRC_SRAM_HCLK : gr55xx_hal_cgc.h
- CGC_FRC_UART0_HCLK : gr55xx_hal_cgc.h
- CGC_FRC_UART1_HCLK : gr55xx_hal_cgc.h
- CGC_FRC_XF_XQSPI_HCLK : gr55xx_hal_cgc.h
- CGC_FRC_XQSPI_DIV4_PCLK : gr55xx_hal_cgc.h
- CGC_WFI_ALL_CLK : gr55xx_hal_cgc.h
- CGC_WFI_AON_MCUSUB_HCLK : gr55xx_hal_cgc.h
- CGC_WFI_APB_SUB_HCLK : gr55xx_hal_cgc.h
- CGC_WFI_BLE_BRG_HCLK : gr55xx_hal_cgc.h
- CGC_WFI_DMA_HCLK : gr55xx_hal_cgc.h
- CGC_WFI_GPIO_HCLK : gr55xx_hal_cgc.h
- CGC_WFI_HTB_HCLK : gr55xx_hal_cgc.h
- CGC_WFI_I2S_S_HCLK : gr55xx_hal_cgc.h
- CGC_WFI_PWM_HCLK : gr55xx_hal_cgc.h
- CGC_WFI_ROM_HCLK : gr55xx_hal_cgc.h
- CGC_WFI_SECU_DIV4_PCLK : gr55xx_hal_cgc.h
- CGC_WFI_SECU_HCLK : gr55xx_hal_cgc.h
- CGC_WFI_SERIAL_HCLK : gr55xx_hal_cgc.h
- CGC_WFI_SIM_HCLK : gr55xx_hal_cgc.h
- CGC_WFI_SNSADC_HCLK : gr55xx_hal_cgc.h
- CGC_WFI_SRAM_HCLK : gr55xx_hal_cgc.h
- CGC_WFI_XF_XQSPI_HCLK : gr55xx_hal_cgc.h
- CGC_WFI_XQSPI_DIV4_PCLK : gr55xx_hal_cgc.h
- CHECK_IS_ON_FPGA : gr55xx_hal.h
- CO_BIT : ble_gapm.h
- CO_MAX : gr55xx_hal.h
- COMP_DEFAULT_CONFIG : gr55xx_hal_comp.h
- COMP_INPUT_SRC_IO0 : gr55xx_hal_comp.h
- COMP_INPUT_SRC_IO1 : gr55xx_hal_comp.h
- COMP_INPUT_SRC_IO2 : gr55xx_hal_comp.h
- COMP_INPUT_SRC_IO3 : gr55xx_hal_comp.h
- COMP_INPUT_SRC_IO4 : gr55xx_hal_comp.h
- COMP_REF_SRC_IO0 : gr55xx_hal_comp.h
- COMP_REF_SRC_IO1 : gr55xx_hal_comp.h
- COMP_REF_SRC_IO2 : gr55xx_hal_comp.h
- COMP_REF_SRC_IO3 : gr55xx_hal_comp.h
- COMP_REF_SRC_IO4 : gr55xx_hal_comp.h
- COMP_REF_SRC_VBAT : gr55xx_hal_comp.h
- COMP_REF_SRC_VREF : gr55xx_hal_comp.h
- CSCS_CHAR_FULL : cscs.h
- CSCS_CHAR_MANDATORY : cscs.h
- CSCS_CHAR_SC_CTRL_POINT : cscs.h
- CSCS_CHAR_SENSOR_LOC_SUP : cscs.h
- CSCS_CONNECTION_MAX : cscs.h
- CSCS_CTRL_PT_RSP_LEN_MIN : cscs.h
- CSCS_CTRL_PT_VAL_LEN_MAX : cscs.h
- CSCS_ERROR_CCCD_INVALID : cscs.h
- CSCS_ERROR_PROC_IN_PROGRESS : cscs.h
- CSCS_FEAR_FULL_BIT : cscs.h
- CSCS_FEAT_CRANK_REVOLUTION_SUP_BIT : cscs.h
- CSCS_FEAT_MULTIPLE_SENSORS_BIT : cscs.h
- CSCS_FEAT_VAL_LEN_MAX : cscs.h
- CSCS_FEAT_WHEEL_REVOLUTION_SUP_BIT : cscs.h
- CSCS_MEAS_FLAG_CRANK_REVOLUTION_BIT : cscs.h
- CSCS_MEAS_FLAG_WHEEL_REVOLUTION_BIT : cscs.h
- CSCS_MEAS_VAL_LEN_MAX : cscs.h
- CSCS_SENSOR_LOC_VAL_LEN_MAX : cscs.h
- CTS_AR_DST_CHANGE : cts.h
- CTS_AR_EXT_REF_TIME_UPDATE : cts.h
- CTS_AR_MAUAL_TIME_UPDATE : cts.h
- CTS_AR_NO_CHANGE : cts.h
- CTS_AR_TIME_ZONE_CHANGE : cts.h
- CTS_C_AR_DST_CHANGE : cts_c.h
- CTS_C_AR_EXT_REF_TIME_UPDATE : cts_c.h
- CTS_C_AR_MAUAL_TIME_UPDATE : cts_c.h
- CTS_C_AR_NO_CHANGE : cts_c.h
- CTS_C_AR_TIME_ZONE_CHANGE : cts_c.h
- CTS_C_CONNECTION_MAX : cts_c.h
- CTS_C_CUR_TIME_VAL_LEN : cts_c.h
- CTS_C_ERROR_FIELDS_IGNORED : cts_c.h
- CTS_C_LOC_TIME_INFO_VAL_LEN : cts_c.h
- CTS_C_TIME_ACCURACT_UNKNOWN : cts_c.h
- CTS_C_TIME_ACCURACY_OUT_RANGE : cts_c.h
- CTS_C_TIME_Y_M_D_UNKNOWN : cts_c.h
- CTS_C_TIME_YEAR_VALID_VAL_MAX : cts_c.h
- CTS_C_TIME_YEAR_VALID_VAL_MIN : cts_c.h
- CTS_C_TIME_ZONE_OFFSET_MAX : cts_c.h
- CTS_C_TIME_ZONE_OFFSET_MIN : cts_c.h
- CTS_CHAR_FULL : cts.h
- CTS_CHAR_LOC_TIME_INFO_SUP : cts.h
- CTS_CHAR_MANDATORY : cts.h
- CTS_CHAR_REF_TIME_INFO_SUP : cts.h
- CTS_CONNECTION_MAX : cts.h
- CTS_CUR_TIME_VAL_LEN : cts.h
- CTS_ERROR_FIELDS_IGNORED : cts.h
- CTS_LOC_TIME_INFO_VAL_LEN : cts.h
- CTS_REF_TIME_INFO_VAL_LEN : cts.h
- CTS_TIME_ACCURACT_UNKNOWN : cts.h
- CTS_TIME_ACCURACY_OUT_RANGE : cts.h
- CTS_TIME_YEAR_VALID_VAL_MAX : cts.h
- CTS_TIME_YEAR_VALID_VAL_MIN : cts.h
- CTS_TIME_ZONE_OFFSET_MAX : cts.h
- CTS_TIME_ZONE_OFFSET_MIN : cts.h