Public Attributes | List of all members
ble_gap_ext_init_param_t Struct Reference
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Management » Structures

Extended initiating parameters. More...

`#include <ble_gapm.h>`

Collaboration diagram for ble_gap_ext_init_param_t:
[legend]

## Public Attributes
ble_gap_init_type_t | type
| Initiating type (see enum ble_gap_init_type_t). More...
uint8_t | prop
| Properties for the initiating procedure (see enum ble_gap_init_prop_t for bit signification). More...
uint16_t | conn_to
| Timeout for automatic connection establishment (in unit of 10ms). More...
ble_gap_scan_wd_op_param_t | scan_param_1m
| Scan window opening parameters for LE 1M PHY. More...
ble_gap_scan_wd_op_param_t | scan_param_coded
| Scan window opening parameters for LE Coded PHY. More...
ble_gap_ext_conn_param_t | conn_param_1m
| Connection parameters for LE 1M PHY. More...
ble_gap_ext_conn_param_t | conn_param_2m
| Connection parameters for LE 2M PHY. More...
ble_gap_ext_conn_param_t | conn_param_coded
| Connection parameters for LE Coded PHY. More...
ble_gap_bdaddr_t | peer_addr
| Address of peer device in case white list is not used for connection. More...

## Detailed Description

Extended initiating parameters.

Definition at line 702 of file ble_gapm.h.

## Member Data Documentation

## ◆ conn_param_1m

ble_gap_ext_conn_param_t ble_gap_ext_init_param_t::conn_param_1m

Connection parameters for LE 1M PHY.

Definition at line 709 of file ble_gapm.h.

## ◆ conn_param_2m

ble_gap_ext_conn_param_t ble_gap_ext_init_param_t::conn_param_2m

Connection parameters for LE 2M PHY.

Definition at line 710 of file ble_gapm.h.

## ◆ conn_param_coded

ble_gap_ext_conn_param_t ble_gap_ext_init_param_t::conn_param_coded

Connection parameters for LE Coded PHY.

Definition at line 711 of file ble_gapm.h.

## ◆ conn_to

uint16_t ble_gap_ext_init_param_t::conn_to

Timeout for automatic connection establishment (in unit of 10ms).

Cancel the procedure if connection has not been connected when the timeout occurs.0 means there is no timeout.

Definition at line 706 of file ble_gapm.h.

## ◆ peer_addr

ble_gap_bdaddr_t ble_gap_ext_init_param_t::peer_addr

Address of peer device in case white list is not used for connection.

Definition at line 712 of file ble_gapm.h.

## ◆ prop

uint8_t ble_gap_ext_init_param_t::prop

Properties for the initiating procedure (see enum ble_gap_init_prop_t for bit signification).

Definition at line 705 of file ble_gapm.h.

## ◆ scan_param_1m

ble_gap_scan_wd_op_param_t ble_gap_ext_init_param_t::scan_param_1m

Scan window opening parameters for LE 1M PHY.

Definition at line 707 of file ble_gapm.h.

## ◆ scan_param_coded

ble_gap_scan_wd_op_param_t ble_gap_ext_init_param_t::scan_param_coded

Scan window opening parameters for LE Coded PHY.

Definition at line 708 of file ble_gapm.h.

## ◆ type

ble_gap_init_type_t ble_gap_ext_init_param_t::type

Initiating type (see enum ble_gap_init_type_t).

Definition at line 704 of file ble_gapm.h.

The documentation for this struct was generated from the following file:

- ble_gapm.h