Macros
Post-process mode
Peripheral Driver » LL Driver » RNG » Defines » RNG Exported Constants
Collaboration diagram for Post-process mode:

## Macros
#define | LL_RNG_POST_PRO_NOT (0x00000000UL)
| No post process. More...
#define | LL_RNG_POST_PRO_SKIPPING (1UL << RNG_CONFIG_POST_MODE_Pos)
| bit skipping. More...
#define | LL_RNG_POST_PRO_COUNTING (2UL << RNG_CONFIG_POST_MODE_Pos)
| bit counting. More...
#define | LL_RNG_POST_PRO_NEUMANN (3UL << RNG_CONFIG_POST_MODE_Pos)
| Von-Neumann. More...

## Detailed Description

## Macro Definition Documentation

## ◆ LL_RNG_POST_PRO_COUNTING

#define LL_RNG_POST_PRO_COUNTING (2UL << RNG_CONFIG_POST_MODE_Pos)

bit counting.

Definition at line 127 of file gr55xx_ll_rng.h.

## ◆ LL_RNG_POST_PRO_NEUMANN

#define LL_RNG_POST_PRO_NEUMANN (3UL << RNG_CONFIG_POST_MODE_Pos)

Von-Neumann.

Definition at line 128 of file gr55xx_ll_rng.h.

## ◆ LL_RNG_POST_PRO_NOT

#define LL_RNG_POST_PRO_NOT (0x00000000UL)

No post process.

Definition at line 125 of file gr55xx_ll_rng.h.

## ◆ LL_RNG_POST_PRO_SKIPPING

#define LL_RNG_POST_PRO_SKIPPING (1UL << RNG_CONFIG_POST_MODE_Pos)

bit skipping.

Definition at line 126 of file gr55xx_ll_rng.h.