Macros
IT Defines
Peripheral Driver » LL Driver » SPI » Defines » SPI Exported Constants

Interrupt definitions which can be used with LL_SPI_ReadReg and LL_SPI_WriteReg functions. More...

Collaboration diagram for IT Defines:

## Macros
#define | LL_SSI_IM_MST SSI_INTMASK_MSTIM
| Multi-Master Contention Interrupt enable More...
#define | LL_SSI_IM_RXF SSI_INTMASK_RXFIM
| Receive FIFO Full Interrupt enable More...
#define | LL_SSI_IM_RXO SSI_INTMASK_RXOIM
| Receive FIFO Overflow Interrupt enable More...
#define | LL_SSI_IM_RXU SSI_INTMASK_RXUIM
| Receive FIFO Underflow Interrupt enable More...
#define | LL_SSI_IM_TXO SSI_INTMASK_TXOIM
| Transmit FIFO Overflow Interrupt enable More...
#define | LL_SSI_IM_TXE SSI_INTMASK_TXEIM
| Transmit FIFO Empty Interrupt enable More...
#define | LL_SSI_IS_MST SSI_INTSTAT_MSTIS
| Multi-Master Contention Interrupt flag More...
#define | LL_SSI_IS_RXF SSI_INTSTAT_RXFIS
| Receive FIFO Full Interrupt flag More...
#define | LL_SSI_IS_RXO SSI_INTSTAT_RXOIS
| Receive FIFO Overflow Interrupt flag More...
#define | LL_SSI_IS_RXU SSI_INTSTAT_RXUIS
| Receive FIFO Underflow Interrupt flag More...
#define | LL_SSI_IS_TXO SSI_INTSTAT_TXOIS
| Transmit FIFO Overflow Interrupt flag More...
#define | LL_SSI_IS_TXE SSI_INTSTAT_TXEIS
| Transmit FIFO Empty Interrupt flag More...
#define | LL_SSI_RIS_MST SSI_RAW_INTSTAT_MSTIR
| Multi-Master Contention RAW Interrupt flag. More...
#define | LL_SSI_RIS_RXF SSI_RAW_INTSTAT_RXFIR
| Receive FIFO Full RAW Interrupt flag More...
#define | LL_SSI_RIS_RXO SSI_RAW_INTSTAT_RXOIR
| Receive FIFO Overflow RAW Interrupt flag More...
#define | LL_SSI_RIS_RXU SSI_RAW_INTSTAT_RXUIR
| Receive FIFO Underflow RAW Interrupt flag. More...
#define | LL_SSI_RIS_TXO SSI_RAW_INTSTAT_TXOIR
| Transmit FIFO Overflow RAW Interrupt flag. More...
#define | LL_SSI_RIS_TXE SSI_RAW_INTSTAT_TXEIR
| Transmit FIFO Empty RAW Interrupt flag More...

## Detailed Description

Interrupt definitions which can be used with LL_SPI_ReadReg and LL_SPI_WriteReg functions.

## Macro Definition Documentation

## ◆ LL_SSI_IM_MST

#define LL_SSI_IM_MST SSI_INTMASK_MSTIM

Multi-Master Contention Interrupt enable

Definition at line 218 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_IM_RXF

#define LL_SSI_IM_RXF SSI_INTMASK_RXFIM

Receive FIFO Full Interrupt enable

Definition at line 219 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_IM_RXO

#define LL_SSI_IM_RXO SSI_INTMASK_RXOIM

Receive FIFO Overflow Interrupt enable

Definition at line 220 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_IM_RXU

#define LL_SSI_IM_RXU SSI_INTMASK_RXUIM

Receive FIFO Underflow Interrupt enable

Definition at line 221 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_IM_TXE

#define LL_SSI_IM_TXE SSI_INTMASK_TXEIM

Transmit FIFO Empty Interrupt enable

Definition at line 223 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_IM_TXO

#define LL_SSI_IM_TXO SSI_INTMASK_TXOIM

Transmit FIFO Overflow Interrupt enable

Definition at line 222 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_IS_MST

#define LL_SSI_IS_MST SSI_INTSTAT_MSTIS

Multi-Master Contention Interrupt flag

Definition at line 225 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_IS_RXF

#define LL_SSI_IS_RXF SSI_INTSTAT_RXFIS

Receive FIFO Full Interrupt flag

Definition at line 226 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_IS_RXO

#define LL_SSI_IS_RXO SSI_INTSTAT_RXOIS

Receive FIFO Overflow Interrupt flag

Definition at line 227 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_IS_RXU

#define LL_SSI_IS_RXU SSI_INTSTAT_RXUIS

Receive FIFO Underflow Interrupt flag

Definition at line 228 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_IS_TXE

#define LL_SSI_IS_TXE SSI_INTSTAT_TXEIS

Transmit FIFO Empty Interrupt flag

Definition at line 230 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_IS_TXO

#define LL_SSI_IS_TXO SSI_INTSTAT_TXOIS

Transmit FIFO Overflow Interrupt flag

Definition at line 229 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_RIS_MST

#define LL_SSI_RIS_MST SSI_RAW_INTSTAT_MSTIR

Multi-Master Contention RAW Interrupt flag.

Definition at line 232 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_RIS_RXF

#define LL_SSI_RIS_RXF SSI_RAW_INTSTAT_RXFIR

Receive FIFO Full RAW Interrupt flag

Definition at line 233 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_RIS_RXO

#define LL_SSI_RIS_RXO SSI_RAW_INTSTAT_RXOIR

Receive FIFO Overflow RAW Interrupt flag

Definition at line 234 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_RIS_RXU

#define LL_SSI_RIS_RXU SSI_RAW_INTSTAT_RXUIR

Receive FIFO Underflow RAW Interrupt flag.

Definition at line 235 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_RIS_TXE

#define LL_SSI_RIS_TXE SSI_RAW_INTSTAT_TXEIR

Transmit FIFO Empty RAW Interrupt flag

Definition at line 237 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_RIS_TXO

#define LL_SSI_RIS_TXO SSI_RAW_INTSTAT_TXOIR

Transmit FIFO Overflow RAW Interrupt flag.

Definition at line 236 of file gr55xx_ll_spi.h.