Public Attributes | List of all members
hrs_init_t Struct Reference
BLE Services » Heart Rate Service (HRS) » Structures

Heart Rate Service Init variable. More...

`#include <hrs.h>`

Collaboration diagram for hrs_init_t:
[legend]

## Public Attributes
hrs_evt_handler_t | evt_handler
| Heart Rate Service event handler. More...
bool | is_sensor_contact_supported
| Determine if sensor contact detection is to be supported. More...
uint8_t | char_mask
| Mask of Supported characteristics, and configured with Characteristics Mask. More...
hrs_sensor_loc_t | sensor_loc
| The value of Body Sensor Location characteristic is static while in a connection. More...

## Detailed Description

Heart Rate Service Init variable.

Definition at line 148 of file hrs.h.

## Member Data Documentation

## ◆ char_mask

uint8_t hrs_init_t::char_mask

Mask of Supported characteristics, and configured with Characteristics Mask.

Definition at line 152 of file hrs.h.

## ◆ evt_handler

hrs_evt_handler_t hrs_init_t::evt_handler

Heart Rate Service event handler.

Definition at line 150 of file hrs.h.

## ◆ is_sensor_contact_supported

bool hrs_init_t::is_sensor_contact_supported

Determine if sensor contact detection is to be supported.

Definition at line 151 of file hrs.h.

## ◆ sensor_loc

hrs_sensor_loc_t hrs_init_t::sensor_loc

The value of Body Sensor Location characteristic is static while in a connection.

Definition at line 153 of file hrs.h.

The documentation for this struct was generated from the following file:

- hrs.h