Macros
InitStrcut default configuartion
Peripheral Driver » LL Driver » DUAL_TIMER » Defines » DUAL_TIM Exported Constants
Collaboration diagram for InitStrcut default configuartion:

## Macros
#define | DUAL_TIMER_DEFAULT_CONFIG
| LL DUAL_TIMER InitStrcut default configuartion. More...

## Detailed Description

## Macro Definition Documentation

## ◆ DUAL_TIMER_DEFAULT_CONFIG

#define DUAL_TIMER_DEFAULT_CONFIG

Value:
{ \
.prescaler = LL_DUAL_TIMER_PRESCALER_DIV0, \
.counter_size = LL_DUAL_TIMER_COUNTERSIZE_32, \
.counter_mode = LL_DUAL_TIMER_PERIODIC_MODE, \
.auto_reload = SystemCoreClock - 1, \
}

LL DUAL_TIMER InitStrcut default configuartion.

Definition at line 144 of file gr55xx_ll_dual_tim.h.

LL_DUAL_TIMER_PRESCALER_DIV0
#define LL_DUAL_TIMER_PRESCALER_DIV0
0 stage of prescale, clock is divided by 1.
Definition: gr55xx_ll_dual_tim.h:125
LL_DUAL_TIMER_PERIODIC_MODE
#define LL_DUAL_TIMER_PERIODIC_MODE
Periodic mode.
Definition: gr55xx_ll_dual_tim.h:119
LL_DUAL_TIMER_COUNTERSIZE_32
#define LL_DUAL_TIMER_COUNTERSIZE_32
Counter size 32 bits.
Definition: gr55xx_ll_dual_tim.h:134