Macros
Data Width
Peripheral Driver » HAL Driver » QSPI » Defines » QSPI Exported Constants
Collaboration diagram for Data Width:

## Macros
#define | QSPI_DATASIZE_04_BITS LL_SSI_DATASIZE_4BIT
| Data length for SPI transfer: 4 bits. More...
#define | QSPI_DATASIZE_05_BITS LL_SSI_DATASIZE_5BIT
| Data length for SPI transfer: 5 bits. More...
#define | QSPI_DATASIZE_06_BITS LL_SSI_DATASIZE_6BIT
| Data length for SPI transfer: 6 bits. More...
#define | QSPI_DATASIZE_07_BITS LL_SSI_DATASIZE_7BIT
| Data length for SPI transfer: 7 bits. More...
#define | QSPI_DATASIZE_08_BITS LL_SSI_DATASIZE_8BIT
| Data length for SPI transfer: 8 bits. More...
#define | QSPI_DATASIZE_09_BITS LL_SSI_DATASIZE_9BIT
| Data length for SPI transfer: 9 bits. More...
#define | QSPI_DATASIZE_10_BITS LL_SSI_DATASIZE_10BIT
| Data length for SPI transfer: 10 bits. More...
#define | QSPI_DATASIZE_11_BITS LL_SSI_DATASIZE_11BIT
| Data length for SPI transfer: 11 bits. More...
#define | QSPI_DATASIZE_12_BITS LL_SSI_DATASIZE_12BIT
| Data length for SPI transfer: 12 bits. More...
#define | QSPI_DATASIZE_13_BITS LL_SSI_DATASIZE_13BIT
| Data length for SPI transfer: 13 bits. More...
#define | QSPI_DATASIZE_14_BITS LL_SSI_DATASIZE_14BIT
| Data length for SPI transfer: 14 bits. More...
#define | QSPI_DATASIZE_15_BITS LL_SSI_DATASIZE_15BIT
| Data length for SPI transfer: 15 bits. More...
#define | QSPI_DATASIZE_16_BITS LL_SSI_DATASIZE_16BIT
| Data length for SPI transfer: 16 bits. More...
#define | QSPI_DATASIZE_17_BITS LL_SSI_DATASIZE_17BIT
| Data length for SPI transfer: 17 bits. More...
#define | QSPI_DATASIZE_18_BITS LL_SSI_DATASIZE_18BIT
| Data length for SPI transfer: 18 bits. More...
#define | QSPI_DATASIZE_19_BITS LL_SSI_DATASIZE_19BIT
| Data length for SPI transfer: 19 bits. More...
#define | QSPI_DATASIZE_20_BITS LL_SSI_DATASIZE_20BIT
| Data length for SPI transfer: 20 bits. More...
#define | QSPI_DATASIZE_21_BITS LL_SSI_DATASIZE_21BIT
| Data length for SPI transfer: 21 bits. More...
#define | QSPI_DATASIZE_22_BITS LL_SSI_DATASIZE_22BIT
| Data length for SPI transfer: 22 bits. More...
#define | QSPI_DATASIZE_23_BITS LL_SSI_DATASIZE_23BIT
| Data length for SPI transfer: 23 bits. More...
#define | QSPI_DATASIZE_24_BITS LL_SSI_DATASIZE_24BIT
| Data length for SPI transfer: 24 bits. More...
#define | QSPI_DATASIZE_25_BITS LL_SSI_DATASIZE_25BIT
| Data length for SPI transfer: 25 bits. More...
#define | QSPI_DATASIZE_26_BITS LL_SSI_DATASIZE_26BIT
| Data length for SPI transfer: 26 bits. More...
#define | QSPI_DATASIZE_27_BITS LL_SSI_DATASIZE_27BIT
| Data length for SPI transfer: 27 bits. More...
#define | QSPI_DATASIZE_28_BITS LL_SSI_DATASIZE_28BIT
| Data length for SPI transfer: 28 bits. More...
#define | QSPI_DATASIZE_29_BITS LL_SSI_DATASIZE_29BIT
| Data length for SPI transfer: 29 bits. More...
#define | QSPI_DATASIZE_30_BITS LL_SSI_DATASIZE_30BIT
| Data length for SPI transfer: 30 bits. More...
#define | QSPI_DATASIZE_31_BITS LL_SSI_DATASIZE_31BIT
| Data length for SPI transfer: 31 bits. More...
#define | QSPI_DATASIZE_32_BITS LL_SSI_DATASIZE_32BIT
| Data length for SPI transfer: 32 bits. More...

## Detailed Description

## Macro Definition Documentation

## ◆ QSPI_DATASIZE_04_BITS

#define QSPI_DATASIZE_04_BITS LL_SSI_DATASIZE_4BIT

Data length for SPI transfer: 4 bits.

Definition at line 294 of file gr55xx_hal_qspi.h.

## ◆ QSPI_DATASIZE_05_BITS

#define QSPI_DATASIZE_05_BITS LL_SSI_DATASIZE_5BIT

Data length for SPI transfer: 5 bits.

Definition at line 295 of file gr55xx_hal_qspi.h.

## ◆ QSPI_DATASIZE_06_BITS

#define QSPI_DATASIZE_06_BITS LL_SSI_DATASIZE_6BIT

Data length for SPI transfer: 6 bits.

Definition at line 296 of file gr55xx_hal_qspi.h.

## ◆ QSPI_DATASIZE_07_BITS

#define QSPI_DATASIZE_07_BITS LL_SSI_DATASIZE_7BIT

Data length for SPI transfer: 7 bits.

Definition at line 297 of file gr55xx_hal_qspi.h.

## ◆ QSPI_DATASIZE_08_BITS

#define QSPI_DATASIZE_08_BITS LL_SSI_DATASIZE_8BIT

Data length for SPI transfer: 8 bits.

Definition at line 298 of file gr55xx_hal_qspi.h.

## ◆ QSPI_DATASIZE_09_BITS

#define QSPI_DATASIZE_09_BITS LL_SSI_DATASIZE_9BIT

Data length for SPI transfer: 9 bits.

Definition at line 299 of file gr55xx_hal_qspi.h.

## ◆ QSPI_DATASIZE_10_BITS

#define QSPI_DATASIZE_10_BITS LL_SSI_DATASIZE_10BIT

Data length for SPI transfer: 10 bits.

Definition at line 300 of file gr55xx_hal_qspi.h.

## ◆ QSPI_DATASIZE_11_BITS

#define QSPI_DATASIZE_11_BITS LL_SSI_DATASIZE_11BIT

Data length for SPI transfer: 11 bits.

Definition at line 301 of file gr55xx_hal_qspi.h.

## ◆ QSPI_DATASIZE_12_BITS

#define QSPI_DATASIZE_12_BITS LL_SSI_DATASIZE_12BIT

Data length for SPI transfer: 12 bits.

Definition at line 302 of file gr55xx_hal_qspi.h.

## ◆ QSPI_DATASIZE_13_BITS

#define QSPI_DATASIZE_13_BITS LL_SSI_DATASIZE_13BIT

Data length for SPI transfer: 13 bits.

Definition at line 303 of file gr55xx_hal_qspi.h.

## ◆ QSPI_DATASIZE_14_BITS

#define QSPI_DATASIZE_14_BITS LL_SSI_DATASIZE_14BIT

Data length for SPI transfer: 14 bits.

Definition at line 304 of file gr55xx_hal_qspi.h.

## ◆ QSPI_DATASIZE_15_BITS

#define QSPI_DATASIZE_15_BITS LL_SSI_DATASIZE_15BIT

Data length for SPI transfer: 15 bits.

Definition at line 305 of file gr55xx_hal_qspi.h.

## ◆ QSPI_DATASIZE_16_BITS

#define QSPI_DATASIZE_16_BITS LL_SSI_DATASIZE_16BIT

Data length for SPI transfer: 16 bits.

Definition at line 306 of file gr55xx_hal_qspi.h.

## ◆ QSPI_DATASIZE_17_BITS

#define QSPI_DATASIZE_17_BITS LL_SSI_DATASIZE_17BIT

Data length for SPI transfer: 17 bits.

Definition at line 307 of file gr55xx_hal_qspi.h.

## ◆ QSPI_DATASIZE_18_BITS

#define QSPI_DATASIZE_18_BITS LL_SSI_DATASIZE_18BIT

Data length for SPI transfer: 18 bits.

Definition at line 308 of file gr55xx_hal_qspi.h.

## ◆ QSPI_DATASIZE_19_BITS

#define QSPI_DATASIZE_19_BITS LL_SSI_DATASIZE_19BIT

Data length for SPI transfer: 19 bits.

Definition at line 309 of file gr55xx_hal_qspi.h.

## ◆ QSPI_DATASIZE_20_BITS

#define QSPI_DATASIZE_20_BITS LL_SSI_DATASIZE_20BIT

Data length for SPI transfer: 20 bits.

Definition at line 310 of file gr55xx_hal_qspi.h.

## ◆ QSPI_DATASIZE_21_BITS

#define QSPI_DATASIZE_21_BITS LL_SSI_DATASIZE_21BIT

Data length for SPI transfer: 21 bits.

Definition at line 311 of file gr55xx_hal_qspi.h.

## ◆ QSPI_DATASIZE_22_BITS

#define QSPI_DATASIZE_22_BITS LL_SSI_DATASIZE_22BIT

Data length for SPI transfer: 22 bits.

Definition at line 312 of file gr55xx_hal_qspi.h.

## ◆ QSPI_DATASIZE_23_BITS

#define QSPI_DATASIZE_23_BITS LL_SSI_DATASIZE_23BIT

Data length for SPI transfer: 23 bits.

Definition at line 313 of file gr55xx_hal_qspi.h.

## ◆ QSPI_DATASIZE_24_BITS

#define QSPI_DATASIZE_24_BITS LL_SSI_DATASIZE_24BIT

Data length for SPI transfer: 24 bits.

Definition at line 314 of file gr55xx_hal_qspi.h.

## ◆ QSPI_DATASIZE_25_BITS

#define QSPI_DATASIZE_25_BITS LL_SSI_DATASIZE_25BIT

Data length for SPI transfer: 25 bits.

Definition at line 315 of file gr55xx_hal_qspi.h.

## ◆ QSPI_DATASIZE_26_BITS

#define QSPI_DATASIZE_26_BITS LL_SSI_DATASIZE_26BIT

Data length for SPI transfer: 26 bits.

Definition at line 316 of file gr55xx_hal_qspi.h.

## ◆ QSPI_DATASIZE_27_BITS

#define QSPI_DATASIZE_27_BITS LL_SSI_DATASIZE_27BIT

Data length for SPI transfer: 27 bits.

Definition at line 317 of file gr55xx_hal_qspi.h.

## ◆ QSPI_DATASIZE_28_BITS

#define QSPI_DATASIZE_28_BITS LL_SSI_DATASIZE_28BIT

Data length for SPI transfer: 28 bits.

Definition at line 318 of file gr55xx_hal_qspi.h.

## ◆ QSPI_DATASIZE_29_BITS

#define QSPI_DATASIZE_29_BITS LL_SSI_DATASIZE_29BIT

Data length for SPI transfer: 29 bits.

Definition at line 319 of file gr55xx_hal_qspi.h.

## ◆ QSPI_DATASIZE_30_BITS

#define QSPI_DATASIZE_30_BITS LL_SSI_DATASIZE_30BIT

Data length for SPI transfer: 30 bits.

Definition at line 320 of file gr55xx_hal_qspi.h.

## ◆ QSPI_DATASIZE_31_BITS

#define QSPI_DATASIZE_31_BITS LL_SSI_DATASIZE_31BIT

Data length for SPI transfer: 31 bits.

Definition at line 321 of file gr55xx_hal_qspi.h.

## ◆ QSPI_DATASIZE_32_BITS

#define QSPI_DATASIZE_32_BITS LL_SSI_DATASIZE_32BIT

Data length for SPI transfer: 32 bits.

Definition at line 322 of file gr55xx_hal_qspi.h.