Macros
GAP Address types
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Connection Control » Defines
Collaboration diagram for GAP Address types:

## Macros
#define | BLE_GAP_ADDR_TYPE_PUBLIC 0x00
| Public (identity) address. More...
#define | BLE_GAP_ADDR_TYPE_RANDOM_STATIC 0x01
| Random static (identity) address. More...

## Detailed Description

## Macro Definition Documentation

## ◆ BLE_GAP_ADDR_TYPE_PUBLIC

#define BLE_GAP_ADDR_TYPE_PUBLIC 0x00

Public (identity) address.

Definition at line 75 of file ble_gapc.h.

## ◆ BLE_GAP_ADDR_TYPE_RANDOM_STATIC

#define BLE_GAP_ADDR_TYPE_RANDOM_STATIC 0x01

Random static (identity) address.

Definition at line 76 of file ble_gapc.h.