Functions
IT_Management
Peripheral Driver » LL Driver » AON_GPIO » Functions
Collaboration diagram for IT_Management:

## Functions
__STATIC_INLINE void | ll_aon_gpio_enable_falling_trigger (uint32_t pin_mask)
| Enable AON_GPIO Falling Edge Trigger of specified AON_GPIO pins. More...
__STATIC_INLINE uint32_t | ll_aon_gpio_is_enabled_falling_trigger (uint32_t pin_mask)
| Check if falling edge trigger is enabled of specified AON_GPIO pins. More...
__STATIC_INLINE void | ll_aon_gpio_enable_rising_trigger (uint32_t pin_mask)
| Enable AON_GPIO Rising Edge Trigger of specified AON_GPIO pins. More...
__STATIC_INLINE uint32_t | ll_aon_gpio_is_enabled_rising_trigger (uint32_t pin_mask)
| Check if rising edge trigger is enabled of specified AON_GPIO pins. More...
__STATIC_INLINE void | ll_aon_gpio_enable_high_trigger (uint32_t pin_mask)
| Enable AON_GPIO High Level Trigger of specified AON_GPIO pins. More...
__STATIC_INLINE uint32_t | ll_aon_gpio_is_enabled_high_trigger (uint32_t pin_mask)
| Check if high level trigger is enabled of specified AON_GPIO pins. More...
__STATIC_INLINE void | ll_aon_gpio_enable_low_trigger (uint32_t pin_mask)
| Enable AON_GPIO Low Level Trigger of specified AON_GPIO pins. More...
__STATIC_INLINE uint32_t | ll_aon_gpio_is_enabled_low_trigger (uint32_t pin_mask)
| Check if low level trigger is enabled of specified AON_GPIO pins. More...
__STATIC_INLINE void | ll_aon_gpio_enable_it (uint32_t pin_mask)
| Enable AON_GPIO interrupts of specified AON_GPIO pins. More...
__STATIC_INLINE void | ll_aon_gpio_disable_it (uint32_t pin_mask)
| Disable AON_GPIO interrupts of specified AON_GPIO pins. More...
__STATIC_INLINE uint32_t | ll_aon_gpio_is_enabled_it (uint32_t pin_mask)
| Check if the Interrupt of specified GPIO pins is enabled or disabled. More...

## Detailed Description

## Function Documentation

## ◆ ll_aon_gpio_disable_it()

__STATIC_INLINE void ll_aon_gpio_disable_it | ( | uint32_t | pin_mask | ) |

Disable AON_GPIO interrupts of specified AON_GPIO pins.

Note
  Interrupt Trigger can be used to specify the interrupt trigger type

\rst +-------------------—+--------------------------------—+ | Register | BitsName | +======================+===================================+ | INTENCLR | INTENCLR | +-------------------—+--------------------------------—+ \endrst

Parameters

  pin_mask | This parameter can be a combination of the following values: LL_AON_GPIO_PIN_0 LL_AON_GPIO_PIN_1 LL_AON_GPIO_PIN_2 LL_AON_GPIO_PIN_3 LL_AON_GPIO_PIN_4 LL_AON_GPIO_PIN_5 LL_AON_GPIO_PIN_6 LL_AON_GPIO_PIN_7 LL_AON_GPIO_PIN_ALL

Return values

  None |

Definition at line 1055 of file gr55xx_ll_aon_gpio.h.

## ◆ ll_aon_gpio_enable_falling_trigger()

__STATIC_INLINE void ll_aon_gpio_enable_falling_trigger | ( | uint32_t | pin_mask | ) |

Enable AON_GPIO Falling Edge Trigger of specified AON_GPIO pins.

\rst +-------------------—+--------------------------------—+ | Register | BitsName | +======================+===================================+ | INTPOLCLR | INTPOLCLR | +-------------------—+--------------------------------—+ \endrst INTTYPESET | INTTYPESET

Parameters

  pin_mask | This parameter can be a combination of the following values: LL_AON_GPIO_PIN_0 LL_AON_GPIO_PIN_1 LL_AON_GPIO_PIN_2 LL_AON_GPIO_PIN_3 LL_AON_GPIO_PIN_4 LL_AON_GPIO_PIN_5 LL_AON_GPIO_PIN_6 LL_AON_GPIO_PIN_7 LL_AON_GPIO_PIN_ALL

Return values

  None |

Definition at line 785 of file gr55xx_ll_aon_gpio.h.

## ◆ ll_aon_gpio_enable_high_trigger()

__STATIC_INLINE void ll_aon_gpio_enable_high_trigger | ( | uint32_t | pin_mask | ) |

Enable AON_GPIO High Level Trigger of specified AON_GPIO pins.

\rst +-------------------—+--------------------------------—+ | Register | BitsName | +======================+===================================+ | INTPOLSET | INTPOLSET | +-------------------—+--------------------------------—+ \endrst INTTYPECLR | INTTYPECLR

Parameters

  pin_mask | This parameter can be a combination of the following values: LL_AON_GPIO_PIN_0 LL_AON_GPIO_PIN_1 LL_AON_GPIO_PIN_2 LL_AON_GPIO_PIN_3 LL_AON_GPIO_PIN_4 LL_AON_GPIO_PIN_5 LL_AON_GPIO_PIN_6 LL_AON_GPIO_PIN_7 LL_AON_GPIO_PIN_ALL

Return values

  None |

Definition at line 906 of file gr55xx_ll_aon_gpio.h.

## ◆ ll_aon_gpio_enable_it()

__STATIC_INLINE void ll_aon_gpio_enable_it | ( | uint32_t | pin_mask | ) |

Enable AON_GPIO interrupts of specified AON_GPIO pins.

Note
  Interrupt Trigger can be used to specify the interrupt trigger type

\rst +-------------------—+--------------------------------—+ | Register | BitsName | +======================+===================================+ | INTENSET | INTENSET | +-------------------—+--------------------------------—+ \endrst

Parameters

  pin_mask | This parameter can be a combination of the following values: LL_AON_GPIO_PIN_0 LL_AON_GPIO_PIN_1 LL_AON_GPIO_PIN_2 LL_AON_GPIO_PIN_3 LL_AON_GPIO_PIN_4 LL_AON_GPIO_PIN_5 LL_AON_GPIO_PIN_6 LL_AON_GPIO_PIN_7 LL_AON_GPIO_PIN_ALL

Return values

  None |

Definition at line 1026 of file gr55xx_ll_aon_gpio.h.

## ◆ ll_aon_gpio_enable_low_trigger()

__STATIC_INLINE void ll_aon_gpio_enable_low_trigger | ( | uint32_t | pin_mask | ) |

Enable AON_GPIO Low Level Trigger of specified AON_GPIO pins.

\rst +-------------------—+--------------------------------—+ | Register | BitsName | +======================+===================================+ | INTPOLCLR | INTPOLCLR | +-------------------—+--------------------------------—+ \endrst INTTYPECLR | INTTYPECLR

Parameters

  pin_mask | This parameter can be a combination of the following values: LL_AON_GPIO_PIN_0 LL_AON_GPIO_PIN_1 LL_AON_GPIO_PIN_2 LL_AON_GPIO_PIN_3 LL_AON_GPIO_PIN_4 LL_AON_GPIO_PIN_5 LL_AON_GPIO_PIN_6 LL_AON_GPIO_PIN_7 LL_AON_GPIO_PIN_ALL

Return values

  None |

Definition at line 966 of file gr55xx_ll_aon_gpio.h.

## ◆ ll_aon_gpio_enable_rising_trigger()

__STATIC_INLINE void ll_aon_gpio_enable_rising_trigger | ( | uint32_t | pin_mask | ) |

Enable AON_GPIO Rising Edge Trigger of specified AON_GPIO pins.

\rst +-------------------—+--------------------------------—+ | Register | BitsName | +======================+===================================+ | INTPOLSET | INTPOLSET | +-------------------—+--------------------------------—+ \endrst INTTYPESET | INTTYPESET

Parameters

  pin_mask | This parameter can be a combination of the following values: LL_AON_GPIO_PIN_0 LL_AON_GPIO_PIN_1 LL_AON_GPIO_PIN_2 LL_AON_GPIO_PIN_3 LL_AON_GPIO_PIN_4 LL_AON_GPIO_PIN_5 LL_AON_GPIO_PIN_6 LL_AON_GPIO_PIN_7 LL_AON_GPIO_PIN_ALL

Return values

  None |

Definition at line 845 of file gr55xx_ll_aon_gpio.h.

## ◆ ll_aon_gpio_is_enabled_falling_trigger()

__STATIC_INLINE uint32_t ll_aon_gpio_is_enabled_falling_trigger | ( | uint32_t | pin_mask | ) |

Check if falling edge trigger is enabled of specified AON_GPIO pins.

\rst +-------------------—+--------------------------------—+ | Register | BitsName | +======================+===================================+ | INTPOLCLR | INTPOLCLR | +-------------------—+--------------------------------—+ \endrst INTTYPESET | INTTYPESET

Parameters

  pin_mask | This parameter can be a combination of the following values: LL_AON_GPIO_PIN_0 LL_AON_GPIO_PIN_1 LL_AON_GPIO_PIN_2 LL_AON_GPIO_PIN_3 LL_AON_GPIO_PIN_4 LL_AON_GPIO_PIN_5 LL_AON_GPIO_PIN_6 LL_AON_GPIO_PIN_7 LL_AON_GPIO_PIN_ALL

Return values

  State | of bit (1 or 0).

Definition at line 815 of file gr55xx_ll_aon_gpio.h.

## ◆ ll_aon_gpio_is_enabled_high_trigger()

__STATIC_INLINE uint32_t ll_aon_gpio_is_enabled_high_trigger | ( | uint32_t | pin_mask | ) |

Check if high level trigger is enabled of specified AON_GPIO pins.

\rst +-------------------—+--------------------------------—+ | Register | BitsName | +======================+===================================+ | INTPOLSET | INTPOLSET | +-------------------—+--------------------------------—+ \endrst INTTYPECLR | INTTYPECLR

Parameters

  pin_mask | This parameter can be a combination of the following values: LL_AON_GPIO_PIN_0 LL_AON_GPIO_PIN_1 LL_AON_GPIO_PIN_2 LL_AON_GPIO_PIN_3 LL_AON_GPIO_PIN_4 LL_AON_GPIO_PIN_5 LL_AON_GPIO_PIN_6 LL_AON_GPIO_PIN_7 LL_AON_GPIO_PIN_ALL

Return values

  State | of bit (1 or 0).

Definition at line 936 of file gr55xx_ll_aon_gpio.h.

## ◆ ll_aon_gpio_is_enabled_it()

__STATIC_INLINE uint32_t ll_aon_gpio_is_enabled_it | ( | uint32_t | pin_mask | ) |

Check if the Interrupt of specified GPIO pins is enabled or disabled.

\rst +-------------------—+--------------------------------—+ | Register | BitsName | +======================+===================================+ | INTENSET | INTENSET | +-------------------—+--------------------------------—+ \endrst

Parameters

  pin_mask | This parameter can be a combination of the following values: LL_AON_GPIO_PIN_0 LL_AON_GPIO_PIN_1 LL_AON_GPIO_PIN_2 LL_AON_GPIO_PIN_3 LL_AON_GPIO_PIN_4 LL_AON_GPIO_PIN_5 LL_AON_GPIO_PIN_6 LL_AON_GPIO_PIN_7 LL_AON_GPIO_PIN_ALL

Return values

  State | of bit (1 or 0).

Definition at line 1083 of file gr55xx_ll_aon_gpio.h.

## ◆ ll_aon_gpio_is_enabled_low_trigger()

__STATIC_INLINE uint32_t ll_aon_gpio_is_enabled_low_trigger | ( | uint32_t | pin_mask | ) |

Check if low level trigger is enabled of specified AON_GPIO pins.

\rst +-------------------—+--------------------------------—+ | Register | BitsName | +======================+===================================+ | INTPOLCLR | INTPOLCLR | +-------------------—+--------------------------------—+ \endrst INTTYPECLR | INTTYPECLR

Parameters

  pin_mask | This parameter can be a combination of the following values: LL_AON_GPIO_PIN_0 LL_AON_GPIO_PIN_1 LL_AON_GPIO_PIN_2 LL_AON_GPIO_PIN_3 LL_AON_GPIO_PIN_4 LL_AON_GPIO_PIN_5 LL_AON_GPIO_PIN_6 LL_AON_GPIO_PIN_7 LL_AON_GPIO_PIN_ALL

Return values

  State | of bit (1 or 0).

Definition at line 996 of file gr55xx_ll_aon_gpio.h.

## ◆ ll_aon_gpio_is_enabled_rising_trigger()

__STATIC_INLINE uint32_t ll_aon_gpio_is_enabled_rising_trigger | ( | uint32_t | pin_mask | ) |

Check if rising edge trigger is enabled of specified AON_GPIO pins.

Note
  Please check each device line mapping for AON_GPIO Line availability

\rst +-------------------—+--------------------------------—+ | Register | BitsName | +======================+===================================+ | INTPOLSET | INTPOLSET | +-------------------—+--------------------------------—+ \endrst INTTYPESET | INTTYPESET

Parameters

  pin_mask | This parameter can be a combination of the following values: LL_AON_GPIO_PIN_0 LL_AON_GPIO_PIN_1 LL_AON_GPIO_PIN_2 LL_AON_GPIO_PIN_3 LL_AON_GPIO_PIN_4 LL_AON_GPIO_PIN_5 LL_AON_GPIO_PIN_6 LL_AON_GPIO_PIN_7 LL_AON_GPIO_PIN_ALL

Return values

  State | of bit (1 or 0).

Definition at line 876 of file gr55xx_ll_aon_gpio.h.