Here is a list of all file members with links to the files they belong to:

### - h -

- hal_adc_callback_t : gr55xx_hal_adc.h
- hal_adc_conv_cplt_callback() : gr55xx_hal_adc.h
- hal_adc_deinit() : gr55xx_hal_adc.h
- HAL_ADC_ERROR_DMA : gr55xx_hal_adc.h
- HAL_ADC_ERROR_INVALID_PARAM : gr55xx_hal_adc.h
- HAL_ADC_ERROR_NONE : gr55xx_hal_adc.h
- HAL_ADC_ERROR_TIMEOUT : gr55xx_hal_adc.h
- hal_adc_get_dma_threshold() : gr55xx_hal_adc.h
- hal_adc_get_error() : gr55xx_hal_adc.h
- hal_adc_get_state() : gr55xx_hal_adc.h
- hal_adc_init() : gr55xx_hal_adc.h
- HAL_ADC_MODULE_ENABLED : gr55xx_hal_conf.h
- hal_adc_msp_deinit() : gr55xx_hal_adc.h
- hal_adc_msp_init() : gr55xx_hal_adc.h
- hal_adc_poll_for_conversion() : gr55xx_hal_adc.h
- hal_adc_resume_reg() : gr55xx_hal_adc.h
- hal_adc_set_dma_threshold() : gr55xx_hal_adc.h
- hal_adc_start_dma() : gr55xx_hal_adc.h
- HAL_ADC_STATE_BUSY : gr55xx_hal_adc.h
- HAL_ADC_STATE_ERROR : gr55xx_hal_adc.h
- HAL_ADC_STATE_READY : gr55xx_hal_adc.h
- HAL_ADC_STATE_RESET : gr55xx_hal_adc.h
- hal_adc_state_t : gr55xx_hal_adc.h
- hal_adc_stop_dma() : gr55xx_hal_adc.h
- hal_adc_suspend_reg() : gr55xx_hal_adc.h
- hal_adc_temp_init() : gr55xx_hal_adc_temp_api.h
- hal_adc_temp_read() : gr55xx_hal_adc_temp_api.h
- hal_adc_vbat_init() : gr55xx_hal_adc_vbat_api.h
- hal_adc_vbat_read() : gr55xx_hal_adc_vbat_api.h
- hal_adc_voltage_extern() : gr55xx_hal_adc_voltage_api.h
- hal_adc_voltage_intern() : gr55xx_hal_adc_voltage_api.h
- hal_aes_callback_t : gr55xx_hal_aes.h
- hal_aes_cbc_decrypt() : gr55xx_hal_aes.h
- hal_aes_cbc_decrypt_dma() : gr55xx_hal_aes.h
- hal_aes_cbc_decrypt_it() : gr55xx_hal_aes.h
- hal_aes_cbc_encrypt() : gr55xx_hal_aes.h
- hal_aes_cbc_encrypt_dma() : gr55xx_hal_aes.h
- hal_aes_cbc_encrypt_it() : gr55xx_hal_aes.h
- hal_aes_deinit() : gr55xx_hal_aes.h
- hal_aes_done_callback() : gr55xx_hal_aes.h
- hal_aes_ecb_decrypt() : gr55xx_hal_aes.h
- hal_aes_ecb_decrypt_dma() : gr55xx_hal_aes.h
- hal_aes_ecb_decrypt_it() : gr55xx_hal_aes.h
- hal_aes_ecb_encrypt() : gr55xx_hal_aes.h
- hal_aes_ecb_encrypt_dma() : gr55xx_hal_aes.h
- hal_aes_ecb_encrypt_it() : gr55xx_hal_aes.h
- hal_aes_error_callback() : gr55xx_hal_aes.h
- HAL_AES_ERROR_INVALID_PARAM : gr55xx_hal_aes.h
- HAL_AES_ERROR_NONE : gr55xx_hal_aes.h
- HAL_AES_ERROR_TIMEOUT : gr55xx_hal_aes.h
- HAL_AES_ERROR_TRANSFER : gr55xx_hal_aes.h
- hal_aes_get_error() : gr55xx_hal_aes.h
- hal_aes_get_state() : gr55xx_hal_aes.h
- hal_aes_init() : gr55xx_hal_aes.h
- hal_aes_irq_handler() : gr55xx_hal_aes.h
- HAL_AES_MODULE_ENABLED : gr55xx_hal_conf.h
- hal_aes_msp_deinit() : gr55xx_hal_aes.h
- hal_aes_msp_init() : gr55xx_hal_aes.h
- hal_aes_resume_reg() : gr55xx_hal_aes.h
- hal_aes_set_timeout() : gr55xx_hal_aes.h
- HAL_AES_STATE_BUSY : gr55xx_hal_aes.h
- HAL_AES_STATE_ERROR : gr55xx_hal_aes.h
- HAL_AES_STATE_READY : gr55xx_hal_aes.h
- HAL_AES_STATE_RESET : gr55xx_hal_aes.h
- HAL_AES_STATE_SUSPENDED : gr55xx_hal_aes.h
- hal_aes_state_t : gr55xx_hal_aes.h
- HAL_AES_STATE_TIMEOUT : gr55xx_hal_aes.h
- hal_aes_suspend_reg() : gr55xx_hal_aes.h
- HAL_AES_TIMEOUT_DEFAULT_VALUE : gr55xx_hal_aes.h
- hal_aon_gpio_callback() : gr55xx_hal_aon_gpio.h
- hal_aon_gpio_callback_t : gr55xx_hal_aon_gpio.h
- hal_aon_gpio_deinit() : gr55xx_hal_aon_gpio.h
- hal_aon_gpio_init() : gr55xx_hal_aon_gpio.h
- hal_aon_gpio_irq_handler() : gr55xx_hal_aon_gpio.h
- HAL_AON_GPIO_MODULE_ENABLED : gr55xx_hal_conf.h
- hal_aon_gpio_read_pin() : gr55xx_hal_aon_gpio.h
- hal_aon_gpio_toggle_pin() : gr55xx_hal_aon_gpio.h
- hal_aon_gpio_write_pin() : gr55xx_hal_aon_gpio.h
- hal_aon_wdt_alarm_callback() : gr55xx_hal_aon_wdt.h
- hal_aon_wdt_callback_t : gr55xx_hal_aon_wdt.h
- hal_aon_wdt_deinit() : gr55xx_hal_aon_wdt.h
- hal_aon_wdt_init() : gr55xx_hal_aon_wdt.h
- hal_aon_wdt_irq_handler() : gr55xx_hal_aon_wdt.h
- HAL_AON_WDT_MODULE_ENABLED : gr55xx_hal_conf.h
- hal_aon_wdt_refresh() : gr55xx_hal_aon_wdt.h
- HAL_BOD2_DISABLE : gr55xx_hal_bod.h
- hal_bod2_enable() : gr55xx_hal_bod.h
- HAL_BOD2_ENABLE : gr55xx_hal_bod.h
- HAL_BOD2_LEVEL_0 : gr55xx_hal_bod.h
- HAL_BOD2_LEVEL_1 : gr55xx_hal_bod.h
- HAL_BOD2_LEVEL_2 : gr55xx_hal_bod.h
- HAL_BOD2_LEVEL_3 : gr55xx_hal_bod.h
- HAL_BOD2_LEVEL_4 : gr55xx_hal_bod.h
- HAL_BOD2_LEVEL_5 : gr55xx_hal_bod.h
- HAL_BOD2_LEVEL_6 : gr55xx_hal_bod.h
- HAL_BOD2_LEVEL_7 : gr55xx_hal_bod.h
- hal_bod2_set_level() : gr55xx_hal_bod.h
- hal_bod_deinit() : gr55xx_hal_bod.h
- HAL_BOD_DISABLE : gr55xx_hal_bod.h
- HAL_BOD_ENABLE : gr55xx_hal_bod.h
- hal_bod_enable() : gr55xx_hal_bod.h
- hal_bod_fedge_callback() : gr55xx_hal_bod.h
- hal_bod_fedge_irq_handler() : gr55xx_hal_bod.h
- hal_bod_init() : gr55xx_hal_bod.h
- HAL_BOD_MODULE_ENABLED : gr55xx_hal_conf.h
- hal_bod_msp_deinit() : gr55xx_hal_bod.h
- hal_bod_msp_init() : gr55xx_hal_bod.h
- HAL_BOD_STATIC_DISABLE : gr55xx_hal_bod.h
- HAL_BOD_STATIC_ENABLE : gr55xx_hal_bod.h
- hal_bod_static_mode_enable() : gr55xx_hal_bod.h
- HAL_BUSY : gr55xx_hal_def.h
- hal_calendar_alarm_callback() : gr55xx_hal_calendar.h
- hal_calendar_callback_t : gr55xx_hal_calendar.h
- hal_calendar_deinit() : gr55xx_hal_calendar.h
- hal_calendar_disable_event() : gr55xx_hal_calendar.h
- hal_calendar_get_time() : gr55xx_hal_calendar.h
- hal_calendar_init() : gr55xx_hal_calendar.h
- hal_calendar_init_time() : gr55xx_hal_calendar.h
- hal_calendar_irq_handler() : gr55xx_hal_calendar.h
- HAL_CALENDAR_MODULE_ENABLED : gr55xx_hal_conf.h
- hal_calendar_overflow_callback() : gr55xx_hal_calendar.h
- hal_calendar_set_alarm() : gr55xx_hal_calendar.h
- hal_calendar_set_tick() : gr55xx_hal_calendar.h
- HAL_CALENDAR_STATE_ERROR : gr55xx_hal_calendar.h
- HAL_CALENDAR_STATE_READY : gr55xx_hal_calendar.h
- HAL_CALENDAR_STATE_RESET : gr55xx_hal_calendar.h
- hal_calendar_tick_callback() : gr55xx_hal_calendar.h
- hal_calender_state_t : gr55xx_hal_calendar.h
- hal_callback_t : gr55xx_hal.h
- hal_cgc_config_force_clk() : gr55xx_hal_cgc.h
- hal_cgc_config_wfi_clk() : gr55xx_hal_cgc.h
- hal_cgc_deinit() : gr55xx_hal_cgc.h
- hal_cgc_get_force_clk() : gr55xx_hal_cgc.h
- hal_cgc_get_wfi_clk() : gr55xx_hal_cgc.h
- hal_cgc_init() : gr55xx_hal_cgc.h
- HAL_CGC_MODULE_ENABLED : gr55xx_hal_conf.h
- hal_comp_callback_t : gr55xx_hal_comp.h
- hal_comp_deinit() : gr55xx_hal_comp.h
- HAL_COMP_ERROR_INVALID_PARAM : gr55xx_hal_comp.h
- HAL_COMP_ERROR_NONE : gr55xx_hal_comp.h
- HAL_COMP_ERROR_TIMEOUT : gr55xx_hal_comp.h
- hal_comp_get_error() : gr55xx_hal_comp.h
- hal_comp_get_state() : gr55xx_hal_comp.h
- hal_comp_init() : gr55xx_hal_comp.h
- hal_comp_irq_handler() : gr55xx_hal_comp.h
- HAL_COMP_MODULE_ENABLED : gr55xx_hal_conf.h
- hal_comp_msp_deinit() : gr55xx_hal_comp.h
- hal_comp_msp_init() : gr55xx_hal_comp.h
- hal_comp_resume_reg() : gr55xx_hal_comp.h
- hal_comp_start() : gr55xx_hal_comp.h
- HAL_COMP_STATE_BUSY : gr55xx_hal_comp.h
- HAL_COMP_STATE_ERROR : gr55xx_hal_comp.h
- HAL_COMP_STATE_READY : gr55xx_hal_comp.h
- HAL_COMP_STATE_RESET : gr55xx_hal_comp.h
- hal_comp_state_t : gr55xx_hal_comp.h
- hal_comp_stop() : gr55xx_hal_comp.h
- hal_comp_suspend_reg() : gr55xx_hal_comp.h
- hal_comp_trigger_callback() : gr55xx_hal_comp.h
- HAL_CORTEX_MODULE_ENABLED : gr55xx_hal_conf.h
- hal_deinit() : gr55xx_hal.h
- hal_dma_abort() : gr55xx_hal_dma.h
- hal_dma_abort_it() : gr55xx_hal_dma.h
- hal_dma_callback_id_t : gr55xx_hal_dma.h
- hal_dma_deinit() : gr55xx_hal_dma.h
- HAL_DMA_ERROR_NO_XFER : gr55xx_hal_dma.h
- HAL_DMA_ERROR_NONE : gr55xx_hal_dma.h
- HAL_DMA_ERROR_TE : gr55xx_hal_dma.h
- HAL_DMA_ERROR_TIMEOUT : gr55xx_hal_dma.h
- hal_dma_get_error() : gr55xx_hal_dma.h
- hal_dma_get_state() : gr55xx_hal_dma.h
- hal_dma_init() : gr55xx_hal_dma.h
- hal_dma_irq_handler() : gr55xx_hal_dma.h
- HAL_DMA_MODULE_ENABLED : gr55xx_hal_conf.h
- hal_dma_poll_for_transfer() : gr55xx_hal_dma.h
- hal_dma_register_callback() : gr55xx_hal_dma.h
- hal_dma_resume_reg() : gr55xx_hal_dma.h
- hal_dma_start() : gr55xx_hal_dma.h
- hal_dma_start_it() : gr55xx_hal_dma.h
- HAL_DMA_STATE_BUSY : gr55xx_hal_dma.h
- HAL_DMA_STATE_ERROR : gr55xx_hal_dma.h
- HAL_DMA_STATE_READY : gr55xx_hal_dma.h
- HAL_DMA_STATE_RESET : gr55xx_hal_dma.h
- hal_dma_state_t : gr55xx_hal_dma.h
- HAL_DMA_STATE_TIMEOUT : gr55xx_hal_dma.h
- hal_dma_suspend_reg() : gr55xx_hal_dma.h
- hal_dma_unregister_callback() : gr55xx_hal_dma.h
- HAL_DMA_XFER_ABORT_CB_ID : gr55xx_hal_dma.h
- HAL_DMA_XFER_ALL_CB_ID : gr55xx_hal_dma.h
- HAL_DMA_XFER_BLK_CB_ID : gr55xx_hal_dma.h
- HAL_DMA_XFER_ERROR_CB_ID : gr55xx_hal_dma.h
- HAL_DMA_XFER_TFR_CB_ID : gr55xx_hal_dma.h
- hal_dual_timer_base_deinit() : gr55xx_hal_dual_tim.h
- hal_dual_timer_base_init() : gr55xx_hal_dual_tim.h
- hal_dual_timer_base_msp_deinit() : gr55xx_hal_dual_tim.h
- hal_dual_timer_base_msp_init() : gr55xx_hal_dual_tim.h
- hal_dual_timer_base_start() : gr55xx_hal_dual_tim.h
- hal_dual_timer_base_start_it() : gr55xx_hal_dual_tim.h
- hal_dual_timer_base_stop() : gr55xx_hal_dual_tim.h
- hal_dual_timer_base_stop_it() : gr55xx_hal_dual_tim.h
- hal_dual_timer_callback_t : gr55xx_hal_dual_tim.h
- hal_dual_timer_get_counter_value() : gr55xx_hal_dual_tim.h
- hal_dual_timer_get_state() : gr55xx_hal_dual_tim.h
- hal_dual_timer_irq_handler() : gr55xx_hal_dual_tim.h
- HAL_DUAL_TIMER_MODULE_ENABLED : gr55xx_hal_conf.h
- hal_dual_timer_period_elapsed_callback() : gr55xx_hal_dual_tim.h
- hal_dual_timer_set_background_reload() : gr55xx_hal_dual_tim.h
- hal_dual_timer_set_config() : gr55xx_hal_dual_tim.h
- hal_dual_timer_set_reload_background_reload() : gr55xx_hal_dual_tim.h
- HAL_DUAL_TIMER_STATE_BUSY : gr55xx_hal_dual_tim.h
- HAL_DUAL_TIMER_STATE_ERROR : gr55xx_hal_dual_tim.h
- HAL_DUAL_TIMER_STATE_READY : gr55xx_hal_dual_tim.h
- HAL_DUAL_TIMER_STATE_RESET : gr55xx_hal_dual_tim.h
- hal_dual_timer_state_t : gr55xx_hal_dual_tim.h
- hal_dwt_disable() : gr55xx_delay.h
- hal_dwt_enable() : gr55xx_delay.h
- hal_eflash_security : gr55xx_hal_exflash.h
- hal_efuse_callback_t : gr55xx_hal_efuse.h
- hal_efuse_crc_calculate() : gr55xx_hal_efuse.h
- hal_efuse_deinit() : gr55xx_hal_efuse.h
- HAL_EFUSE_ERROR_INVALID_PARAM : gr55xx_hal_efuse.h
- HAL_EFUSE_ERROR_NONE : gr55xx_hal_efuse.h
- HAL_EFUSE_ERROR_TIMEOUT : gr55xx_hal_efuse.h
- hal_efuse_init() : gr55xx_hal_efuse.h
- hal_efuse_initial_value_check() : gr55xx_hal_efuse.h
- HAL_EFUSE_MODULE_ENABLED : gr55xx_hal_conf.h
- hal_efuse_msp_deinit() : gr55xx_hal_efuse.h
- hal_efuse_msp_init() : gr55xx_hal_efuse.h
- hal_efuse_read() : gr55xx_hal_efuse.h
- hal_efuse_read_trim() : gr55xx_hal_efuse.h
- hal_efuse_set_main_backup() : gr55xx_hal_efuse.h
- HAL_EFUSE_STATE_BUSY : gr55xx_hal_efuse.h
- HAL_EFUSE_STATE_ERROR : gr55xx_hal_efuse.h
- HAL_EFUSE_STATE_READY : gr55xx_hal_efuse.h
- HAL_EFUSE_STATE_RESET : gr55xx_hal_efuse.h
- hal_efuse_state_t : gr55xx_hal_efuse.h
- hal_efuse_write() : gr55xx_hal_efuse.h
- hal_efuse_write_keyram() : gr55xx_hal_efuse.h
- HAL_ERR_CODE_CHECK : app_drv_error.h
- HAL_ERROR : gr55xx_hal_def.h
- hal_exflash_callback_t : gr55xx_hal_exflash.h
- hal_exflash_deepsleep() : gr55xx_hal_exflash.h
- hal_exflash_deinit() : gr55xx_hal_exflash.h
- HAL_EXFLASH_ENCRYPTED : gr55xx_hal_exflash.h
- hal_exflash_erase() : gr55xx_hal_exflash.h
- HAL_EXFLASH_ERROR_ID : gr55xx_hal_exflash.h
- HAL_EXFLASH_ERROR_INVALID_PARAM : gr55xx_hal_exflash.h
- HAL_EXFLASH_ERROR_NONE : gr55xx_hal_exflash.h
- HAL_EXFLASH_ERROR_QUAD : gr55xx_hal_exflash.h
- HAL_EXFLASH_ERROR_TIMEOUT : gr55xx_hal_exflash.h
- HAL_EXFLASH_ERROR_TRANSFER : gr55xx_hal_exflash.h
- hal_exflash_get_error() : gr55xx_hal_exflash.h
- hal_exflash_get_state() : gr55xx_hal_exflash.h
- hal_exflash_init() : gr55xx_hal_exflash.h
- hal_exflash_lock() : gr55xx_hal_exflash.h
- HAL_EXFLASH_MODULE_ENABLED : gr55xx_hal_conf.h
- hal_exflash_msp_deinit() : gr55xx_hal_exflash.h
- hal_exflash_msp_init() : gr55xx_hal_exflash.h
- hal_exflash_operation() : gr55xx_hal_exflash.h
- hal_exflash_operation_protection() : gr55xx_hal_exflash.h
- hal_exflash_read() : gr55xx_hal_exflash.h
- hal_exflash_read_align_word() : gr55xx_hal_exflash.h
- hal_exflash_read_status_reg() : gr55xx_hal_exflash.h
- hal_exflash_read_uid() : gr55xx_hal_exflash.h
- hal_exflash_reset() : gr55xx_hal_exflash.h
- hal_exflash_resume() : gr55xx_hal_exflash.h
- HAL_EXFLASH_RETRY_DEFAULT_VALUE : gr55xx_hal_exflash.h
- hal_exflash_set_retry() : gr55xx_hal_exflash.h
- HAL_EXFLASH_STATE_BUSY : gr55xx_hal_exflash.h
- HAL_EXFLASH_STATE_BUSY_ERASE : gr55xx_hal_exflash.h
- HAL_EXFLASH_STATE_BUSY_READ : gr55xx_hal_exflash.h
- HAL_EXFLASH_STATE_BUSY_WRITE : gr55xx_hal_exflash.h
- HAL_EXFLASH_STATE_ERROR : gr55xx_hal_exflash.h
- HAL_EXFLASH_STATE_READY : gr55xx_hal_exflash.h
- HAL_EXFLASH_STATE_RESET : gr55xx_hal_exflash.h
- HAL_EXFLASH_STATE_SUSPEND_ERASE : gr55xx_hal_exflash.h
- HAL_EXFLASH_STATE_SUSPEND_WRITE : gr55xx_hal_exflash.h
- hal_exflash_state_t : gr55xx_hal_exflash.h
- hal_exflash_suspend() : gr55xx_hal_exflash.h
- HAL_EXFLASH_UNENCRYPTED : gr55xx_hal_exflash.h
- hal_exflash_unlock() : gr55xx_hal_exflash.h
- hal_exflash_wakeup() : gr55xx_hal_exflash.h
- hal_exflash_write() : gr55xx_hal_exflash.h
- hal_exflash_write_status_reg() : gr55xx_hal_exflash.h
- hal_get_hal_version() : gr55xx_hal.h , hal.h
- hal_gpio_callback_t : gr55xx_hal_gpio.h
- hal_gpio_deinit() : gr55xx_hal_gpio.h
- hal_gpio_exti_callback() : gr55xx_hal_gpio.h
- hal_gpio_exti_irq_handler() : gr55xx_hal_gpio.h
- hal_gpio_init() : gr55xx_hal_gpio.h
- HAL_GPIO_MODULE_ENABLED : gr55xx_hal_conf.h
- hal_gpio_read_pin() : gr55xx_hal_gpio.h
- hal_gpio_toggle_pin() : gr55xx_hal_gpio.h
- hal_gpio_write_pin() : gr55xx_hal_gpio.h
- hal_hmac_callback_t : gr55xx_hal_hmac.h
- hal_hmac_deinit() : gr55xx_hal_hmac.h
- hal_hmac_done_callback() : gr55xx_hal_hmac.h
- hal_hmac_error_callback() : gr55xx_hal_hmac.h
- HAL_HMAC_ERROR_INVALID_PARAM : gr55xx_hal_hmac.h
- HAL_HMAC_ERROR_NONE : gr55xx_hal_hmac.h
- HAL_HMAC_ERROR_TIMEOUT : gr55xx_hal_hmac.h
- HAL_HMAC_ERROR_TRANSFER : gr55xx_hal_hmac.h
- hal_hmac_get_error() : gr55xx_hal_hmac.h
- hal_hmac_get_state() : gr55xx_hal_hmac.h
- hal_hmac_init() : gr55xx_hal_hmac.h
- hal_hmac_irq_handler() : gr55xx_hal_hmac.h
- HAL_HMAC_KEYTYPE_AHB : gr55xx_hal_hmac.h
- HAL_HMAC_KEYTYPE_KRAM : gr55xx_hal_hmac.h
- HAL_HMAC_KEYTYPE_MCU : gr55xx_hal_hmac.h
- HAL_HMAC_MODULE_ENABLED : gr55xx_hal_conf.h
- hal_hmac_msp_deinit() : gr55xx_hal_hmac.h
- hal_hmac_msp_init() : gr55xx_hal_hmac.h
- hal_hmac_resume_reg() : gr55xx_hal_hmac.h
- hal_hmac_set_timeout() : gr55xx_hal_hmac.h
- hal_hmac_sha256_digest() : gr55xx_hal_hmac.h
- hal_hmac_sha256_digest_dma() : gr55xx_hal_hmac.h
- hal_hmac_sha256_digest_it() : gr55xx_hal_hmac.h
- HAL_HMAC_STATE_BUSY : gr55xx_hal_hmac.h
- HAL_HMAC_STATE_ERROR : gr55xx_hal_hmac.h
- HAL_HMAC_STATE_READY : gr55xx_hal_hmac.h
- HAL_HMAC_STATE_RESET : gr55xx_hal_hmac.h
- HAL_HMAC_STATE_SUSPENDED : gr55xx_hal_hmac.h
- hal_hmac_state_t : gr55xx_hal_hmac.h
- HAL_HMAC_STATE_TIMEOUT : gr55xx_hal_hmac.h
- hal_hmac_suspend_reg() : gr55xx_hal_hmac.h
- HAL_HMAC_TIMEOUT_DEFAULT_VALUE : gr55xx_hal_hmac.h
- hal_i2c_abort_cplt_callback() : gr55xx_hal_i2c.h
- hal_i2c_callback_t : gr55xx_hal_i2c.h
- hal_i2c_deinit() : gr55xx_hal_i2c.h
- hal_i2c_disable_listen_it() : gr55xx_hal_i2c.h
- hal_i2c_enable_listen_it() : gr55xx_hal_i2c.h
- HAL_I2C_ERROR_ARB_LOST : gr55xx_hal_i2c.h
- hal_i2c_error_callback() : gr55xx_hal_i2c.h
- HAL_I2C_ERROR_DMA : gr55xx_hal_i2c.h
- HAL_I2C_ERROR_NOACK : gr55xx_hal_i2c.h
- HAL_I2C_ERROR_NONE : gr55xx_hal_i2c.h
- HAL_I2C_ERROR_OVER : gr55xx_hal_i2c.h
- HAL_I2C_ERROR_TIMEOUT : gr55xx_hal_i2c.h
- hal_i2c_get_error() : gr55xx_hal_i2c.h
- hal_i2c_get_mode() : gr55xx_hal_i2c.h
- hal_i2c_get_state() : gr55xx_hal_i2c.h
- hal_i2c_init() : gr55xx_hal_i2c.h
- hal_i2c_irq_handler() : gr55xx_hal_i2c.h
- hal_i2c_listen_cplt_callback() : gr55xx_hal_i2c.h
- hal_i2c_master_abort_it() : gr55xx_hal_i2c.h
- hal_i2c_master_receive() : gr55xx_hal_i2c.h
- hal_i2c_master_receive_dma() : gr55xx_hal_i2c.h
- hal_i2c_master_receive_it() : gr55xx_hal_i2c.h
- hal_i2c_master_rx_cplt_callback() : gr55xx_hal_i2c.h
- hal_i2c_master_sequential_receive_it() : gr55xx_hal_i2c.h
- hal_i2c_master_sequential_transmit_it() : gr55xx_hal_i2c.h
- hal_i2c_master_transmit() : gr55xx_hal_i2c.h
- hal_i2c_master_transmit_dma() : gr55xx_hal_i2c.h
- hal_i2c_master_transmit_it() : gr55xx_hal_i2c.h
- hal_i2c_master_transmit_receive() : gr55xx_hal_i2c.h
- hal_i2c_master_tx_cplt_callback() : gr55xx_hal_i2c.h
- hal_i2c_mem_read() : gr55xx_hal_i2c.h
- hal_i2c_mem_read_dma() : gr55xx_hal_i2c.h
- hal_i2c_mem_read_it() : gr55xx_hal_i2c.h
- hal_i2c_mem_rx_cplt_callback() : gr55xx_hal_i2c.h
- hal_i2c_mem_tx_cplt_callback() : gr55xx_hal_i2c.h
- hal_i2c_mem_write() : gr55xx_hal_i2c.h
- hal_i2c_mem_write_dma() : gr55xx_hal_i2c.h
- hal_i2c_mem_write_it() : gr55xx_hal_i2c.h
- HAL_I2C_MODE_MASTER : gr55xx_hal_i2c.h
- HAL_I2C_MODE_MEM : gr55xx_hal_i2c.h
- HAL_I2C_MODE_NONE : gr55xx_hal_i2c.h
- HAL_I2C_MODE_SLAVE : gr55xx_hal_i2c.h
- hal_i2c_mode_t : gr55xx_hal_i2c.h
- HAL_I2C_MODULE_ENABLED : gr55xx_hal_conf.h
- hal_i2c_msp_deinit() : gr55xx_hal_i2c.h
- hal_i2c_msp_init() : gr55xx_hal_i2c.h
- hal_i2c_resume_reg() : gr55xx_hal_i2c.h
- hal_i2c_slave_receive() : gr55xx_hal_i2c.h
- hal_i2c_slave_receive_dma() : gr55xx_hal_i2c.h
- hal_i2c_slave_receive_it() : gr55xx_hal_i2c.h
- hal_i2c_slave_receive_transmit() : gr55xx_hal_i2c.h
- hal_i2c_slave_rx_cplt_callback() : gr55xx_hal_i2c.h
- hal_i2c_slave_sequential_receive_it() : gr55xx_hal_i2c.h
- hal_i2c_slave_sequential_transmit_it() : gr55xx_hal_i2c.h
- hal_i2c_slave_transmit() : gr55xx_hal_i2c.h
- hal_i2c_slave_transmit_dma() : gr55xx_hal_i2c.h
- hal_i2c_slave_transmit_it() : gr55xx_hal_i2c.h
- hal_i2c_slave_tx_cplt_callback() : gr55xx_hal_i2c.h
- HAL_I2C_STATE_ABORT : gr55xx_hal_i2c.h
- HAL_I2C_STATE_BUSY : gr55xx_hal_i2c.h
- HAL_I2C_STATE_BUSY_RX : gr55xx_hal_i2c.h
- HAL_I2C_STATE_BUSY_RX_LISTEN : gr55xx_hal_i2c.h
- HAL_I2C_STATE_BUSY_TX : gr55xx_hal_i2c.h
- HAL_I2C_STATE_BUSY_TX_LISTEN : gr55xx_hal_i2c.h
- HAL_I2C_STATE_ERROR : gr55xx_hal_i2c.h
- HAL_I2C_STATE_LISTEN : gr55xx_hal_i2c.h
- HAL_I2C_STATE_READY : gr55xx_hal_i2c.h
- HAL_I2C_STATE_RESET : gr55xx_hal_i2c.h
- hal_i2c_state_t : gr55xx_hal_i2c.h
- HAL_I2C_STATE_TIMEOUT : gr55xx_hal_i2c.h
- hal_i2c_suspend_reg() : gr55xx_hal_i2c.h
- hal_i2c_timing_adjust() : gr55xx_hal_i2c.h
- hal_i2c_timing_get() : gr55xx_hal_i2c.h
- hal_i2s_abort() : gr55xx_hal_i2s.h
- hal_i2s_callback_t : gr55xx_hal_i2s.h
- hal_i2s_deinit() : gr55xx_hal_i2s.h
- hal_i2s_error_callback() : gr55xx_hal_i2s.h
- HAL_I2S_ERROR_DMA : gr55xx_hal_i2s.h
- HAL_I2S_ERROR_INVALID_PARAM : gr55xx_hal_i2s.h
- HAL_I2S_ERROR_NONE : gr55xx_hal_i2s.h
- HAL_I2S_ERROR_RX_OVERFLOW : gr55xx_hal_i2s.h
- HAL_I2S_ERROR_TIMEOUT : gr55xx_hal_i2s.h
- HAL_I2S_ERROR_TRANSFER : gr55xx_hal_i2s.h
- HAL_I2S_ERROR_TX_OVERFLOW : gr55xx_hal_i2s.h
- hal_i2s_get_error() : gr55xx_hal_i2s.h
- hal_i2s_get_rx_fifo_threshold() : gr55xx_hal_i2s.h
- hal_i2s_get_state() : gr55xx_hal_i2s.h
- hal_i2s_get_tx_fifo_threshold() : gr55xx_hal_i2s.h
- hal_i2s_init() : gr55xx_hal_i2s.h
- hal_i2s_irq_handler() : gr55xx_hal_i2s.h
- HAL_I2S_MODULE_ENABLED : gr55xx_hal_conf.h
- hal_i2s_msp_deinit() : gr55xx_hal_i2s.h
- hal_i2s_msp_init() : gr55xx_hal_i2s.h
- hal_i2s_receive() : gr55xx_hal_i2s.h
- hal_i2s_receive_dma() : gr55xx_hal_i2s.h
- hal_i2s_receive_it() : gr55xx_hal_i2s.h
- hal_i2s_resume_reg() : gr55xx_hal_i2s.h
- hal_i2s_rx_cplt_callback() : gr55xx_hal_i2s.h
- hal_i2s_set_rx_fifo_threshold() : gr55xx_hal_i2s.h
- hal_i2s_set_tx_fifo_threshold() : gr55xx_hal_i2s.h
- hal_i2s_start_clock() : gr55xx_hal_i2s.h
- HAL_I2S_STATE_ABORT : gr55xx_hal_i2s.h
- HAL_I2S_STATE_BUSY : gr55xx_hal_i2s.h
- HAL_I2S_STATE_BUSY_RX : gr55xx_hal_i2s.h
- HAL_I2S_STATE_BUSY_TX : gr55xx_hal_i2s.h
- HAL_I2S_STATE_BUSY_TX_RX : gr55xx_hal_i2s.h
- HAL_I2S_STATE_ERROR : gr55xx_hal_i2s.h
- HAL_I2S_STATE_READY : gr55xx_hal_i2s.h
- HAL_I2S_STATE_RESET : gr55xx_hal_i2s.h
- hal_i2s_state_t : gr55xx_hal_i2s.h
- hal_i2s_stop_clock() : gr55xx_hal_i2s.h
- hal_i2s_suspend_reg() : gr55xx_hal_i2s.h
- HAL_I2S_TIMEOUT_DEFAULT_VALUE : gr55xx_hal_i2s.h
- hal_i2s_transmit() : gr55xx_hal_i2s.h
- hal_i2s_transmit_dma() : gr55xx_hal_i2s.h
- hal_i2s_transmit_it() : gr55xx_hal_i2s.h
- hal_i2s_transmit_receive() : gr55xx_hal_i2s.h
- hal_i2s_transmit_receive_dma() : gr55xx_hal_i2s.h
- hal_i2s_transmit_receive_it() : gr55xx_hal_i2s.h
- hal_i2s_tx_cplt_callback() : gr55xx_hal_i2s.h
- hal_i2s_tx_rx_cplt_callback() : gr55xx_hal_i2s.h
- hal_init() : gr55xx_hal.h
- hal_init_tick() : gr55xx_hal.h
- HAL_IS_BIT_CLR : gr55xx_hal_def.h
- HAL_IS_BIT_SET : gr55xx_hal_def.h
- hal_iso7816_abort() : gr55xx_hal_iso7816.h
- hal_iso7816_abort_cplt_callback() : gr55xx_hal_iso7816.h
- HAL_ISO7816_ACTION_NONE : gr55xx_hal_iso7816.h
- HAL_ISO7816_ACTION_OFF : gr55xx_hal_iso7816.h
- HAL_ISO7816_ACTION_ON : gr55xx_hal_iso7816.h
- HAL_ISO7816_ACTION_RX : gr55xx_hal_iso7816.h
- HAL_ISO7816_ACTION_STOPCLK : gr55xx_hal_iso7816.h
- HAL_ISO7816_ACTION_TX : gr55xx_hal_iso7816.h
- HAL_ISO7816_ACTION_TXRX : gr55xx_hal_iso7816.h
- HAL_ISO7816_ACTION_WARMRST : gr55xx_hal_iso7816.h
- hal_iso7816_atr_cplt_callback() : gr55xx_hal_iso7816.h
- hal_iso7816_callback_t : gr55xx_hal_iso7816.h
- HAL_ISO7816_CARD_ABSENT : gr55xx_hal_iso7816.h
- HAL_ISO7816_CARD_PRESENT : gr55xx_hal_iso7816.h
- hal_iso7816_deinit() : gr55xx_hal_iso7816.h
- hal_iso7816_error_callback() : gr55xx_hal_iso7816.h
- HAL_ISO7816_ERROR_INVALID_PARAM : gr55xx_hal_iso7816.h
- HAL_ISO7816_ERROR_NONE : gr55xx_hal_iso7816.h
- HAL_ISO7816_ERROR_TIMEOUT : gr55xx_hal_iso7816.h
- HAL_ISO7816_ERROR_TRANSFER : gr55xx_hal_iso7816.h
- hal_iso7816_get_error() : gr55xx_hal_iso7816.h
- hal_iso7816_get_power_states() : gr55xx_hal_iso7816.h
- hal_iso7816_get_state() : gr55xx_hal_iso7816.h
- hal_iso7816_init() : gr55xx_hal_iso7816.h
- HAL_ISO7816_INTR_DMA_ERR : gr55xx_hal_iso7816.h
- HAL_ISO7816_INTR_DONE : gr55xx_hal_iso7816.h
- HAL_ISO7816_INTR_PRESENCE : gr55xx_hal_iso7816.h
- HAL_ISO7816_INTR_RETRY_ERR : gr55xx_hal_iso7816.h
- HAL_ISO7816_INTR_RX_ERR : gr55xx_hal_iso7816.h
- HAL_ISO7816_INTR_STATE_ERR : gr55xx_hal_iso7816.h
- HAL_ISO7816_INTR_TEST : gr55xx_hal_iso7816.h
- HAL_ISO7816_IO_STATE_IDLE : gr55xx_hal_iso7816.h
- HAL_ISO7816_IO_STATE_OFF : gr55xx_hal_iso7816.h
- HAL_ISO7816_IO_STATE_RX : gr55xx_hal_iso7816.h
- HAL_ISO7816_IO_STATE_RX_WAIT : gr55xx_hal_iso7816.h
- HAL_ISO7816_IO_STATE_TX : gr55xx_hal_iso7816.h
- HAL_ISO7816_IO_STATE_TX_GUARD : gr55xx_hal_iso7816.h
- hal_iso7816_irq_handler() : gr55xx_hal_iso7816.h
- HAL_ISO7816_MODULE_ENABLED : gr55xx_hal_conf.h
- hal_iso7816_msp_deinit() : gr55xx_hal_iso7816.h
- hal_iso7816_msp_init() : gr55xx_hal_iso7816.h
- hal_iso7816_presence_callback() : gr55xx_hal_iso7816.h
- HAL_ISO7816_PWR_STATE_IDLE : gr55xx_hal_iso7816.h
- HAL_ISO7816_PWR_STATE_OFF : gr55xx_hal_iso7816.h
- HAL_ISO7816_PWR_STATE_PWRDN_RST : gr55xx_hal_iso7816.h
- HAL_ISO7816_PWR_STATE_PWRDN_VCC : gr55xx_hal_iso7816.h
- HAL_ISO7816_PWR_STATE_PWRUP_RST : gr55xx_hal_iso7816.h
- HAL_ISO7816_PWR_STATE_PWRUP_VCC : gr55xx_hal_iso7816.h
- HAL_ISO7816_PWR_STATE_RX : gr55xx_hal_iso7816.h
- HAL_ISO7816_PWR_STATE_RX_TS0 : gr55xx_hal_iso7816.h
- HAL_ISO7816_PWR_STATE_RX_TS1 : gr55xx_hal_iso7816.h
- HAL_ISO7816_PWR_STATE_STOP : gr55xx_hal_iso7816.h
- HAL_ISO7816_PWR_STATE_STOP_POST : gr55xx_hal_iso7816.h
- HAL_ISO7816_PWR_STATE_STOP_PRE : gr55xx_hal_iso7816.h
- HAL_ISO7816_PWR_STATE_TX : gr55xx_hal_iso7816.h
- HAL_ISO7816_PWR_STATE_TX_RX : gr55xx_hal_iso7816.h
- hal_iso7816_receive() : gr55xx_hal_iso7816.h
- hal_iso7816_receive_it() : gr55xx_hal_iso7816.h
- hal_iso7816_resume_reg() : gr55xx_hal_iso7816.h
- hal_iso7816_rx_cplt_callback() : gr55xx_hal_iso7816.h
- hal_iso7816_set_action() : gr55xx_hal_iso7816.h
- hal_iso7816_set_etudiv() : gr55xx_hal_iso7816.h
- HAL_ISO7816_STATE_ABORT : gr55xx_hal_iso7816.h
- HAL_ISO7816_STATE_BUSY : gr55xx_hal_iso7816.h
- HAL_ISO7816_STATE_BUSY_RX : gr55xx_hal_iso7816.h
- HAL_ISO7816_STATE_BUSY_TX : gr55xx_hal_iso7816.h
- HAL_ISO7816_STATE_BUSY_TX_RX : gr55xx_hal_iso7816.h
- HAL_ISO7816_STATE_ERROR : gr55xx_hal_iso7816.h
- HAL_ISO7816_STATE_READY : gr55xx_hal_iso7816.h
- HAL_ISO7816_STATE_RESET : gr55xx_hal_iso7816.h
- hal_iso7816_state_t : gr55xx_hal_iso7816.h
- HAL_ISO7816_STATE_TIMEOUT : gr55xx_hal_iso7816.h
- hal_iso7816_suspend_reg() : gr55xx_hal_iso7816.h
- hal_iso7816_transmit() : gr55xx_hal_iso7816.h
- hal_iso7816_transmit_it() : gr55xx_hal_iso7816.h
- hal_iso7816_transmit_receive() : gr55xx_hal_iso7816.h
- hal_iso7816_transmit_receive_it() : gr55xx_hal_iso7816.h
- hal_iso7816_tx_cplt_callback() : gr55xx_hal_iso7816.h
- hal_iso7816_tx_rx_cplt_callback() : gr55xx_hal_iso7816.h
- hal_lock_t : gr55xx_hal_def.h
- HAL_LOCKED : gr55xx_hal_def.h
- HAL_MAX_DELAY : gr55xx_hal_def.h
- HAL_MODULE_ENABLED : gr55xx_hal_conf.h
- hal_msio_deinit() : gr55xx_hal_msio.h
- hal_msio_init() : gr55xx_hal_msio.h
- HAL_MSIO_MODULE_ENABLED : gr55xx_hal_conf.h
- hal_msio_read_pin() : gr55xx_hal_msio.h
- hal_msio_toggle_pin() : gr55xx_hal_msio.h
- hal_msio_write_pin() : gr55xx_hal_msio.h
- hal_msp_deinit() : gr55xx_hal.h
- hal_msp_init() : gr55xx_hal.h
- HAL_NEVER_TIMEOUT : gr55xx_hal_def.h
- hal_nvic_clear_pending_irq() : gr55xx_hal_cortex.h
- hal_nvic_disable_irq() : gr55xx_hal_cortex.h
- hal_nvic_enable_irq() : gr55xx_hal_cortex.h
- hal_nvic_get_active() : gr55xx_hal_cortex.h
- hal_nvic_get_pending_irq() : gr55xx_hal_cortex.h
- hal_nvic_get_priority() : gr55xx_hal_cortex.h
- hal_nvic_get_priority_grouping() : gr55xx_hal_cortex.h
- hal_nvic_set_pending_irq() : gr55xx_hal_cortex.h
- hal_nvic_set_priority() : gr55xx_hal_cortex.h
- hal_nvic_set_priority_grouping() : gr55xx_hal_cortex.h
- hal_nvic_system_reset() : gr55xx_hal_cortex.h
- HAL_OK : gr55xx_hal_def.h
- hal_pkc_big_number_add() : gr55xx_hal_pkc.h
- hal_pkc_big_number_add_it() : gr55xx_hal_pkc.h
- hal_pkc_big_number_multi() : gr55xx_hal_pkc.h
- hal_pkc_big_number_multi_it() : gr55xx_hal_pkc.h
- hal_pkc_callback_t : gr55xx_hal_pkc.h
- hal_pkc_deinit() : gr55xx_hal_pkc.h
- hal_pkc_done_callback() : gr55xx_hal_pkc.h
- hal_pkc_ecc_point_multi() : gr55xx_hal_pkc.h
- hal_pkc_ecc_point_multi_it() : gr55xx_hal_pkc.h
- hal_pkc_error_callback() : gr55xx_hal_pkc.h
- HAL_PKC_ERROR_INVALID_PARAM : gr55xx_hal_pkc.h
- HAL_PKC_ERROR_INVERSE_K : gr55xx_hal_pkc.h
- HAL_PKC_ERROR_IRREVERSIBLE : gr55xx_hal_pkc.h
- HAL_PKC_ERROR_NONE : gr55xx_hal_pkc.h
- HAL_PKC_ERROR_OVERFLOW : gr55xx_hal_pkc.h
- HAL_PKC_ERROR_TIMEOUT : gr55xx_hal_pkc.h
- HAL_PKC_ERROR_TRANSFER : gr55xx_hal_pkc.h
- hal_pkc_get_error() : gr55xx_hal_pkc.h
- hal_pkc_get_state() : gr55xx_hal_pkc.h
- hal_pkc_init() : gr55xx_hal_pkc.h
- hal_pkc_irq_handler() : gr55xx_hal_pkc.h
- hal_pkc_modular_add() : gr55xx_hal_pkc.h
- hal_pkc_modular_add_it() : gr55xx_hal_pkc.h
- hal_pkc_modular_compare() : gr55xx_hal_pkc.h
- hal_pkc_modular_compare_it() : gr55xx_hal_pkc.h
- hal_pkc_modular_left_shift() : gr55xx_hal_pkc.h
- hal_pkc_modular_left_shift_it() : gr55xx_hal_pkc.h
- hal_pkc_modular_sub() : gr55xx_hal_pkc.h
- hal_pkc_modular_sub_it() : gr55xx_hal_pkc.h
- HAL_PKC_MODULE_ENABLED : gr55xx_hal_conf.h
- hal_pkc_montgomery_inversion() : gr55xx_hal_pkc.h
- hal_pkc_montgomery_inversion_it() : gr55xx_hal_pkc.h
- hal_pkc_montgomery_multi() : gr55xx_hal_pkc.h
- hal_pkc_montgomery_multi_it() : gr55xx_hal_pkc.h
- hal_pkc_msp_deinit() : gr55xx_hal_pkc.h
- hal_pkc_msp_init() : gr55xx_hal_pkc.h
- hal_pkc_overflow_callback() : gr55xx_hal_pkc.h
- hal_pkc_resume_reg() : gr55xx_hal_pkc.h
- hal_pkc_rsa_modular_exponent() : gr55xx_hal_pkc.h
- hal_pkc_set_timeout() : gr55xx_hal_pkc.h
- HAL_PKC_STATE_BUSY : gr55xx_hal_pkc.h
- HAL_PKC_STATE_ERROR : gr55xx_hal_pkc.h
- HAL_PKC_STATE_READY : gr55xx_hal_pkc.h
- HAL_PKC_STATE_RESET : gr55xx_hal_pkc.h
- hal_pkc_state_t : gr55xx_hal_pkc.h
- HAL_PKC_STATE_TIMEOUT : gr55xx_hal_pkc.h
- hal_pkc_suspend_reg() : gr55xx_hal_pkc.h
- HAL_PKC_TIMEOUT_DEFAULT_VALUE : gr55xx_hal_pkc.h
- HAL_PWM_ACTIVE_CHANNEL_A : gr55xx_hal_pwm.h
- HAL_PWM_ACTIVE_CHANNEL_ALL : gr55xx_hal_pwm.h
- HAL_PWM_ACTIVE_CHANNEL_B : gr55xx_hal_pwm.h
- HAL_PWM_ACTIVE_CHANNEL_C : gr55xx_hal_pwm.h
- HAL_PWM_ACTIVE_CHANNEL_CLEARED : gr55xx_hal_pwm.h
- hal_pwm_active_channel_t : gr55xx_hal_pwm.h
- hal_pwm_callback_t : gr55xx_hal_pwm.h
- hal_pwm_config_channel() : gr55xx_hal_pwm.h
- hal_pwm_deinit() : gr55xx_hal_pwm.h
- hal_pwm_get_state() : gr55xx_hal_pwm.h
- hal_pwm_init() : gr55xx_hal_pwm.h
- HAL_PWM_MODULE_ENABLED : gr55xx_hal_conf.h
- hal_pwm_msp_deinit() : gr55xx_hal_pwm.h
- hal_pwm_msp_init() : gr55xx_hal_pwm.h
- hal_pwm_resume_reg() : gr55xx_hal_pwm.h
- hal_pwm_start() : gr55xx_hal_pwm.h
- HAL_PWM_STATE_BUSY : gr55xx_hal_pwm.h
- HAL_PWM_STATE_ERROR : gr55xx_hal_pwm.h
- HAL_PWM_STATE_READY : gr55xx_hal_pwm.h
- HAL_PWM_STATE_RESET : gr55xx_hal_pwm.h
- hal_pwm_state_t : gr55xx_hal_pwm.h
- hal_pwm_stop() : gr55xx_hal_pwm.h
- hal_pwm_suspend_reg() : gr55xx_hal_pwm.h
- hal_pwm_update_freq() : gr55xx_hal_pwm.h
- hal_pwr_config_ext_wakeup() : gr55xx_hal_pwr.h
- hal_pwr_config_timer_wakeup() : gr55xx_hal_pwr.h
- hal_pwr_disable_ext_wakeup() : gr55xx_hal_pwr.h
- hal_pwr_enter_chip_deepsleep() : gr55xx_hal_pwr.h
- hal_pwr_get_timer_current_value() : gr55xx_hal_pwr.h
- hal_pwr_handler_t : gr55xx_hal_pwr.h
- HAL_PWR_MODULE_ENABLED : gr55xx_hal_conf.h
- hal_pwr_set_comm_mode() : gr55xx_hal_pwr.h
- hal_pwr_set_comm_power() : gr55xx_hal_pwr.h
- hal_pwr_set_wakeup_condition() : gr55xx_hal_pwr.h
- hal_pwr_sleep_timer_elapsed_callback() : gr55xx_hal_pwr.h
- hal_pwr_sleep_timer_irq_handler() : gr55xx_hal_pwr.h
- HAL_PWR_TIMEOUT_DEFAULT_VALUE : gr55xx_hal_pwr.h
- hal_qspi_abort() : gr55xx_hal_qspi.h
- hal_qspi_abort_cplt_callback() : gr55xx_hal_qspi.h
- hal_qspi_abort_it() : gr55xx_hal_qspi.h
- hal_qspi_callback_t : gr55xx_hal_qspi.h
- hal_qspi_command() : gr55xx_hal_qspi.h
- hal_qspi_command_dma() : gr55xx_hal_qspi.h
- hal_qspi_command_it() : gr55xx_hal_qspi.h
- hal_qspi_command_receive() : gr55xx_hal_qspi.h
- hal_qspi_command_receive_dma() : gr55xx_hal_qspi.h
- hal_qspi_command_receive_it() : gr55xx_hal_qspi.h
- hal_qspi_command_transmit() : gr55xx_hal_qspi.h
- hal_qspi_command_transmit_dma() : gr55xx_hal_qspi.h
- hal_qspi_command_transmit_it() : gr55xx_hal_qspi.h
- hal_qspi_deinit() : gr55xx_hal_qspi.h
- hal_qspi_error_callback() : gr55xx_hal_qspi.h
- HAL_QSPI_ERROR_DMA : gr55xx_hal_qspi.h
- HAL_QSPI_ERROR_INVALID_PARAM : gr55xx_hal_qspi.h
- HAL_QSPI_ERROR_NONE : gr55xx_hal_qspi.h
- HAL_QSPI_ERROR_TIMEOUT : gr55xx_hal_qspi.h
- HAL_QSPI_ERROR_TRANSFER : gr55xx_hal_qspi.h
- hal_qspi_fifo_threshold_callback() : gr55xx_hal_qspi.h
- hal_qspi_get_error() : gr55xx_hal_qspi.h
- hal_qspi_get_rx_fifo_threshold() : gr55xx_hal_qspi.h
- hal_qspi_get_state() : gr55xx_hal_qspi.h
- hal_qspi_get_tx_fifo_threshold() : gr55xx_hal_qspi.h
- hal_qspi_init() : gr55xx_hal_qspi.h
- hal_qspi_irq_handler() : gr55xx_hal_qspi.h
- HAL_QSPI_MODULE_ENABLED : gr55xx_hal_conf.h
- hal_qspi_msp_deinit() : gr55xx_hal_qspi.h
- hal_qspi_msp_init() : gr55xx_hal_qspi.h
- hal_qspi_receive() : gr55xx_hal_qspi.h
- hal_qspi_receive_dma() : gr55xx_hal_qspi.h
- hal_qspi_receive_it() : gr55xx_hal_qspi.h
- hal_qspi_resume_reg() : gr55xx_hal_qspi.h
- hal_qspi_rx_cplt_callback() : gr55xx_hal_qspi.h
- hal_qspi_set_rx_fifo_threshold() : gr55xx_hal_qspi.h
- hal_qspi_set_timeout() : gr55xx_hal_qspi.h
- hal_qspi_set_tx_fifo_threshold() : gr55xx_hal_qspi.h
- HAL_QSPI_STATE_ABORT : gr55xx_hal_qspi.h
- HAL_QSPI_STATE_BUSY : gr55xx_hal_qspi.h
- HAL_QSPI_STATE_BUSY_INDIRECT_RX : gr55xx_hal_qspi.h
- HAL_QSPI_STATE_BUSY_INDIRECT_TX : gr55xx_hal_qspi.h
- HAL_QSPI_STATE_ERROR : gr55xx_hal_qspi.h
- HAL_QSPI_STATE_READY : gr55xx_hal_qspi.h
- HAL_QSPI_STATE_RESET : gr55xx_hal_qspi.h
- hal_qspi_state_t : gr55xx_hal_qspi.h
- hal_qspi_suspend_reg() : gr55xx_hal_qspi.h
- HAL_QSPI_TIMEOUT_DEFAULT_VALUE : gr55xx_hal_qspi.h
- hal_qspi_transmit() : gr55xx_hal_qspi.h
- hal_qspi_transmit_dma() : gr55xx_hal_qspi.h
- hal_qspi_transmit_it() : gr55xx_hal_qspi.h
- hal_qspi_tx_cplt_callback() : gr55xx_hal_qspi.h
- hal_resume_tick() : gr55xx_hal.h
- hal_rng_callback_t : gr55xx_hal_rng.h
- hal_rng_deinit() : gr55xx_hal_rng.h
- hal_rng_generate_random_number() : gr55xx_hal_rng.h
- hal_rng_generate_random_number_it() : gr55xx_hal_rng.h
- hal_rng_get_state() : gr55xx_hal_rng.h
- hal_rng_init() : gr55xx_hal_rng.h
- hal_rng_irq_handler() : gr55xx_hal_rng.h
- HAL_RNG_MODULE_ENABLED : gr55xx_hal_conf.h
- hal_rng_msp_deinit() : gr55xx_hal_rng.h
- hal_rng_msp_init() : gr55xx_hal_rng.h
- hal_rng_read_last_random_number() : gr55xx_hal_rng.h
- hal_rng_ready_data_callback() : gr55xx_hal_rng.h
- hal_rng_resume_reg() : gr55xx_hal_rng.h
- HAL_RNG_STATE_BUSY : gr55xx_hal_rng.h
- HAL_RNG_STATE_ERROR : gr55xx_hal_rng.h
- HAL_RNG_STATE_READY : gr55xx_hal_rng.h
- HAL_RNG_STATE_RESET : gr55xx_hal_rng.h
- hal_rng_state_t : gr55xx_hal_rng.h
- HAL_RNG_STATE_TIMEOUT : gr55xx_hal_rng.h
- hal_rng_suspend_reg() : gr55xx_hal_rng.h
- hal_sleep_timer_config_and_start() : gr55xx_hal_sleep_timer.h
- hal_sleep_timer_get_clock_freq() : gr55xx_hal_sleep_timer.h
- hal_sleep_timer_get_current_value() : gr55xx_hal_sleep_timer.h
- HAL_SLEEP_TIMER_MODULE_ENABLED : gr55xx_hal_conf.h
- hal_sleep_timer_status_get() : gr55xx_hal_sleep_timer.h
- hal_sleep_timer_stop() : gr55xx_hal_sleep_timer.h
- hal_spi_abort() : gr55xx_hal_spi.h
- hal_spi_abort_cplt_callback() : gr55xx_hal_spi.h
- hal_spi_abort_it() : gr55xx_hal_spi.h
- hal_spi_callback_t : gr55xx_hal_spi.h
- hal_spi_deinit() : gr55xx_hal_spi.h
- hal_spi_error_callback() : gr55xx_hal_spi.h
- HAL_SPI_ERROR_DMA : gr55xx_hal_spi.h
- HAL_SPI_ERROR_INVALID_PARAM : gr55xx_hal_spi.h
- HAL_SPI_ERROR_NONE : gr55xx_hal_spi.h
- HAL_SPI_ERROR_TIMEOUT : gr55xx_hal_spi.h
- HAL_SPI_ERROR_TRANSFER : gr55xx_hal_spi.h
- hal_spi_get_error() : gr55xx_hal_spi.h
- hal_spi_get_rx_fifo_threshold() : gr55xx_hal_spi.h
- hal_spi_get_state() : gr55xx_hal_spi.h
- hal_spi_get_tx_fifo_threshold() : gr55xx_hal_spi.h
- hal_spi_init() : gr55xx_hal_spi.h
- hal_spi_irq_handler() : gr55xx_hal_spi.h
- HAL_SPI_MODULE_ENABLED : gr55xx_hal_conf.h
- hal_spi_msp_deinit() : gr55xx_hal_spi.h
- hal_spi_msp_init() : gr55xx_hal_spi.h
- hal_spi_read_eeprom() : gr55xx_hal_spi.h
- hal_spi_read_eeprom_dma() : gr55xx_hal_spi.h
- hal_spi_read_eeprom_it() : gr55xx_hal_spi.h
- hal_spi_receive() : gr55xx_hal_spi.h
- hal_spi_receive_dma() : gr55xx_hal_spi.h
- hal_spi_receive_it() : gr55xx_hal_spi.h
- hal_spi_resume_reg() : gr55xx_hal_spi.h
- hal_spi_rx_cplt_callback() : gr55xx_hal_spi.h
- hal_spi_set_rx_fifo_threshold() : gr55xx_hal_spi.h
- hal_spi_set_timeout() : gr55xx_hal_spi.h
- hal_spi_set_tx_fifo_threshold() : gr55xx_hal_spi.h
- HAL_SPI_STATE_ABORT : gr55xx_hal_spi.h
- HAL_SPI_STATE_BUSY : gr55xx_hal_spi.h
- HAL_SPI_STATE_BUSY_RX : gr55xx_hal_spi.h
- HAL_SPI_STATE_BUSY_TX : gr55xx_hal_spi.h
- HAL_SPI_STATE_BUSY_TX_RX : gr55xx_hal_spi.h
- HAL_SPI_STATE_ERROR : gr55xx_hal_spi.h
- HAL_SPI_STATE_READY : gr55xx_hal_spi.h
- HAL_SPI_STATE_RESET : gr55xx_hal_spi.h
- hal_spi_state_t : gr55xx_hal_spi.h
- hal_spi_suspend_reg() : gr55xx_hal_spi.h
- HAL_SPI_TIMEOUT_DEFAULT_VALUE : gr55xx_hal_spi.h
- hal_spi_transmit() : gr55xx_hal_spi.h
- hal_spi_transmit_dma() : gr55xx_hal_spi.h
- hal_spi_transmit_dma_with_ia() : gr55xx_hal_spi.h
- hal_spi_transmit_it() : gr55xx_hal_spi.h
- hal_spi_transmit_receive() : gr55xx_hal_spi.h
- hal_spi_transmit_receive_dma() : gr55xx_hal_spi.h
- hal_spi_transmit_receive_it() : gr55xx_hal_spi.h
- hal_spi_transmit_with_ia() : gr55xx_hal_spi.h
- hal_spi_tx_cplt_callback() : gr55xx_hal_spi.h
- hal_spi_tx_rx_cplt_callback() : gr55xx_hal_spi.h
- hal_spi_v2_abort() : gr55xx_hal_spi_v2.h
- hal_spi_v2_abort_cplt_callback() : gr55xx_hal_spi_v2.h
- hal_spi_v2_abort_it() : gr55xx_hal_spi_v2.h
- hal_spi_v2_deinit() : gr55xx_hal_spi_v2.h
- hal_spi_v2_error_callback() : gr55xx_hal_spi_v2.h
- hal_spi_v2_get_error() : gr55xx_hal_spi_v2.h
- hal_spi_v2_get_rx_fifo_threshold() : gr55xx_hal_spi_v2.h
- hal_spi_v2_get_state() : gr55xx_hal_spi_v2.h
- hal_spi_v2_get_tx_fifo_threshold() : gr55xx_hal_spi_v2.h
- hal_spi_v2_init() : gr55xx_hal_spi_v2.h
- hal_spi_v2_irq_handler() : gr55xx_hal_spi_v2.h
- hal_spi_v2_msp_deinit() : gr55xx_hal_spi_v2.h
- hal_spi_v2_msp_init() : gr55xx_hal_spi_v2.h
- hal_spi_v2_receive_32bit() : gr55xx_hal_spi_v2.h
- hal_spi_v2_receive_32bit_dma() : gr55xx_hal_spi_v2.h
- hal_spi_v2_receive_8bit() : gr55xx_hal_spi_v2.h
- hal_spi_v2_receive_8bit_dma() : gr55xx_hal_spi_v2.h
- hal_spi_v2_resume_reg() : gr55xx_hal_spi_v2.h
- hal_spi_v2_rx_cplt_callback() : gr55xx_hal_spi_v2.h
- hal_spi_v2_set_rx_delay() : gr55xx_hal_spi_v2.h
- hal_spi_v2_set_timeout() : gr55xx_hal_spi_v2.h
- hal_spi_v2_suspend_reg() : gr55xx_hal_spi_v2.h
- hal_spi_v2_transmit_32bit() : gr55xx_hal_spi_v2.h
- hal_spi_v2_transmit_32bit_dma() : gr55xx_hal_spi_v2.h
- hal_spi_v2_transmit_8bit() : gr55xx_hal_spi_v2.h
- hal_spi_v2_transmit_8bit_dma() : gr55xx_hal_spi_v2.h
- hal_spi_v2_transmit_8bit_toggle() : gr55xx_hal_spi_v2.h
- hal_spi_v2_transmit_dma_with_toggle() : gr55xx_hal_spi_v2.h
- hal_spi_v2_transmit_receive_8bit() : gr55xx_hal_spi_v2.h
- hal_spi_v2_tx_cplt_callback() : gr55xx_hal_spi_v2.h
- hal_spi_v2_tx_rx_cplt_callback() : gr55xx_hal_spi_v2.h
- hal_status_t : gr55xx_hal_def.h
- hal_suspend_tick() : gr55xx_hal.h
- hal_systick_callback() : gr55xx_hal_cortex.h
- hal_systick_clk_source_config() : gr55xx_hal_cortex.h
- hal_systick_config() : gr55xx_hal_cortex.h
- hal_systick_irq_handler() : gr55xx_hal_cortex.h
- HAL_TIMEOUT : gr55xx_hal_def.h
- HAL_TIMEOUT_DEINIT : gr55xx_delay.h
- HAL_TIMEOUT_INIT : gr55xx_delay.h
- hal_timer_base_deinit() : gr55xx_hal_tim.h
- hal_timer_base_init() : gr55xx_hal_tim.h
- hal_timer_base_msp_deinit() : gr55xx_hal_tim.h
- hal_timer_base_msp_init() : gr55xx_hal_tim.h
- hal_timer_base_start() : gr55xx_hal_tim.h
- hal_timer_base_start_it() : gr55xx_hal_tim.h
- hal_timer_base_stop() : gr55xx_hal_tim.h
- hal_timer_base_stop_it() : gr55xx_hal_tim.h
- hal_timer_callback_t : gr55xx_hal_tim.h
- hal_timer_get_state() : gr55xx_hal_tim.h
- hal_timer_irq_handler() : gr55xx_hal_tim.h
- HAL_TIMER_MODULE_ENABLED : gr55xx_hal_conf.h
- hal_timer_period_elapsed_callback() : gr55xx_hal_tim.h
- hal_timer_set_config() : gr55xx_hal_tim.h
- HAL_TIMER_STATE_BUSY : gr55xx_hal_tim.h
- HAL_TIMER_STATE_ERROR : gr55xx_hal_tim.h
- HAL_TIMER_STATE_READY : gr55xx_hal_tim.h
- HAL_TIMER_STATE_RESET : gr55xx_hal_tim.h
- hal_timer_state_t : gr55xx_hal_tim.h
- hal_uart_abort() : gr55xx_hal_uart.h
- hal_uart_abort_cplt_callback() : gr55xx_hal_uart.h
- hal_uart_abort_it() : gr55xx_hal_uart.h
- hal_uart_abort_receive() : gr55xx_hal_uart.h
- hal_uart_abort_receive_it() : gr55xx_hal_uart.h
- hal_uart_abort_rx_cplt_callback() : gr55xx_hal_uart.h
- hal_uart_abort_transmit() : gr55xx_hal_uart.h
- hal_uart_abort_transmit_it() : gr55xx_hal_uart.h
- hal_uart_abort_tx_cplt_callback() : gr55xx_hal_uart.h
- hal_uart_callback_t : gr55xx_hal_uart.h
- hal_uart_deinit() : gr55xx_hal_uart.h
- hal_uart_dma_pause() : gr55xx_hal_uart.h
- hal_uart_dma_resume() : gr55xx_hal_uart.h
- hal_uart_dma_stop() : gr55xx_hal_uart.h
- HAL_UART_ERROR_BI : gr55xx_hal_uart.h
- HAL_UART_ERROR_BUSY : gr55xx_hal_uart.h
- hal_uart_error_callback() : gr55xx_hal_uart.h
- HAL_UART_ERROR_DMA : gr55xx_hal_uart.h
- HAL_UART_ERROR_FE : gr55xx_hal_uart.h
- HAL_UART_ERROR_NONE : gr55xx_hal_uart.h
- HAL_UART_ERROR_OE : gr55xx_hal_uart.h
- HAL_UART_ERROR_PE : gr55xx_hal_uart.h
- hal_uart_get_error() : gr55xx_hal_uart.h
- hal_uart_get_state() : gr55xx_hal_uart.h
- hal_uart_init() : gr55xx_hal_uart.h
- hal_uart_irq_handler() : gr55xx_hal_uart.h
- HAL_UART_MODULE_ENABLED : gr55xx_hal_conf.h
- hal_uart_msp_deinit() : gr55xx_hal_uart.h
- hal_uart_msp_init() : gr55xx_hal_uart.h
- hal_uart_receive() : gr55xx_hal_uart.h
- hal_uart_receive_dma() : gr55xx_hal_uart.h
- hal_uart_receive_it() : gr55xx_hal_uart.h
- hal_uart_resume_reg() : gr55xx_hal_uart.h
- hal_uart_rx_cplt_callback() : gr55xx_hal_uart.h
- HAL_UART_STATE_BUSY : gr55xx_hal_uart.h
- HAL_UART_STATE_BUSY_RX : gr55xx_hal_uart.h
- HAL_UART_STATE_BUSY_TX : gr55xx_hal_uart.h
- HAL_UART_STATE_BUSY_TXRX : gr55xx_hal_uart.h
- HAL_UART_STATE_ERROR : gr55xx_hal_uart.h
- HAL_UART_STATE_READY : gr55xx_hal_uart.h
- HAL_UART_STATE_RESET : gr55xx_hal_uart.h
- hal_uart_state_t : gr55xx_hal_uart.h
- HAL_UART_STATE_TIMEOUT : gr55xx_hal_uart.h
- hal_uart_suspend_reg() : gr55xx_hal_uart.h
- HAL_UART_TIMEOUT_DEFAULT_VALUE : gr55xx_hal_uart.h
- hal_uart_transmit() : gr55xx_hal_uart.h
- hal_uart_transmit_dma() : gr55xx_hal_uart.h
- hal_uart_transmit_it() : gr55xx_hal_uart.h
- hal_uart_tx_cplt_callback() : gr55xx_hal_uart.h
- HAL_UNLOCKED : gr55xx_hal_def.h
- hal_wdt_callback_t : gr55xx_hal_wdt.h
- hal_wdt_deinit() : gr55xx_hal_wdt.h
- hal_wdt_init() : gr55xx_hal_wdt.h
- hal_wdt_irq_handler() : gr55xx_hal_wdt.h
- HAL_WDT_MODULE_ENABLED : gr55xx_hal_conf.h
- hal_wdt_msp_deinit() : gr55xx_hal_wdt.h
- hal_wdt_msp_init() : gr55xx_hal_wdt.h
- hal_wdt_period_elapsed_callback() : gr55xx_hal_wdt.h
- hal_wdt_refresh() : gr55xx_hal_wdt.h
- hal_xqspi_callback_t : gr55xx_hal_xqspi.h
- hal_xqspi_command_receive() : gr55xx_hal_xqspi.h
- hal_xqspi_command_transmit() : gr55xx_hal_xqspi.h
- hal_xqspi_deinit() : gr55xx_hal_xqspi.h
- HAL_XQSPI_ERROR_INVALID_PARAM : gr55xx_hal_xqspi.h
- HAL_XQSPI_ERROR_NONE : gr55xx_hal_xqspi.h
- HAL_XQSPI_ERROR_TIMEOUT : gr55xx_hal_xqspi.h
- HAL_XQSPI_ERROR_TRANSFER : gr55xx_hal_xqspi.h
- hal_xqspi_get_error() : gr55xx_hal_xqspi.h
- hal_xqspi_get_rx_fifo_threshold() : gr55xx_hal_xqspi.h
- hal_xqspi_get_state() : gr55xx_hal_xqspi.h
- hal_xqspi_get_tx_fifo_threshold() : gr55xx_hal_xqspi.h
- hal_xqspi_init() : gr55xx_hal_xqspi.h
- HAL_XQSPI_MODULE_ENABLED : gr55xx_hal_conf.h
- hal_xqspi_msp_deinit() : gr55xx_hal_xqspi.h
- hal_xqspi_msp_init() : gr55xx_hal_xqspi.h
- hal_xqspi_receive() : gr55xx_hal_xqspi.h
- HAL_XQSPI_RETRY_DEFAULT_VALUE : gr55xx_hal_xqspi.h
- hal_xqspi_set_retry() : gr55xx_hal_xqspi.h
- hal_xqspi_set_rx_fifo_threshold() : gr55xx_hal_xqspi.h
- hal_xqspi_set_tx_fifo_threshold() : gr55xx_hal_xqspi.h
- hal_xqspi_set_xip_present_status() : gr55xx_hal_xqspi.h
- HAL_XQSPI_STATE_ABORT : gr55xx_hal_xqspi.h
- HAL_XQSPI_STATE_BUSY : gr55xx_hal_xqspi.h
- HAL_XQSPI_STATE_BUSY_INDIRECT_RX : gr55xx_hal_xqspi.h
- HAL_XQSPI_STATE_BUSY_INDIRECT_TX : gr55xx_hal_xqspi.h
- HAL_XQSPI_STATE_ERROR : gr55xx_hal_xqspi.h
- HAL_XQSPI_STATE_READY : gr55xx_hal_xqspi.h
- HAL_XQSPI_STATE_RESET : gr55xx_hal_xqspi.h
- hal_xqspi_state_t : gr55xx_hal_xqspi.h
- hal_xqspi_transmit() : gr55xx_hal_xqspi.h
- HID_INFO_FLAG_NORMALLY_CONNECTABLE_MSK : hids.h
- HID_INFO_FLAG_REMOTE_WAKE_MSK : hids.h
- hids_boot_kb_in_rep_send() : hids.h
- hids_boot_mouse_in_rep_send() : hids.h
- HIDS_CONNECTION_MAX : hids.h
- HIDS_EVT_BOOT_MODE_ENTERED : hids.h
- hids_evt_handler_t : hids.h
- HIDS_EVT_HOST_EXIT_SUSP : hids.h
- HIDS_EVT_HOST_SUSP : hids.h
- HIDS_EVT_IN_REP_NOTIFY_DISABLED : hids.h
- HIDS_EVT_IN_REP_NOTIFY_ENABLED : hids.h
- HIDS_EVT_INVALID : hids.h
- HIDS_EVT_REP_CHAR_WRITE : hids.h
- HIDS_EVT_REPORT_MODE_ENTERED : hids.h
- hids_evt_type_t : hids.h
- hids_input_rep_send() : hids.h
- HIDS_REP_TYPE_FEATURE : hids.h
- HIDS_REP_TYPE_INPUT : hids.h
- HIDS_REP_TYPE_OUTPUT : hids.h
- HIDS_REPORT_MAP_MAX_SIZE : hids.h
- HIDS_REPORT_MAX_SIZE : hids.h
- HIDS_REPORT_TYPE_FEATURE : hids.h
- HIDS_REPORT_TYPE_IN1 : hids.h
- HIDS_REPORT_TYPE_IN2 : hids.h
- HIDS_REPORT_TYPE_IN3 : hids.h
- HIDS_REPORT_TYPE_KB_IN : hids.h
- HIDS_REPORT_TYPE_KB_OUT : hids.h
- HIDS_REPORT_TYPE_MOUSE_IN : hids.h
- HIDS_REPORT_TYPE_OUT : hids.h
- HIDS_REPORT_TYPE_RESERVED : hids.h
- hids_report_type_t : hids.h
- hids_service_init() : hids.h
- hids_service_start_handle_get() : hids.h
- HMAC_BLOCK_MAX : gr55xx_hal_hmac.h
- HMAC_BLOCKSIZE_BITS : gr55xx_hal_hmac.h
- HMAC_BLOCKSIZE_BYTES : gr55xx_hal_hmac.h
- HMAC_BLOCKSIZE_WORDS : gr55xx_hal_hmac.h
- HMAC_DIGESTSIZE_BITS : gr55xx_hal_hmac.h
- HMAC_DIGESTSIZE_BYTES : gr55xx_hal_hmac.h
- HMAC_DIGESTSIZE_WORDS : gr55xx_hal_hmac.h
- HMAC_DMA_BLOCK_MAX : gr55xx_hal_hmac.h
- HMAC_FLAG_DATAREADY_HMAC : gr55xx_hal_hmac.h
- HMAC_FLAG_DATAREADY_SHA : gr55xx_hal_hmac.h
- HMAC_FLAG_DMA_DONE : gr55xx_hal_hmac.h
- HMAC_FLAG_DMA_ERR : gr55xx_hal_hmac.h
- HMAC_FLAG_DMA_MESSAGEDONE : gr55xx_hal_hmac.h
- HMAC_FLAG_KEY_VALID : gr55xx_hal_hmac.h
- hmac_handle_t : gr55xx_hal_hmac.h
- hmac_init_t : gr55xx_hal_hmac.h
- HMAC_IT_DONE : gr55xx_hal_hmac.h
- HMAC_MODE_HMAC : gr55xx_hal_hmac.h
- HMAC_MODE_SHA : gr55xx_hal_hmac.h
- HRRCPS_CONNECTION_MAX : hrrcps.h
- HRRCPS_CTRL_PT_HRS_CONN_STA_REPORT : hrrcps.h
- HRRCPS_CTRL_PT_HRS_DISCONN : hrrcps.h
- HRRCPS_CTRL_PT_HRS_NTF_DISABLE : hrrcps.h
- HRRCPS_CTRL_PT_HRS_NTF_ENABLE : hrrcps.h
- HRRCPS_CTRL_PT_HRS_SEN_LOC_READ : hrrcps.h
- hrrcps_ctrl_pt_id_t : hrrcps.h
- HRRCPS_CTRL_PT_RSCS_CONN_STA_REPORT : hrrcps.h
- HRRCPS_CTRL_PT_RSCS_DISCONN : hrrcps.h
- HRRCPS_CTRL_PT_RSCS_NTF_DISABLE : hrrcps.h
- HRRCPS_CTRL_PT_RSCS_NTF_ENABLE : hrrcps.h
- HRRCPS_CTRL_PT_RSCS_SEN_LOC_READ : hrrcps.h
- HRRCPS_CTRL_PT_RSP_CODE : hrrcps.h
- hrrcps_ctrl_pt_rsp_send() : hrrcps.h
- HRRCPS_CTRL_PT_RSP_VAL_LEN : hrrcps.h
- HRRCPS_CTRL_PT_SCAN_HRS : hrrcps.h
- HRRCPS_CTRL_PT_SCAN_RSCS : hrrcps.h
- HRRCPS_CTRL_PT_VAL_LEN : hrrcps.h
- HRRCPS_EVT_CTRL_PT_IND_DISABLE : hrrcps.h
- HRRCPS_EVT_CTRL_PT_IND_ENABLE : hrrcps.h
- HRRCPS_EVT_DISABLE_HRS_NTF : hrrcps.h
- HRRCPS_EVT_DISABLE_RSCS_NTF : hrrcps.h
- HRRCPS_EVT_DISCONN_HRS_LINK : hrrcps.h
- HRRCPS_EVT_DISCONN_RSCS_LINK : hrrcps.h
- HRRCPS_EVT_ENABLE_HRS_NTF : hrrcps.h
- HRRCPS_EVT_ENABLE_RSCS_NTF : hrrcps.h
- hrrcps_evt_handler_t : hrrcps.h
- HRRCPS_EVT_HRS_SENSOR_LOC_READ : hrrcps.h
- HRRCPS_EVT_INVALID : hrrcps.h
- HRRCPS_EVT_RSCS_SENSOR_LOC_READ : hrrcps.h
- HRRCPS_EVT_SCAN_HRS : hrrcps.h
- HRRCPS_EVT_SCAN_RSCS : hrrcps.h
- hrrcps_evt_type_t : hrrcps.h
- HRRCPS_RSP_ID_ERROR : hrrcps.h
- HRRCPS_RSP_ID_OK : hrrcps.h
- hrrcps_rsp_id_t : hrrcps.h
- hrrcps_service_init() : hrrcps.h
- HRRCPS_SERVICE_UUID : hrrcps.h
- HRS_C_BIT_ENERGY_EXPENDED_STATUS : hrs_c.h
- HRS_C_BIT_INTERVAL : hrs_c.h
- HRS_C_BIT_RATE_FORMAT : hrs_c.h
- HRS_C_BIT_SENSOR_CONTACT_DETECTED : hrs_c.h
- HRS_C_BIT_SENSOR_CONTACT_SUPPORTED : hrs_c.h
- HRS_C_CONNECTION_MAX : hrs_c.h
- HRS_C_CTRL_POINT_ENERGY_EXP : hrs_c.h
- hrs_c_ctrl_point_set() : hrs_c.h
- hrs_c_disc_srvc_start() : hrs_c.h
- HRS_C_EVT_CTRL_POINT_SET : hrs_c.h
- HRS_C_EVT_DISCOVERY_COMPLETE : hrs_c.h
- HRS_C_EVT_DISCOVERY_FAIL : hrs_c.h
- hrs_c_evt_handler_t : hrs_c.h
- HRS_C_EVT_HR_MEAS_NTF_SET_SUCCESS : hrs_c.h
- HRS_C_EVT_HR_MEAS_VAL_RECEIVE : hrs_c.h
- HRS_C_EVT_INVALID : hrs_c.h
- HRS_C_EVT_SENSOR_LOC_READ_RSP : hrs_c.h
- hrs_c_evt_type_t : hrs_c.h
- HRS_C_EVT_WRITE_OP_ERR : hrs_c.h
- hrs_c_flag_bit_t : hrs_c.h
- hrs_c_heart_rate_meas_notify_set() : hrs_c.h
- HRS_C_RR_INTERVALS_NUM_MAX : hrs_c.h
- HRS_C_SENS_LOC_CHEST : hrs_c.h
- HRS_C_SENS_LOC_EARLOBE : hrs_c.h
- HRS_C_SENS_LOC_FINGER : hrs_c.h
- HRS_C_SENS_LOC_FOOT : hrs_c.h
- HRS_C_SENS_LOC_HAND : hrs_c.h
- HRS_C_SENS_LOC_OTHER : hrs_c.h
- HRS_C_SENS_LOC_WRIST : hrs_c.h
- hrs_c_sensor_loc_read() : hrs_c.h
- hrs_c_sensor_loc_t : hrs_c.h
- HRS_CHAR_BODY_SENSOR_LOC_SUP : hrs.h
- HRS_CHAR_ENGY_EXP_SUP : hrs.h
- HRS_CHAR_MANDATORY : hrs.h
- hrs_client_init() : hrs_c.h
- HRS_CONNECTION_MAX : hrs.h
- hrs_energy_update() : hrs.h
- hrs_evt_handler_t : hrs.h
- HRS_EVT_NOTIFICATION_DISABLED : hrs.h
- HRS_EVT_NOTIFICATION_ENABLED : hrs.h
- HRS_EVT_READ_BODY_SEN_LOCATION : hrs.h
- HRS_EVT_RESET_ENERGY_EXPENDED : hrs.h
- hrs_evt_type_t : hrs.h
- hrs_heart_rate_measurement_send() : hrs.h
- HRS_MAX_BUFFERED_RR_INTERVALS : hrs.h
- HRS_MEAS_MAX_LEN : hrs.h
- hrs_rr_interval_add() : hrs.h
- HRS_SENS_LOC_CHEST : hrs.h
- HRS_SENS_LOC_EARLOBE : hrs.h
- HRS_SENS_LOC_FINGER : hrs.h
- HRS_SENS_LOC_FOOT : hrs.h
- HRS_SENS_LOC_HAND : hrs.h
- HRS_SENS_LOC_OTHER : hrs.h
- HRS_SENS_LOC_WRIST : hrs.h
- hrs_sensor_contact_detected_update() : hrs.h
- hrs_sensor_contact_supported_set() : hrs.h
- hrs_sensor_loc_t : hrs.h
- hrs_sensor_location_set() : hrs.h
- hrs_service_init() : hrs.h
- hrs_service_start_handle_get() : hrs.h
- HTS_CHAR_FULL : hts.h
- HTS_CHAR_INTM_TEM_SUP : hts.h
- HTS_CHAR_MANDATORY : hts.h
- HTS_CHAR_MEAS_INTERVAL_SUP : hts.h
- HTS_CHAR_TEM_TYPE_SUP : hts.h
- HTS_CONNECTION_MAX : hts.h
- hts_date_time_t : hts.h
- hts_evt_handler_t : hts.h
- HTS_EVT_INTM_TEM_NOTIFICATION_DISABLE : hts.h
- HTS_EVT_INTM_TEM_NOTIFICATION_ENABLE : hts.h
- HTS_EVT_INVALID : hts.h
- HTS_EVT_MEAS_INTERVAL_INDICATION_DISABLE : hts.h
- HTS_EVT_MEAS_INTERVAL_UPDATE : hts.h
- HTS_EVT_MEAS_INTREVAL_INDICATION_ENABLE : hts.h
- HTS_EVT_READ_CHARACTERISTIC : hts.h
- HTS_EVT_TEM_MEAS_INDICATION_DISABLE : hts.h
- HTS_EVT_TEM_MEAS_INDICATION_ENABLE : hts.h
- hts_evt_type_t : hts.h
- hts_flag_bit_t : hts.h
- HTS_INTM_TEM_MAX_LEN : hts.h
- HTS_MEAS_FLAG_TEM_TYPE_BIT : hts.h
- HTS_MEAS_FLAG_TEM_UINTS_BIT : hts.h
- HTS_MEAS_FLAG_TIME_STAMP_BIT : hts.h
- HTS_MEAS_INTERVAL_MAX_LEN : hts.h
- HTS_MEAS_INTV_DFLT_MAX : hts.h
- HTS_MEAS_INTV_DFLT_MIN : hts.h
- hts_measurement_interval_send() : hts.h
- hts_measurement_send() : hts.h
- HTS_READ_CHAR_MEAS_INTL : hts.h
- HTS_READ_CHAR_TEMP_TYPE : hts.h
- hts_read_characteristic_t : hts.h
- hts_service_init() : hts.h
- HTS_TEM_MEAS_MAX_LEN : hts.h
- HTS_TEM_TYPE_MAX_LEN : hts.h
- hts_temp_meas_loc_t : hts.h
- hts_temp_meas_type_t : hts.h
- HTS_TEMP_TYPE_ARMPIT : hts.h
- HTS_TEMP_TYPE_BODY : hts.h
- HTS_TEMP_TYPE_EAR : hts.h
- HTS_TEMP_TYPE_EAR_DRUM : hts.h
- HTS_TEMP_TYPE_FINGER : hts.h
- HTS_TEMP_TYPE_GI_TRACT : hts.h
- HTS_TEMP_TYPE_MOUTH : hts.h
- HTS_TEMP_TYPE_RECTUM : hts.h
- HTS_TEMP_TYPE_TOE : hts.h
- hts_temp_unit_t : hts.h
- HTS_TEMPERATURE_CELCIUS : hts.h
- HTS_TEMPERATURE_FAHRENHEIT : hts.h
- HTS_TEMPERATURE_INTERMEDIATE : hts.h
- HTS_TEMPERATURE_STABLE : hts.h