Public Attributes | List of all members
rscs_c_meas_val_t Struct Reference
BLE Services » Running Speed and Cadence Service Client (RSCS_C) » Structures

Running Speed and Cadence Measurement Character value structure. More...

`#include <rscs_c.h>`

## Public Attributes
bool | inst_stride_length_present
| If Instantaneous Stride Length is present. More...
bool | total_distance_present
| If Total Distance is present. More...
bool | is_run_or_walk
| True: Running, False: Walking. More...
uint16_t | inst_speed
| Instantaneous Speed. More...
uint8_t | inst_cadence
| Instantaneous Cadence. More...
uint16_t | inst_stride_length
| Instantaneous Stride Length. More...
uint32_t | total_distance
| Total Distance. More...

## Detailed Description

Running Speed and Cadence Measurement Character value structure.

Definition at line 161 of file rscs_c.h.

## Member Data Documentation

## ◆ inst_cadence

uint8_t rscs_c_meas_val_t::inst_cadence

Instantaneous Cadence.

Definition at line 167 of file rscs_c.h.

## ◆ inst_speed

uint16_t rscs_c_meas_val_t::inst_speed

Instantaneous Speed.

Definition at line 166 of file rscs_c.h.

## ◆ inst_stride_length

uint16_t rscs_c_meas_val_t::inst_stride_length

Instantaneous Stride Length.

Definition at line 168 of file rscs_c.h.

## ◆ inst_stride_length_present

bool rscs_c_meas_val_t::inst_stride_length_present

If Instantaneous Stride Length is present.

Definition at line 163 of file rscs_c.h.

## ◆ is_run_or_walk

bool rscs_c_meas_val_t::is_run_or_walk

True: Running, False: Walking.

Definition at line 165 of file rscs_c.h.

## ◆ total_distance

uint32_t rscs_c_meas_val_t::total_distance

Total Distance.

Definition at line 169 of file rscs_c.h.

## ◆ total_distance_present

bool rscs_c_meas_val_t::total_distance_present

If Total Distance is present.

Definition at line 164 of file rscs_c.h.

The documentation for this struct was generated from the following file:

- rscs_c.h