Macros
XQSPI FIFO Threshold, FIFO depth is 64*4bytes, only in QSPI mode
Peripheral Driver » HAL Driver » XQSPI » Defines » XQSPI Exported Constants
Collaboration diagram for XQSPI FIFO Threshold, FIFO depth is 64*4bytes, only in QSPI mode:

## Macros
#define | XQSPI_FIFO_THRESHOLD_1_8 LL_XQSPI_QSPI_FIFO_WATERMARK_1_8
| FIFO depth/8 More...
#define | XQSPI_FIFO_THRESHOLD_1_4 LL_XQSPI_QSPI_FIFO_WATERMARK_1_4
| FIFO depth/4 More...
#define | XQSPI_FIFO_THRESHOLD_1_2 LL_XQSPI_QSPI_FIFO_WATERMARK_1_2
| FIFO depth/2 More...
#define | XQSPI_FIFO_THRESHOLD_3_4 LL_XQSPI_QSPI_FIFO_WATERMARK_3_4
| FIFO depth*3/4 More...
#define | XQSPI_FIFO_DEPTH LL_XQSPI_QSPI_FIFO_DEPTH
| FIFO full depth More...

## Detailed Description

## Macro Definition Documentation

## ◆ XQSPI_FIFO_DEPTH

#define XQSPI_FIFO_DEPTH LL_XQSPI_QSPI_FIFO_DEPTH

FIFO full depth

Definition at line 301 of file gr55xx_hal_xqspi.h.

## ◆ XQSPI_FIFO_THRESHOLD_1_2

#define XQSPI_FIFO_THRESHOLD_1_2 LL_XQSPI_QSPI_FIFO_WATERMARK_1_2

FIFO depth/2

Definition at line 299 of file gr55xx_hal_xqspi.h.

## ◆ XQSPI_FIFO_THRESHOLD_1_4

#define XQSPI_FIFO_THRESHOLD_1_4 LL_XQSPI_QSPI_FIFO_WATERMARK_1_4

FIFO depth/4

Definition at line 298 of file gr55xx_hal_xqspi.h.

## ◆ XQSPI_FIFO_THRESHOLD_1_8

#define XQSPI_FIFO_THRESHOLD_1_8 LL_XQSPI_QSPI_FIFO_WATERMARK_1_8

FIFO depth/8

Definition at line 297 of file gr55xx_hal_xqspi.h.

## ◆ XQSPI_FIFO_THRESHOLD_3_4

#define XQSPI_FIFO_THRESHOLD_3_4 LL_XQSPI_QSPI_FIFO_WATERMARK_3_4

FIFO depth*3/4

Definition at line 300 of file gr55xx_hal_xqspi.h.