Macros
Get Flags Defines
Peripheral Driver » LL Driver » I2C » Defines » I2C Exported Constants

Flags definitions which can be used with LL_I2C_ReadReg function. More...

Collaboration diagram for Get Flags Defines:

## Macros
#define | LL_I2C_INTR_STAT_MST_ON_HOLD I2C_INTR_GEN_CALL
| MST_ON_HOLD interrupt flag. More...
#define | LL_I2C_INTR_STAT_RESTART_DET I2C_INTR_RESTART_DET
| RESTART_DET interrupt flag. More...
#define | LL_I2C_INTR_STAT_GEN_CALL I2C_INTR_GEN_CALL
| GEN_CALL interrupt flag. More...
#define | LL_I2C_INTR_STAT_START_DET I2C_INTR_START_DET
| START_DET interrupt flag. More...
#define | LL_I2C_INTR_STAT_STOP_DET I2C_INTR_STOP_DET
| STOP_DET interrupt flag. More...
#define | LL_I2C_INTR_STAT_ACTIVITY I2C_INTR_ACTIVITY
| ACTIVITY interrupt flag. More...
#define | LL_I2C_INTR_STAT_RX_DONE I2C_INTR_RX_DONE
| RX_DONE interrupt flag. More...
#define | LL_I2C_INTR_STAT_TX_ABRT I2C_INTR_TX_ABRT
| TX_ABRT interrupt flag. More...
#define | LL_I2C_INTR_STAT_RD_REQ I2C_INTR_RD_REQ
| RD_REQ interrupt flag. More...
#define | LL_I2C_INTR_STAT_TX_EMPTY I2C_INTR_TX_EMPTY
| TX_EMPTY interrupt flag. More...
#define | LL_I2C_INTR_STAT_TX_OVER I2C_INTR_TX_OVER
| TX_OVER interrupt flag. More...
#define | LL_I2C_INTR_STAT_RX_FULL I2C_INTR_RX_FULL
| RX_FULL interrupt flag. More...
#define | LL_I2C_INTR_STAT_RX_OVER I2C_INTR_RX_OVER
| RX_OVER interrupt flag. More...
#define | LL_I2C_INTR_STAT_RX_UNDER I2C_INTR_RX_UNDER
| RX_UNDER interrupt flag. More...
#define | LL_I2C_ABRT_TX_FLUSH_CNT I2C_TX_ABRT_SRC_TX_FLUSH_CNT
| Transfer abort detected by master. More...
#define | LL_I2C_ABRT_USER_ABRT I2C_TX_ABRT_SRC_USER_ABRT
| Transfer abort detected by master. More...
#define | LL_I2C_ABRT_SLVRD_INTX I2C_TX_ABRT_SRC_SLVRD_INTX
| Slave trying to transmit to remote master in read mode. More...
#define | LL_I2C_ABRT_SLV_ARBLOST I2C_TX_ABRT_SRC_SLV_ARBLOST
| Slave lost arbitration to remote master. More...
#define | LL_I2C_ABRT_SLVFLUSH_TXFIFO I2C_TX_ABRT_SRC_SLVFLUSH_TXFIFO
| Slave flushes existing data in TX-FIFO upon getting read command. More...
#define | LL_I2C_ABRT_ARB_LOST I2C_TX_ABRT_SRC_ARB_LOST
| Master or Slave Transmitter lost arbitration. More...
#define | LL_I2C_ABRT_MST_DIS I2C_TX_ABRT_SRC_MST_DIS
| User intitating master operation when MASTER disabled. More...
#define | LL_I2C_ABRT_10B_RD_NORSTRT I2C_TX_ABRT_SRC_10B_RD_NORSTRT
| Master trying to read in 10-Bit addressing mode when RESTART disabled. More...
#define | LL_I2C_ABRT_SBYTE_NORSTRT I2C_TX_ABRT_SRC_SBYTE_NORSTRT
| User trying to send START byte when RESTART disabled. More...
#define | LL_I2C_ABRT_HS_NORSTRT I2C_TX_ABRT_SRC_HS_NORSTRT
| User trying to swidth Master to HS mode when RESTART disabled. More...
#define | LL_I2C_ABRT_SBYTE_ACKDET I2C_TX_ABRT_SRC_SBYTE_ACKDET
| ACK detected for START byte. More...
#define | LL_I2C_ABRT_HS_ACKDET I2C_TX_ABRT_SRC_HS_ACKDET
| HS Master code is ACKed in HS Mode. More...
#define | LL_I2C_ABRT_GCALL_READ I2C_TX_ABRT_SRC_GCALL_READ
| GCALL is followed by read from bus. More...
#define | LL_I2C_ABRT_GCALL_NOACK I2C_TX_ABRT_SRC_GCALL_NOACK
| GCALL is not ACKed by any slave. More...
#define | LL_I2C_ABRT_TXDATA_NOACK I2C_TX_ABRT_SRC_TXDATA_NOACK
| Transmitted data is not ACKed by addressed slave. More...
#define | LL_I2C_ABRT_10ADDR2_NOACK I2C_TX_ABRT_SRC_10ADDR2_NOACK
| Byte 2 of 10-Bit Address is not ACKed by any slave. More...
#define | LL_I2C_ABRT_10ADDR1_NOACK I2C_TX_ABRT_SRC_10ADDR1_NOACK
| Byte 1 of 10-Bit Address is not ACKed by any slave. More...
#define | LL_I2C_ABRT_7B_ADDR_NOACK I2C_TX_ABRT_SRC_7B_ADDR_NOACK
| 7Bit Address is not ACKed by any slave More...

## Detailed Description

Flags definitions which can be used with LL_I2C_ReadReg function.

## Macro Definition Documentation

## ◆ LL_I2C_ABRT_10ADDR1_NOACK

#define LL_I2C_ABRT_10ADDR1_NOACK I2C_TX_ABRT_SRC_10ADDR1_NOACK

Byte 1 of 10-Bit Address is not ACKed by any slave.

Definition at line 140 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_ABRT_10ADDR2_NOACK

#define LL_I2C_ABRT_10ADDR2_NOACK I2C_TX_ABRT_SRC_10ADDR2_NOACK

Byte 2 of 10-Bit Address is not ACKed by any slave.

Definition at line 139 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_ABRT_10B_RD_NORSTRT

#define LL_I2C_ABRT_10B_RD_NORSTRT I2C_TX_ABRT_SRC_10B_RD_NORSTRT

Master trying to read in 10-Bit addressing mode when RESTART disabled.

Definition at line 131 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_ABRT_7B_ADDR_NOACK

#define LL_I2C_ABRT_7B_ADDR_NOACK I2C_TX_ABRT_SRC_7B_ADDR_NOACK

7Bit Address is not ACKed by any slave

Definition at line 141 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_ABRT_ARB_LOST

#define LL_I2C_ABRT_ARB_LOST I2C_TX_ABRT_SRC_ARB_LOST

Master or Slave Transmitter lost arbitration.

Definition at line 129 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_ABRT_GCALL_NOACK

#define LL_I2C_ABRT_GCALL_NOACK I2C_TX_ABRT_SRC_GCALL_NOACK

GCALL is not ACKed by any slave.

Definition at line 137 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_ABRT_GCALL_READ

#define LL_I2C_ABRT_GCALL_READ I2C_TX_ABRT_SRC_GCALL_READ

GCALL is followed by read from bus.

Definition at line 136 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_ABRT_HS_ACKDET

#define LL_I2C_ABRT_HS_ACKDET I2C_TX_ABRT_SRC_HS_ACKDET

HS Master code is ACKed in HS Mode.

Definition at line 135 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_ABRT_HS_NORSTRT

#define LL_I2C_ABRT_HS_NORSTRT I2C_TX_ABRT_SRC_HS_NORSTRT

User trying to swidth Master to HS mode when RESTART disabled.

Definition at line 133 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_ABRT_MST_DIS

#define LL_I2C_ABRT_MST_DIS I2C_TX_ABRT_SRC_MST_DIS

User intitating master operation when MASTER disabled.

Definition at line 130 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_ABRT_SBYTE_ACKDET

#define LL_I2C_ABRT_SBYTE_ACKDET I2C_TX_ABRT_SRC_SBYTE_ACKDET

ACK detected for START byte.

Definition at line 134 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_ABRT_SBYTE_NORSTRT

#define LL_I2C_ABRT_SBYTE_NORSTRT I2C_TX_ABRT_SRC_SBYTE_NORSTRT

User trying to send START byte when RESTART disabled.

Definition at line 132 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_ABRT_SLV_ARBLOST

#define LL_I2C_ABRT_SLV_ARBLOST I2C_TX_ABRT_SRC_SLV_ARBLOST

Slave lost arbitration to remote master.

Definition at line 127 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_ABRT_SLVFLUSH_TXFIFO

#define LL_I2C_ABRT_SLVFLUSH_TXFIFO I2C_TX_ABRT_SRC_SLVFLUSH_TXFIFO

Slave flushes existing data in TX-FIFO upon getting read command.

Definition at line 128 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_ABRT_SLVRD_INTX

#define LL_I2C_ABRT_SLVRD_INTX I2C_TX_ABRT_SRC_SLVRD_INTX

Slave trying to transmit to remote master in read mode.

Definition at line 126 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_ABRT_TX_FLUSH_CNT

#define LL_I2C_ABRT_TX_FLUSH_CNT I2C_TX_ABRT_SRC_TX_FLUSH_CNT

Transfer abort detected by master.

Definition at line 124 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_ABRT_TXDATA_NOACK

#define LL_I2C_ABRT_TXDATA_NOACK I2C_TX_ABRT_SRC_TXDATA_NOACK

Transmitted data is not ACKed by addressed slave.

Definition at line 138 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_ABRT_USER_ABRT

#define LL_I2C_ABRT_USER_ABRT I2C_TX_ABRT_SRC_USER_ABRT

Transfer abort detected by master.

Definition at line 125 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_INTR_STAT_ACTIVITY

#define LL_I2C_INTR_STAT_ACTIVITY I2C_INTR_ACTIVITY

ACTIVITY interrupt flag.

Definition at line 114 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_INTR_STAT_GEN_CALL

#define LL_I2C_INTR_STAT_GEN_CALL I2C_INTR_GEN_CALL

GEN_CALL interrupt flag.

Definition at line 111 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_INTR_STAT_MST_ON_HOLD

#define LL_I2C_INTR_STAT_MST_ON_HOLD I2C_INTR_GEN_CALL

MST_ON_HOLD interrupt flag.

Definition at line 109 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_INTR_STAT_RD_REQ

#define LL_I2C_INTR_STAT_RD_REQ I2C_INTR_RD_REQ

RD_REQ interrupt flag.

Definition at line 117 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_INTR_STAT_RESTART_DET

#define LL_I2C_INTR_STAT_RESTART_DET I2C_INTR_RESTART_DET

RESTART_DET interrupt flag.

Definition at line 110 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_INTR_STAT_RX_DONE

#define LL_I2C_INTR_STAT_RX_DONE I2C_INTR_RX_DONE

RX_DONE interrupt flag.

Definition at line 115 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_INTR_STAT_RX_FULL

#define LL_I2C_INTR_STAT_RX_FULL I2C_INTR_RX_FULL

RX_FULL interrupt flag.

Definition at line 120 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_INTR_STAT_RX_OVER

#define LL_I2C_INTR_STAT_RX_OVER I2C_INTR_RX_OVER

RX_OVER interrupt flag.

Definition at line 121 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_INTR_STAT_RX_UNDER

#define LL_I2C_INTR_STAT_RX_UNDER I2C_INTR_RX_UNDER

RX_UNDER interrupt flag.

Definition at line 122 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_INTR_STAT_START_DET

#define LL_I2C_INTR_STAT_START_DET I2C_INTR_START_DET

START_DET interrupt flag.

Definition at line 112 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_INTR_STAT_STOP_DET

#define LL_I2C_INTR_STAT_STOP_DET I2C_INTR_STOP_DET

STOP_DET interrupt flag.

Definition at line 113 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_INTR_STAT_TX_ABRT

#define LL_I2C_INTR_STAT_TX_ABRT I2C_INTR_TX_ABRT

TX_ABRT interrupt flag.

Definition at line 116 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_INTR_STAT_TX_EMPTY

#define LL_I2C_INTR_STAT_TX_EMPTY I2C_INTR_TX_EMPTY

TX_EMPTY interrupt flag.

Definition at line 118 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_INTR_STAT_TX_OVER

#define LL_I2C_INTR_STAT_TX_OVER I2C_INTR_TX_OVER

TX_OVER interrupt flag.

Definition at line 119 of file gr55xx_ll_i2c.h.