Macros
Automatic Turn off clocks
Peripheral Driver » HAL Driver » CGC » Defines » CGC Exported Constants
Collaboration diagram for Automatic Turn off clocks:

## Macros
#define | CGC_WFI_SECU_HCLK ((uint32_t)0x00000001U)
| Hclk for all security blocks. More...
#define | CGC_WFI_SIM_HCLK ((uint32_t)0x00000002U)
| Hclk for sim card interface More...
#define | CGC_WFI_HTB_HCLK ((uint32_t)0x00000004U)
| Hclk for hopping table More...
#define | CGC_WFI_PWM_HCLK ((uint32_t)0x00000008U)
| Hclk for PWM More...
#define | CGC_WFI_ROM_HCLK ((uint32_t)0x00000010U)
| Hclk for ROM More...
#define | CGC_WFI_SNSADC_HCLK ((uint32_t)0x00000020U)
| Hclk for sense ADC More...
#define | CGC_WFI_GPIO_HCLK ((uint32_t)0x00000040U)
| Hclk for GPIOs More...
#define | CGC_WFI_DMA_HCLK ((uint32_t)0x00000080U)
| Hclk for DMA engine More...
#define | CGC_WFI_BLE_BRG_HCLK ((uint32_t)0x00000100U)
| Hclk for BLE MCU bridge More...
#define | CGC_WFI_APB_SUB_HCLK ((uint32_t)0x00000200U)
| Hclk for APB subsystem More...
#define | CGC_WFI_SERIAL_HCLK ((uint32_t)0x00000400U)
| Hclk for serial blocks More...
#define | CGC_WFI_I2S_S_HCLK ((uint32_t)0x00000800U)
| Hclk for I2S slave More...
#define | CGC_WFI_AON_MCUSUB_HCLK ((uint32_t)0x00001000U)
| Hclk for Always-on register More...
#define | CGC_WFI_XF_XQSPI_HCLK ((uint32_t)0x00002000U)
| Hclk for cache top More...
#define | CGC_WFI_SRAM_HCLK ((uint32_t)0x00004000U)
| Hclk for SRAMs More...
#define | CGC_WFI_SECU_DIV4_PCLK ((uint32_t)0x00008000U)
| Div4 clk for security blocks. More...
#define | CGC_WFI_XQSPI_DIV4_PCLK ((uint32_t)0x00020000U)
| Div4 clk for xf qspi More...
#define | CGC_WFI_ALL_CLK ((uint32_t)0x0002FFFFU)
| All clocks More...

## Detailed Description

## Macro Definition Documentation

## ◆ CGC_WFI_ALL_CLK

#define CGC_WFI_ALL_CLK ((uint32_t)0x0002FFFFU)

All clocks

Definition at line 129 of file gr55xx_hal_cgc.h.

## ◆ CGC_WFI_AON_MCUSUB_HCLK

#define CGC_WFI_AON_MCUSUB_HCLK ((uint32_t)0x00001000U)

Hclk for Always-on register

Definition at line 123 of file gr55xx_hal_cgc.h.

## ◆ CGC_WFI_APB_SUB_HCLK

#define CGC_WFI_APB_SUB_HCLK ((uint32_t)0x00000200U)

Hclk for APB subsystem

Definition at line 120 of file gr55xx_hal_cgc.h.

## ◆ CGC_WFI_BLE_BRG_HCLK

#define CGC_WFI_BLE_BRG_HCLK ((uint32_t)0x00000100U)

Hclk for BLE MCU bridge

Definition at line 119 of file gr55xx_hal_cgc.h.

## ◆ CGC_WFI_DMA_HCLK

#define CGC_WFI_DMA_HCLK ((uint32_t)0x00000080U)

Hclk for DMA engine

Definition at line 118 of file gr55xx_hal_cgc.h.

## ◆ CGC_WFI_GPIO_HCLK

#define CGC_WFI_GPIO_HCLK ((uint32_t)0x00000040U)

Hclk for GPIOs

Definition at line 117 of file gr55xx_hal_cgc.h.

## ◆ CGC_WFI_HTB_HCLK

#define CGC_WFI_HTB_HCLK ((uint32_t)0x00000004U)

Hclk for hopping table

Definition at line 113 of file gr55xx_hal_cgc.h.

## ◆ CGC_WFI_I2S_S_HCLK

#define CGC_WFI_I2S_S_HCLK ((uint32_t)0x00000800U)

Hclk for I2S slave

Definition at line 122 of file gr55xx_hal_cgc.h.

## ◆ CGC_WFI_PWM_HCLK

#define CGC_WFI_PWM_HCLK ((uint32_t)0x00000008U)

Hclk for PWM

Definition at line 114 of file gr55xx_hal_cgc.h.

## ◆ CGC_WFI_ROM_HCLK

#define CGC_WFI_ROM_HCLK ((uint32_t)0x00000010U)

Hclk for ROM

Definition at line 115 of file gr55xx_hal_cgc.h.

## ◆ CGC_WFI_SECU_DIV4_PCLK

#define CGC_WFI_SECU_DIV4_PCLK ((uint32_t)0x00008000U)

Div4 clk for security blocks.

Definition at line 126 of file gr55xx_hal_cgc.h.

## ◆ CGC_WFI_SECU_HCLK

#define CGC_WFI_SECU_HCLK ((uint32_t)0x00000001U)

Hclk for all security blocks.

Definition at line 111 of file gr55xx_hal_cgc.h.

## ◆ CGC_WFI_SERIAL_HCLK

#define CGC_WFI_SERIAL_HCLK ((uint32_t)0x00000400U)

Hclk for serial blocks

Definition at line 121 of file gr55xx_hal_cgc.h.

## ◆ CGC_WFI_SIM_HCLK

#define CGC_WFI_SIM_HCLK ((uint32_t)0x00000002U)

Hclk for sim card interface

Definition at line 112 of file gr55xx_hal_cgc.h.

## ◆ CGC_WFI_SNSADC_HCLK

#define CGC_WFI_SNSADC_HCLK ((uint32_t)0x00000020U)

Hclk for sense ADC

Definition at line 116 of file gr55xx_hal_cgc.h.

## ◆ CGC_WFI_SRAM_HCLK

#define CGC_WFI_SRAM_HCLK ((uint32_t)0x00004000U)

Hclk for SRAMs

Definition at line 125 of file gr55xx_hal_cgc.h.

## ◆ CGC_WFI_XF_XQSPI_HCLK

#define CGC_WFI_XF_XQSPI_HCLK ((uint32_t)0x00002000U)

Hclk for cache top

Definition at line 124 of file gr55xx_hal_cgc.h.

## ◆ CGC_WFI_XQSPI_DIV4_PCLK

#define CGC_WFI_XQSPI_DIV4_PCLK ((uint32_t)0x00020000U)

Div4 clk for xf qspi

Definition at line 127 of file gr55xx_hal_cgc.h.