Macros
UART Number of Stop Bits
Peripheral Driver » HAL Driver » UART » Defines » UART Exported Constants
Collaboration diagram for UART Number of Stop Bits:

## Macros
#define | UART_STOPBITS_1 LL_UART_STOPBITS_1
| UART frame with 1 stop bit More...
#define | UART_STOPBITS_1_5 LL_UART_STOPBITS_1_5
| UART frame with 1.5 stop bits. More...
#define | UART_STOPBITS_2 LL_UART_STOPBITS_2
| UART frame with 2 stop bits More...

## Detailed Description

## Macro Definition Documentation

## ◆ UART_STOPBITS_1

#define UART_STOPBITS_1 LL_UART_STOPBITS_1

UART frame with 1 stop bit

Definition at line 256 of file gr55xx_hal_uart.h.

## ◆ UART_STOPBITS_1_5

#define UART_STOPBITS_1_5 LL_UART_STOPBITS_1_5

UART frame with 1.5 stop bits.

Definition at line 257 of file gr55xx_hal_uart.h.

## ◆ UART_STOPBITS_2

#define UART_STOPBITS_2 LL_UART_STOPBITS_2

UART frame with 2 stop bits

Definition at line 258 of file gr55xx_hal_uart.h.