cts_c.h
Go to the documentation of this file.
1 /**
2 *****************************************************************************************
3 *
4 * @file cts_c.h
5 *
6 * @brief Current Time Service Client API
7 *
8 *****************************************************************************************
9 * @attention
10 #####Copyright (c) 2019 GOODIX
11 All rights reserved.
12
13 Redistribution and use in source and binary forms, with or without
14 modification, are permitted provided that the following conditions are met:
15 * Redistributions of source code must retain the above copyright
16 notice, this list of conditions and the following disclaimer.
17 * Redistributions in binary form must reproduce the above copyright
18 notice, this list of conditions and the following disclaimer in the
19 documentation and/or other materials provided with the distribution.
20 * Neither the name of GOODIX nor the names of its contributors may be used
21 to endorse or promote products derived from this software without
22 specific prior written permission.
23
24 THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS"
25 AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE
26 IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE
27 ARE DISCLAIMED. IN NO EVENT SHALL COPYRIGHT HOLDERS AND CONTRIBUTORS BE
28 LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR
29 CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF
30 SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS
31 INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN
32 CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE)
33 ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE
34 POSSIBILITY OF SUCH DAMAGE.
35 *****************************************************************************************
36 */
37
38 /**
39 * @addtogroup BLE_SRV BLE Services
40 * @{
41 */
42
43 /**
44 * @defgroup BLE_SDK_CTS_C Current Time Service Client (CTS_C)
45 * @{
46 * @brief Current Time Service Client module.
47 *
48 * @details The Current Time Service Client contains the APIs and types, which can be used
49 * by the application to discover Current Time Service of peer and interact with it.
50 *
51 * The application must provide an event handler to be register, then call \ref cts_client_init().
52 * After Current Time Service Client discovers peer Current Time Service, application can
53 * receive current time value notification from peer, and also call \ref cts_c_cur_time_read()
54 * to get current time from peer. This module provides functions: \ref cts_c_loc_time_info_read()
55 * and \ref cts_c_ref_time_info_read() to read local time information and reference time informarion
56 * on peer.
57 */
58
59 #ifndef __CTS_C_H__
60 #define __CTS_C_H__
61
62 #include "gr_includes.h"
63 #include "custom_config.h"
64 #include "ble_prf_utils.h"
65 #include <stdint.h>
66 #include <stdbool.h>
67
68 /**
69 * @defgroup CTS_C_MACRO Defines
70 * @{
71 */
72 #define CTS_C_CONNECTION_MAX 10 /**< Maximum number of HRS Client connections. */
73 #define CTS_C_CUR_TIME_VAL_LEN 10 /**< Length of current time value. */
74 #define CTS_C_LOC_TIME_INFO_VAL_LEN 2 /**< Length of local time information value. */
75 #define CTS_C_TIME_Y_M_D_UNKNOWN 0 /**< Year or Month or Day is not known. */
76 #define CTS_C_TIME_YEAR_VALID_VAL_MIN 1582 /**< Minimum value of valid year. */
77 #define CTS_C_TIME_YEAR_VALID_VAL_MAX 9999 /**< Maximum value of valid year. */
78 #define CTS_C_TIME_ZONE_OFFSET_MIN -48 /**< Minimum Value of Offset from UTC. */
79 #define CTS_C_TIME_ZONE_OFFSET_MAX 56 /**< Maximum Value of Offset from UTC. */
80 #define CTS_C_TIME_ACCURACY_OUT_RANGE 254 /**< Accuracy out of range. */
81 #define CTS_C_TIME_ACCURACT_UNKNOWN 255 /**< Accuracy Unknown. */
82 #define CTS_C_ERROR_FIELDS_IGNORED 0x80 /**< The server ignored one or more fields. */
83
84 /**
85 * @defgroup CTS_C_ADJ_REASON Current Time Adjust Reason
86 * @{
87 * @brief Current Time Service Adjust Reason.
88 */
89 #define CTS_C_AR_NO_CHANGE (0x00 << 0) /**< No change for current time. */
90 #define CTS_C_AR_MAUAL_TIME_UPDATE (0x01 << 0) /**< Manual time update. */
91 #define CTS_C_AR_EXT_REF_TIME_UPDATE (0x01 << 1) /**< External reference time update. */
92 #define CTS_C_AR_TIME_ZONE_CHANGE (0x01 << 2) /**< Change of time zone. */
93 #define CTS_C_AR_DST_CHANGE (0x01 << 3) /**< Change of DST (daylight savings time). */
94 /** @} */
95 /** @} */
96
97 /**
98 * @defgroup CTS_C_ENUM Enumerations
99 * @{
100 */
101 /**@brief Current Time Day of week. */
102 typedef enum
103 {
104 CTS_C_WEEK_UNKNOWN_DAY, /**< Day of week is not known. */
105 CTS_C_WEEK_MONDAY, /**< Monday. */
106 CTS_C_WEEK_TUSEDAY, /**< Tuesday. */
107 CTS_C_WEEK_WEDNESDAY, /**< Wednesday. */
108 CTS_C_WEEK_THURSDAT, /**< Thursday. */
109 CTS_C_WEEK_FRIDAY, /**< Friday. */
110 CTS_C_WEEK_SATURDAY, /**< Saturday. */
111 CTS_C_WEEK_SUNDAY /**< Sunday. */
112 } cts_c_week_day_t;
113
114 /**@brief Local time information:Daylight Saving Time Offset. */
115 typedef enum
116 {
117 CTS_C_DST_OFFSET_STANDAR_TIME = 0x00, /**< Standard Time. */
118 CTS_C_DST_OFFSET_HALF_HOUR = 0x02, /**< Half An Hour Daylight Time (+0.5h). */
119 CTS_C_DST_OFFSET_DAYLIGHT_TIME = 0x04, /**< Daylight Time (+1h). */
120 CTS_C_DST_OFFSET_DOUB_DAYLIGHT_TIME = 0x08, /**< Double Daylight Time (+2h). */
121 } cts_c_dst_offset_t;
122
123 /**@brief Reference time information:Time Source. */
124 typedef enum
125 {
126 CTS_C_REF_TIME_SRC_UNKNOWN, /**< Unknown. */
127 CTS_C_REF_TIME_SRC_NET_TIME_PROTOCOL, /**< Network Time Protocol. */
128 CTS_C_REF_TIME_SRC_GPS, /**< GPS. */
129 CTS_C_REF_TIME_SRC_RADIO_TIME_SIGNAL, /**< Radio Time Signal. */
130 CTS_C_REF_TIME_SRC_MANUAL, /**< Manual. */
131 CTS_C_REF_TIME_SRC_ATOMIC_CLOCK, /**< Atomic Clock. */
132 CTS_C_REF_TIME_SRC_CELLUAR_NET, /**< Cellular Network. */
133 } cts_c_ref_time_source_t;
134
135 /**@brief Current Time Service Client event type. */
136 typedef enum
137 {
138 CTS_C_EVT_INVALID, /**< CTS Client invalid event. */
139 CTS_C_EVT_DISCOVERY_COMPLETE, /**< CTS Client has found CTS service and its characteristics. */
140 CTS_C_EVT_DISCOVERY_FAIL, /**< CTS Client found CTS service failed because of invalid operation or no found at the peer. */
141 CTS_C_EVT_CUR_TIME_NTF_SET_SUCCESS, /**< CTS Client has set Notification of Current Time characteristic. */
142 CTS_C_EVT_VALID_CUR_TIME_REC, /**< CTS Client has received valid Current Time value (Read or Notification from peer). */
143 CTS_C_EVT_INVALID_CUR_TIME_REC, /**< CTS Client has received invalid Current Time value (Read or Notification from peer). */
144 CTS_C_EVT_VALID_LOC_TIME_INFO_REC, /**< CTS Client has received valid Local Time Information value (Read from peer). */
145 CTS_C_EVT_INVALID_LOC_TIME_INFO_REC, /**< CTS Client has received invalid Local Time Information value (Read from peer). */
146 CTS_C_EVT_VALID_REF_TIME_INFO_REC, /**< CTS Client has received valid Reference Time Information Value (Read from peer). */
147 CTS_C_EVT_INVALID_REF_TIME_INFO_REC, /**< CTS Client has received invalid Reference Time Information Value (Read from peer). */
148 CTS_C_EVT_CUR_TIME_SET_SUCCESS, /**< CTS Client has writen Current Time completely. */
149 CTS_C_EVT_LOC_TIME_INFO_SET_SUCCESS, /**< CTS Client has writen Local Time Information completely. */
150 CTS_C_EVT_WRITE_OP_ERR, /**< Error occured when CTS Client writen to peer. */
151 } cts_c_evt_type_t;
152 /** @} */
153
154 /**
155 * @defgroup CTS_C_STRUCT Structures
156 * @{
157 */
158 /**@brief Handles on the connected peer device needed to interact with it. */
159 typedef struct
160 {
161 uint16_t cts_srvc_start_handle; /**< CTS Service start handle. */
162 uint16_t cts_srvc_end_handle; /**< CTS Service end handle. */
163 uint16_t cts_cur_time_handle; /**< CTS Current Time characteristic Value handle which has been got from peer. */
164 uint16_t cts_cur_time_cccd_handle; /**< CTS CCCD handle of Current Time characteristic which has been got from peer. */
165 uint16_t cts_loc_time_info_handle; /**< CTS Local Time Information characteristic Value handle which has been got from peer. */
166 uint16_t cts_ref_time_info_handle; /**< CTS Reference Time Information characteristic Value handle which has been got from peer. */
167 } cts_c_handles_t;
168
169 /**@brief Exact Time 256. */
170 typedef struct
171 {
172 prf_date_time_t date_time; /**< Date Time. */
173 uint8_t day_of_week; /**< Day of Week. */
174 uint8_t fractions_256; /**< 1/256th of a second. */
175 } cts_c_exact_time_256_t;
176
177 /**@brief Current Time value. */
178 typedef struct
179 {
180 cts_c_exact_time_256_t day_date_time; /**< Exact Time 256. */
181 uint8_t adjust_reason; /**< Adjust Reason. */
182 } cts_c_cur_time_t;
183
184 /**@brief Local Time Information. */
185 typedef struct
186 {
187 int8_t time_zone; /**< Time Zone, Offset from UTC in number of 15 minutes increments. */
188 cts_c_dst_offset_t dst_offset; /**< Daylight Saving Time Offset. */
189 } cts_c_loc_time_info_t;
190
191 /**@brief Reference Time Information. */
192 typedef struct
193 {
194 cts_c_ref_time_source_t source; /**< Time Source. */
195 uint8_t accuracy; /**< Accuracy of time information. */
196 uint8_t days_since_update; /**< Days Since Update. */
197 uint8_t hours_since_update; /**< Hours Since Update. */
198 } cts_c_ref_time_info_t;
199
200 /**@brief Current Time Service Client event. */
201 typedef struct
202 {
203 uint8_t conn_idx; /**< The index of the connection. */
204 cts_c_evt_type_t evt_type; /**< The CTS client event type. */
205 union
206 {
207 cts_c_cur_time_t cur_time; /**< Curren time received. */
208 cts_c_loc_time_info_t loc_time_info; /**< Local time information received. */
209 cts_c_ref_time_info_t ref_time_info; /**< Referen time information received. */
210 } value; /**< Decoded result of value received. */
211 } cts_c_evt_t;
212 /** @} */
213
214 /**
215 * @defgroup CTS_C_TYPEDEF Typedefs
216 * @{
217 */
218 /**@brief Current Time Service Client event handler type. */
219 typedef void (*cts_c_evt_handler_t)(cts_c_evt_t *p_evt);
220 /** @} */
221
222 /**
223 * @defgroup CTS_C_FUNCTION Functions
224 * @{
225 */
226 /**
227 *****************************************************************************************
228 * @brief Register CTS Client event handler.
229 *
230 * @param[in] evt_handler: Current Time Service Client event handler.
231 *
232 * @return Result of initialization.
233 *****************************************************************************************
234 */
235 sdk_err_t cts_client_init(cts_c_evt_handler_t evt_handler);
236
237 /**
238 *****************************************************************************************
239 * @brief Discovery Current Time Service on peer.
240 *
241 * @param[in] conn_idx: Index of connection.
242 *
243 * @return Operation result.
244 *****************************************************************************************
245 */
246 sdk_err_t cts_c_disc_srvc_start(uint8_t conn_idx);
247
248 /**
249 *****************************************************************************************
250 * @brief Enable or disable peer Current Time characteristic notify.
251 *
252 * @param[in] conn_idx: Index of connection.
253 * @param[in] is_enable: True or false.
254 *
255 * @return Operation result.
256 *****************************************************************************************
257 */
258 sdk_err_t cts_c_cur_time_notify_set(uint8_t conn_idx, bool is_enable);
259
260 /**
261 *****************************************************************************************
262 * @brief Read Current Time characteristic value.
263 *
264 * @param[in] conn_idx: Index of connection.
265 *
266 * @return Operation result.
267 *****************************************************************************************
268 */
269 sdk_err_t cts_c_cur_time_read(uint8_t conn_idx);
270
271 /**
272 *****************************************************************************************
273 * @brief Read Local Time Information characteristic value.
274 *
275 * @param[in] conn_idx: Index of connection.
276 *
277 * @return Operation result.
278 *****************************************************************************************
279 */
280 sdk_err_t cts_c_loc_time_info_read(uint8_t conn_idx);
281
282 /**
283 *****************************************************************************************
284 * @brief Read Reference Time Information characteristic value.
285 *
286 * @param[in] conn_idx: Index of connection.
287 *
288 * @return Operation result.
289 *****************************************************************************************
290 */
291 sdk_err_t cts_c_ref_time_info_read(uint8_t conn_idx);
292
293 /**
294 *****************************************************************************************
295 * @brief Set Current Time characteristic value.
296 *
297 * @param[in] conn_idx: Index of connection.
298 * @param[in] p_cur_time: Pointer to current time value set.
299 *
300 * @return Operation result.
301 *****************************************************************************************
302 */
303 sdk_err_t cts_c_cur_time_set(uint8_t conn_idx, cts_c_cur_time_t *p_cur_time);
304
305 /**
306 *****************************************************************************************
307 * @brief Set Local Time Information characteristic value.
308 *
309 * @param[in] conn_idx: Index of connection.
310 * @param[in] p_loc_time_info: Pointer to local time information value set.
311 *
312 * @return Operation result.
313 *****************************************************************************************
314 */
315 sdk_err_t cts_c_loc_time_info_set(uint8_t conn_idx, cts_c_loc_time_info_t *p_loc_time_info);
316
317 /**
318 *****************************************************************************************
319 * @brief Data accepts data and processing functions.
320 *
321 * @param[in] p_data: Serial port data.
322 * @param[in] length: Data length.
323 *****************************************************************************************
324 */
325 void cts_c_data_parse(uint8_t *p_data, uint16_t length);
326 /** @} */
327
328 #endif
329 /** @} */
330 /** @} */
331
CTS_C_REF_TIME_SRC_NET_TIME_PROTOCOL
@ CTS_C_REF_TIME_SRC_NET_TIME_PROTOCOL
Network Time Protocol.
Definition: cts_c.h:127
cts_c_loc_time_info_t
Local Time Information.
Definition: cts_c.h:186
cts_c_ref_time_info_t::hours_since_update
uint8_t hours_since_update
Hours Since Update.
Definition: cts_c.h:197
CTS_C_WEEK_THURSDAT
@ CTS_C_WEEK_THURSDAT
Thursday.
Definition: cts_c.h:108
cts_c_handles_t::cts_cur_time_handle
uint16_t cts_cur_time_handle
CTS Current Time characteristic Value handle which has been got from peer.
Definition: cts_c.h:163
CTS_C_EVT_INVALID_CUR_TIME_REC
@ CTS_C_EVT_INVALID_CUR_TIME_REC
CTS Client has received invalid Current Time value (Read or Notification from peer).
Definition: cts_c.h:143
CTS_C_EVT_CUR_TIME_SET_SUCCESS
@ CTS_C_EVT_CUR_TIME_SET_SUCCESS
CTS Client has writen Current Time completely.
Definition: cts_c.h:148
cts_c_ref_time_source_t
cts_c_ref_time_source_t
Reference time information:Time Source.
Definition: cts_c.h:125
CTS_C_WEEK_UNKNOWN_DAY
@ CTS_C_WEEK_UNKNOWN_DAY
Day of week is not known.
Definition: cts_c.h:104
CTS_C_REF_TIME_SRC_UNKNOWN
@ CTS_C_REF_TIME_SRC_UNKNOWN
Unknown.
Definition: cts_c.h:126
cts_c_evt_t::cur_time
cts_c_cur_time_t cur_time
Curren time received.
Definition: cts_c.h:207
CTS_C_EVT_VALID_REF_TIME_INFO_REC
@ CTS_C_EVT_VALID_REF_TIME_INFO_REC
CTS Client has received valid Reference Time Information Value (Read from peer).
Definition: cts_c.h:146
cts_c_ref_time_info_t::source
cts_c_ref_time_source_t source
Time Source.
Definition: cts_c.h:194
cts_c_cur_time_t::day_date_time
cts_c_exact_time_256_t day_date_time
Exact Time 256.
Definition: cts_c.h:180
cts_c_loc_time_info_read
sdk_err_t cts_c_loc_time_info_read(uint8_t conn_idx)
Read Local Time Information characteristic value.
cts_c_exact_time_256_t::date_time
prf_date_time_t date_time
Date Time.
Definition: cts_c.h:172
cts_c_ref_time_info_t::accuracy
uint8_t accuracy
Accuracy of time information.
Definition: cts_c.h:195
CTS_C_EVT_INVALID_LOC_TIME_INFO_REC
@ CTS_C_EVT_INVALID_LOC_TIME_INFO_REC
CTS Client has received invalid Local Time Information value (Read from peer).
Definition: cts_c.h:145
cts_c_exact_time_256_t
Exact Time 256.
Definition: cts_c.h:171
CTS_C_WEEK_WEDNESDAY
@ CTS_C_WEEK_WEDNESDAY
Wednesday.
Definition: cts_c.h:107
CTS_C_DST_OFFSET_HALF_HOUR
@ CTS_C_DST_OFFSET_HALF_HOUR
Half An Hour Daylight Time (+0.5h).
Definition: cts_c.h:118
cts_c_loc_time_info_t::time_zone
int8_t time_zone
Time Zone, Offset from UTC in number of 15 minutes increments.
Definition: cts_c.h:187
gr_includes.h
Include Files API.
CTS_C_EVT_INVALID_REF_TIME_INFO_REC
@ CTS_C_EVT_INVALID_REF_TIME_INFO_REC
CTS Client has received invalid Reference Time Information Value (Read from peer).
Definition: cts_c.h:147
CTS_C_EVT_INVALID
@ CTS_C_EVT_INVALID
CTS Client invalid event.
Definition: cts_c.h:138
cts_c_handles_t::cts_cur_time_cccd_handle
uint16_t cts_cur_time_cccd_handle
CTS CCCD handle of Current Time characteristic which has been got from peer.
Definition: cts_c.h:164
cts_c_handles_t::cts_ref_time_info_handle
uint16_t cts_ref_time_info_handle
CTS Reference Time Information characteristic Value handle which has been got from peer.
Definition: cts_c.h:166
CTS_C_EVT_VALID_LOC_TIME_INFO_REC
@ CTS_C_EVT_VALID_LOC_TIME_INFO_REC
CTS Client has received valid Local Time Information value (Read from peer).
Definition: cts_c.h:144
CTS_C_REF_TIME_SRC_RADIO_TIME_SIGNAL
@ CTS_C_REF_TIME_SRC_RADIO_TIME_SIGNAL
Radio Time Signal.
Definition: cts_c.h:129
cts_c_handles_t
Handles on the connected peer device needed to interact with it.
Definition: cts_c.h:160
CTS_C_DST_OFFSET_DOUB_DAYLIGHT_TIME
@ CTS_C_DST_OFFSET_DOUB_DAYLIGHT_TIME
Double Daylight Time (+2h).
Definition: cts_c.h:120
cts_c_handles_t::cts_loc_time_info_handle
uint16_t cts_loc_time_info_handle
CTS Local Time Information characteristic Value handle which has been got from peer.
Definition: cts_c.h:165
cts_c_evt_t
Current Time Service Client event.
Definition: cts_c.h:202
cts_c_data_parse
void cts_c_data_parse(uint8_t *p_data, uint16_t length)
Data accepts data and processing functions.
cts_c_disc_srvc_start
sdk_err_t cts_c_disc_srvc_start(uint8_t conn_idx)
Discovery Current Time Service on peer.
CTS_C_EVT_CUR_TIME_NTF_SET_SUCCESS
@ CTS_C_EVT_CUR_TIME_NTF_SET_SUCCESS
CTS Client has set Notification of Current Time characteristic.
Definition: cts_c.h:141
cts_c_cur_time_t::adjust_reason
uint8_t adjust_reason
Adjust Reason.
Definition: cts_c.h:181
cts_c_dst_offset_t
cts_c_dst_offset_t
Local time information:Daylight Saving Time Offset.
Definition: cts_c.h:116
CTS_C_REF_TIME_SRC_MANUAL
@ CTS_C_REF_TIME_SRC_MANUAL
Manual.
Definition: cts_c.h:130
cts_c_ref_time_info_t
Reference Time Information.
Definition: cts_c.h:193
cts_c_evt_t::loc_time_info
cts_c_loc_time_info_t loc_time_info
Local time information received.
Definition: cts_c.h:208
cts_c_handles_t::cts_srvc_end_handle
uint16_t cts_srvc_end_handle
CTS Service end handle.
Definition: cts_c.h:162
cts_c_evt_t::ref_time_info
cts_c_ref_time_info_t ref_time_info
Referen time information received.
Definition: cts_c.h:209
cts_c_cur_time_set
sdk_err_t cts_c_cur_time_set(uint8_t conn_idx, cts_c_cur_time_t *p_cur_time)
Set Current Time characteristic value.
CTS_C_REF_TIME_SRC_ATOMIC_CLOCK
@ CTS_C_REF_TIME_SRC_ATOMIC_CLOCK
Atomic Clock.
Definition: cts_c.h:131
cts_c_loc_time_info_set
sdk_err_t cts_c_loc_time_info_set(uint8_t conn_idx, cts_c_loc_time_info_t *p_loc_time_info)
Set Local Time Information characteristic value.
sdk_err_t
uint16_t sdk_err_t
SDK API result type.
Definition: ble_error.h:274
CTS_C_WEEK_MONDAY
@ CTS_C_WEEK_MONDAY
Monday.
Definition: cts_c.h:105
prf_date_time_t
The date and time structure.
Definition: ble_prf_types.h:101
cts_client_init
sdk_err_t cts_client_init(cts_c_evt_handler_t evt_handler)
Register CTS Client event handler.
cts_c_ref_time_info_read
sdk_err_t cts_c_ref_time_info_read(uint8_t conn_idx)
Read Reference Time Information characteristic value.
CTS_C_DST_OFFSET_STANDAR_TIME
@ CTS_C_DST_OFFSET_STANDAR_TIME
Standard Time.
Definition: cts_c.h:117
cts_c_exact_time_256_t::fractions_256
uint8_t fractions_256
1/256th of a second.
Definition: cts_c.h:174
cts_c_evt_type_t
cts_c_evt_type_t
Current Time Service Client event type.
Definition: cts_c.h:137
cts_c_handles_t::cts_srvc_start_handle
uint16_t cts_srvc_start_handle
CTS Service start handle.
Definition: cts_c.h:161
cts_c_loc_time_info_t::dst_offset
cts_c_dst_offset_t dst_offset
Daylight Saving Time Offset.
Definition: cts_c.h:188
cts_c_cur_time_read
sdk_err_t cts_c_cur_time_read(uint8_t conn_idx)
Read Current Time characteristic value.
CTS_C_REF_TIME_SRC_GPS
@ CTS_C_REF_TIME_SRC_GPS
GPS.
Definition: cts_c.h:128
CTS_C_WEEK_FRIDAY
@ CTS_C_WEEK_FRIDAY
Friday.
Definition: cts_c.h:109
cts_c_exact_time_256_t::day_of_week
uint8_t day_of_week
Day of Week.
Definition: cts_c.h:173
cts_c_evt_t::evt_type
cts_c_evt_type_t evt_type
The CTS client event type.
Definition: cts_c.h:204
CTS_C_EVT_DISCOVERY_FAIL
@ CTS_C_EVT_DISCOVERY_FAIL
CTS Client found CTS service failed because of invalid operation or no found at the peer.
Definition: cts_c.h:140
CTS_C_EVT_LOC_TIME_INFO_SET_SUCCESS
@ CTS_C_EVT_LOC_TIME_INFO_SET_SUCCESS
CTS Client has writen Local Time Information completely.
Definition: cts_c.h:149
cts_c_cur_time_t
Current Time value.
Definition: cts_c.h:179
cts_c_evt_t::conn_idx
uint8_t conn_idx
The index of the connection.
Definition: cts_c.h:203
CTS_C_WEEK_TUSEDAY
@ CTS_C_WEEK_TUSEDAY
Tuesday.
Definition: cts_c.h:106
cts_c_evt_handler_t
void(* cts_c_evt_handler_t)(cts_c_evt_t *p_evt)
Current Time Service Client event handler type.
Definition: cts_c.h:219
ble_prf_utils.h
Profile/Service Utilities API.
CTS_C_WEEK_SATURDAY
@ CTS_C_WEEK_SATURDAY
Saturday.
Definition: cts_c.h:110
cts_c_week_day_t
cts_c_week_day_t
Current Time Day of week.
Definition: cts_c.h:103
CTS_C_WEEK_SUNDAY
@ CTS_C_WEEK_SUNDAY
Sunday.
Definition: cts_c.h:111
CTS_C_DST_OFFSET_DAYLIGHT_TIME
@ CTS_C_DST_OFFSET_DAYLIGHT_TIME
Daylight Time (+1h).
Definition: cts_c.h:119
CTS_C_EVT_DISCOVERY_COMPLETE
@ CTS_C_EVT_DISCOVERY_COMPLETE
CTS Client has found CTS service and its characteristics.
Definition: cts_c.h:139
CTS_C_EVT_WRITE_OP_ERR
@ CTS_C_EVT_WRITE_OP_ERR
Error occured when CTS Client writen to peer.
Definition: cts_c.h:150
CTS_C_EVT_VALID_CUR_TIME_REC
@ CTS_C_EVT_VALID_CUR_TIME_REC
CTS Client has received valid Current Time value (Read or Notification from peer).
Definition: cts_c.h:142
CTS_C_REF_TIME_SRC_CELLUAR_NET
@ CTS_C_REF_TIME_SRC_CELLUAR_NET
Cellular Network.
Definition: cts_c.h:132
cts_c_cur_time_notify_set
sdk_err_t cts_c_cur_time_notify_set(uint8_t conn_idx, bool is_enable)
Enable or disable peer Current Time characteristic notify.
cts_c_ref_time_info_t::days_since_update
uint8_t days_since_update
Days Since Update.
Definition: cts_c.h:196