### - d -

- data : app_i2c_evt_t , app_i2s_evt_t , app_iso7816_evt_t , app_qspi_evt_t , app_spi_evt_t , app_uart_evt_t , ble_gap_evt_adv_report_t , ble_l2cap_evt_sdu_recv_t , ble_l2cap_lecb_sdu_t , ble_sec_cfm_enc_t , ble_sec_evt_enc_req_t , dfu_receive_frame_t , hids_evt_t , wechat_evt_t
- data_bits : _ll_pkc_init , _ll_uart_init_t , _uart_init , pkc_init_t
- data_len : dfu_receive_frame_t
- data_length : ble_gapc_evt_t
- data_mode : _qspi_command_t , _xqspi_command_t
- data_order : _ll_xqspi_init_t
- data_size : _i2s_init , _ll_qspi_init_t , _ll_spim_init_t , _ll_spis_init_t , _ll_xqspi_init_t , _qspi_command_t , _spi_init
- data_xfer_width : app_spi_screen_config_t
- date : _calendar_time
- date_of_birth : uds_chars_val_t
- date_time : cts_c_exact_time_256_t , cts_exact_time_256_t , ndcs_time_dst_t
- day : birth_date_t , prf_date_time_t
- day_date_time : cts_adj_info_t , cts_c_cur_time_t , cts_cur_time_t
- day_of_week : cts_c_exact_time_256_t , cts_exact_time_256_t
- days_since_update : cts_c_ref_time_info_t , cts_ref_time_info_t
- db_change_incr_val : uds_evt_t , uds_init_t
- db_ret : stack_heaps_table_t
- db_ret_size : stack_heaps_table_t
- dcdc_vout : pmu_trim_info_t
- description : prf_char_pres_fmt_t
- detect_coding : _ll_iso7816_init , iso7816_init_t
- dev_info : ble_gap_evt_dev_info_get_t , ble_gapm_evt_t
- dev_rf_path_comp : ble_gap_dev_info_t
- dev_tx_power : ble_gap_dev_info_t
- dev_version : ble_gap_dev_info_t
- dfu_ble_send_data : dfu_func_t
- dfu_flash_erase : dfu_func_t
- dfu_flash_erase_chip : dfu_func_t
- dfu_flash_get_info : dfu_func_t
- dfu_flash_get_security : dfu_func_t
- dfu_flash_read : dfu_func_t
- dfu_flash_set_security : dfu_func_t
- dfu_flash_write : dfu_func_t
- dfu_mode : otas_evt_t
- dfu_program_end_callback : dfu_pro_callback_t
- dfu_program_start_callback : dfu_pro_callback_t
- dfu_programing_callback : dfu_pro_callback_t
- dfu_spi_flash_erase : dfu_spi_flash_func_t
- dfu_spi_flash_erase_chip : dfu_spi_flash_func_t
- dfu_spi_flash_get_info : dfu_spi_flash_func_t
- dfu_spi_flash_init : dfu_spi_flash_func_t
- dfu_spi_flash_read : dfu_spi_flash_func_t
- dfu_spi_flash_write : dfu_spi_flash_func_t
- dfu_uart_send_data : dfu_func_t
- diastolic : bps_meas_t
- dig_ldo_16m : pmu_trim_info_t
- dig_ldo_64m : pmu_trim_info_t
- direct_addr : ble_gap_evt_adv_report_t
- direction : _dma_init , _ll_dma_init , _ll_msio_init , _msio_init
- dis_char_handle : dis_c_handles_t
- dis_srvc_end_handle : dis_c_handles_t
- dis_srvc_start_handle : dis_c_handles_t
- disc_mode : ble_gap_adv_param_t , ble_gap_ext_adv_param_t
- disconnected : ble_gapc_evt_t , ble_l2cap_evt_t
- dma_cfg : app_adc_params_t , app_i2c_params_t , app_i2s_params_t , app_qspi_params_t , app_spi_params_t , app_uart_params_t
- dma_channel : app_adc_dma_cfg_t , app_qspi_dma_cfg_t
- dma_id : adc_env_t , i2c_env_t , i2s_env_t , qspi_env_t , spi_env_t , uart_env_t
- dma_instance : app_adc_dma_cfg_t , app_qspi_dma_cfg_t
- dma_rx_mode : _uart_handle
- dma_state : dma_env_t
- dma_tx_mode : _uart_handle
- dpa_mode : _aes_init , _hmac_init
- drive_polarity : _ll_pwm_channel_init_t , app_pwm_channel_init_t , pwm_channel_init_t
- dst_address : _ll_dma_init
- dst_data_alignment : _dma_init
- dst_data_width : _ll_dma_init
- dst_increment : _dma_init
- dst_increment_mode : _ll_dma_init
- dst_offset : cts_c_loc_time_info_t , cts_loc_time_info_t , ndcs_time_dst_t
- dst_peripheral : _ll_dma_init
- dst_request : _dma_init
- dual_tim_env : app_dual_tim_params_t
- dual_tim_state : dual_tim_env_t
- dual_timer_msp_deinit : _hal_dual_timer_callback
- dual_timer_msp_init : _hal_dual_timer_callback
- dual_timer_period_elapsed_callback : _hal_dual_timer_callback
- dummy_cycles : _qspi_command_t , _xqspi_command_t
- dup_filt_pol : ble_gap_ext_scan_param_t
- duration : ble_gap_adv_time_param_t , ble_gap_con_plan_tag_t , ble_gap_ext_scan_param_t , ble_gap_set_pref_slave_evt_dur_param_t , thscps_adv_param_t
- duty : _ll_pwm_channel_init_t , app_pwm_channel_init_t , pwm_channel_init_t