Modules
Multi Link Multi Role Service (MLMR)
BLE Services

Definitions and prototypes for the MLMR interface. More...

Collaboration diagram for Multi Link Multi Role Service (MLMR):

## Modules
| Defines
| Enumerations
| Structures
| Typedefs
| Functions

## Detailed Description

Definitions and prototypes for the MLMR interface.

The Multi Link Multi Role Service is a customized GATT-based service with Tx, Rx and Flow Control characteristics. The application uses the service to send and receive data to and from the peer. The application data is sent to the peer as Handle Value Notification, and the data received from the peer is transmitted with GATT Write Command.

After mlmr_init_t variable is initialized , the application must call mlmr_service_init() to add the Goodix Uart Service and Rx, Tx, Flow Control characteristics to the BLE Stack database. The application can send the data to the peer with mlmr_tx_data_send() after MLMR_EVT_TX_PORT_OPENED received. The application should copy the received data to its own buffer when handling MLMR_EVT_RX_DATA_RECEIVED.