Macros
QSPI Clock Phase
Peripheral Driver » LL Driver » XQSPI » Defines » XQSPI Exported Constants
Collaboration diagram for QSPI Clock Phase:

## Macros
#define | LL_XQSPI_SCPHA_1EDGE 0
| First clock transition is the first data capture edge More...
#define | LL_XQSPI_SCPHA_2EDGE 1
| Second clock transition is the first data capture edge. More...

## Detailed Description

## Macro Definition Documentation

## ◆ LL_XQSPI_SCPHA_1EDGE

#define LL_XQSPI_SCPHA_1EDGE 0

First clock transition is the first data capture edge

Definition at line 265 of file gr55xx_ll_xqspi.h.

## ◆ LL_XQSPI_SCPHA_2EDGE

#define LL_XQSPI_SCPHA_2EDGE 1

Second clock transition is the first data capture edge.

Definition at line 266 of file gr55xx_ll_xqspi.h.