Functions
Initialization and de-initialization functions
Peripheral Driver » LL Driver » AON_GPIO » Functions
Collaboration diagram for Initialization and de-initialization functions:

## Functions
error_status_t | ll_aon_gpio_deinit (void)
| De-initialize AON_GPIO registers (Registers restored to their default values). More...
error_status_t | ll_aon_gpio_init (ll_aon_gpio_init_t *p_aon_gpio_init)
| Initialize AON_GPIO registers according to the specified. More...
void | ll_aon_gpio_struct_init (ll_aon_gpio_init_t *p_aon_gpio_init)
| Set each field of a ll_aon_gpio_init_t type structure to default value. More...

## Detailed Description

## Function Documentation

## ◆ ll_aon_gpio_deinit()

error_status_t ll_aon_gpio_deinit | ( | void |  | ) |

De-initialize AON_GPIO registers (Registers restored to their default values).

Return values

  An | error_status_t enumeration value: SUCCESS: AON_GPIO registers are de-initialized ERROR: AON_GPIO registers are not de-initialized

## ◆ ll_aon_gpio_init()

error_status_t ll_aon_gpio_init | ( | ll_aon_gpio_init_t * | p_aon_gpio_init | ) |

Initialize AON_GPIO registers according to the specified.

parameters in p_aon_gpio_init.

Parameters

  p_aon_gpio_init | Pointer to a ll_aon_gpio_init_t structure that contains the configuration information for the specified AON_GPIO peripheral.

Return values

  An | error_status_t enumeration value: SUCCESS: AON_GPIO registers are initialized according to p_aon_gpio_init content ERROR: Problem occurred during AON_GPIO Registers initialization

## ◆ ll_aon_gpio_struct_init()

void ll_aon_gpio_struct_init | ( | ll_aon_gpio_init_t * | p_aon_gpio_init | ) |

Set each field of a ll_aon_gpio_init_t type structure to default value.

Parameters

  p_aon_gpio_init | Pointer to a ll_aon_gpio_init_t structure whose fields will be set to default values.

Return values

  None |