Public Attributes | List of all members
_ll_spis_init_t Struct Reference
Peripheral Driver » LL Driver » SPI » Structures » SPI Exported init structure

SPIS init structures definition. More...

`#include <gr55xx_ll_spi.h>`

## Public Attributes
uint32_t | data_size
| Specifies the SPI data width. More...
uint32_t | clock_polarity
| Specifies the serial clock steady state. More...
uint32_t | clock_phase
| Specifies the clock active edge for the bit capture. More...

## Detailed Description

SPIS init structures definition.

Definition at line 113 of file gr55xx_ll_spi.h.

## Member Data Documentation

## ◆ clock_phase

uint32_t _ll_spis_init_t::clock_phase

Specifies the clock active edge for the bit capture.

This parameter can be a value of Clock Phase.

This feature can be modified afterwards using unitary function ll_spi_set_clock_phase().

Definition at line 125 of file gr55xx_ll_spi.h.

## ◆ clock_polarity

uint32_t _ll_spis_init_t::clock_polarity

Specifies the serial clock steady state.

This parameter can be a value of Clock Polarity.

This feature can be modified afterwards using unitary function ll_spi_set_clock_polarity().

Definition at line 120 of file gr55xx_ll_spi.h.

## ◆ data_size

uint32_t _ll_spis_init_t::data_size

Specifies the SPI data width.

This parameter can be a value of Datawidth.

This feature can be modified afterwards using unitary function ll_spi_set_data_size().

Definition at line 115 of file gr55xx_ll_spi.h.

The documentation for this struct was generated from the following file:

- gr55xx_ll_spi.h