Modules | Macros
Defines
BLE Services » OTA Service Client (OTAS_C)
Collaboration diagram for Defines:

## Modules
| OTAS UUIDs
| OTAS service and characteristcs UUID.

## Macros
#define | OTAS_C_CONNECTION_MAX 10
| Maximum number of OTAS Client connections. More...
#define | OTAS_C_CTRL_PT_OP_DFU_ENTER 0x474f4f44
| Control point opcode for entering DFU mode. More...

## Detailed Description

## Macro Definition Documentation

## ◆ OTAS_C_CONNECTION_MAX

#define OTAS_C_CONNECTION_MAX 10

Maximum number of OTAS Client connections.

Definition at line 68 of file otas_c.h.

## ◆ OTAS_C_CTRL_PT_OP_DFU_ENTER

#define OTAS_C_CTRL_PT_OP_DFU_ENTER 0x474f4f44

Control point opcode for entering DFU mode.

Definition at line 85 of file otas_c.h.