Enumerations
HAL XQSPI state
Peripheral Driver » HAL Driver » XQSPI » Enumerations
Collaboration diagram for HAL XQSPI state:

## Enumerations
enum | hal_xqspi_state_t { HAL_XQSPI_STATE_RESET = 0x00, HAL_XQSPI_STATE_READY = 0x01, HAL_XQSPI_STATE_BUSY = 0x02, HAL_XQSPI_STATE_BUSY_INDIRECT_TX = 0x12, HAL_XQSPI_STATE_BUSY_INDIRECT_RX = 0x22, HAL_XQSPI_STATE_ABORT = 0x08, HAL_XQSPI_STATE_ERROR = 0x04 }
| HAL XQSPI State Enumerations definition. More...

## Detailed Description

## Enumeration Type Documentation

## ◆ hal_xqspi_state_t

enum hal_xqspi_state_t

HAL XQSPI State Enumerations definition.

Enumerator
HAL_XQSPI_STATE_RESET | Peripheral not initialized
HAL_XQSPI_STATE_READY | Peripheral initialized and ready for use
HAL_XQSPI_STATE_BUSY | Peripheral in indirect mode and busy
HAL_XQSPI_STATE_BUSY_INDIRECT_TX | Peripheral in indirect mode with transmission ongoing.
HAL_XQSPI_STATE_BUSY_INDIRECT_RX | Peripheral in indirect mode with reception ongoing
HAL_XQSPI_STATE_ABORT | Peripheral with abort request ongoing
HAL_XQSPI_STATE_ERROR | Peripheral in error

Definition at line 75 of file gr55xx_hal_xqspi.h.